<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="4.064" y1="1.27" x2="5.334" y2="1.27" width="0" layer="20"/>
<wire x1="5.334" y1="1.27" x2="5.334" y2="2.54" width="0" layer="20"/>
<wire x1="5.334" y1="2.54" x2="9.398" y2="2.54" width="0" layer="20"/>
<wire x1="9.398" y1="2.54" x2="9.398" y2="1.016" width="0" layer="20"/>
<wire x1="9.398" y1="1.016" x2="26.162" y2="1.016" width="0" layer="20"/>
<wire x1="26.162" y1="1.016" x2="26.162" y2="2.54" width="0" layer="20"/>
<wire x1="26.162" y1="2.54" x2="30.226" y2="2.54" width="0" layer="20"/>
<wire x1="30.226" y1="2.54" x2="30.226" y2="1.27" width="0" layer="20"/>
<wire x1="30.226" y1="1.27" x2="31.42" y2="1.27" width="0" layer="20"/>
<wire x1="31.42" y1="1.27" x2="31.42" y2="8.88" width="0" layer="20"/>
<wire x1="31.42" y1="8.88" x2="30.226" y2="8.89" width="0" layer="20"/>
<wire x1="30.226" y1="8.89" x2="30.226" y2="7.62" width="0" layer="20"/>
<wire x1="30.226" y1="7.62" x2="26.162" y2="7.62" width="0" layer="20"/>
<wire x1="26.162" y1="7.62" x2="26.162" y2="9.144" width="0" layer="20"/>
<wire x1="26.162" y1="9.144" x2="9.398" y2="9.144" width="0" layer="20"/>
<wire x1="9.398" y1="9.144" x2="9.398" y2="7.62" width="0" layer="20"/>
<wire x1="9.398" y1="7.62" x2="5.334" y2="7.62" width="0" layer="20"/>
<wire x1="5.334" y1="7.62" x2="5.334" y2="8.88" width="0" layer="20"/>
<wire x1="5.334" y1="8.88" x2="4.064" y2="8.88" width="0" layer="20"/>
<wire x1="4.064" y1="8.88" x2="4.064" y2="1.27" width="0" layer="20"/>
<text>M+</text>
<text>S+</text>
<text>S-</text>
<text>M</text>
<text>S</text>
<hole x="7.366" y="5.08" drill="3.2"/>
<hole x="28.194" y="5.08" drill="3.2"/>
<text>John Boiles
KK6GIP</text>
<text>r2</text>
<text>-</text>
<text>TRRS</text>
<text>UV5R</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="10k"/>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="2.2k"/>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="2.2k"/>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value=".01uF"/>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X03_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="C1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="BAOFENGMIC+">
<contactref element="JP3" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
