<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="46" y2="0" width="0" layer="20"/>
<wire x1="46" y1="0" x2="46" y2="23" width="0" layer="20"/>
<wire x1="46" y1="23" x2="0" y2="23" width="0" layer="20"/>
<wire x1="0" y1="23" x2="0" y2="0" width="0" layer="20"/>
<text>TX OFF</text>
<text>TX ON</text>
<text>UART_TX</text>
<text>UART_RX</text>
<text>GND</text>
<text>GND</text>
<text>VDD</text>
<text>SPARE</text>
</plain>
<libraries>
<library name="MyPassives">
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="slide-switches">
<packages>
<package name="DPDT-SMD">
</package>
</packages>
</library>
<library name="JiangsuQinHeng">
<packages>
<package name="SOIC-8">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="MyPassives" package="0603" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
</element>
<element name="C2" library="MyPassives" package="0603" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="USB-MICROB" value="USB-MICROB">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09505"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="slide-switches" package="DPDT-SMD" value="JS202011SCQN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="JiangsuQinHeng" package="SOIC-8" value="CH330N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="SOT23-5" value="V_REG_LDOSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="MyPassives" package="0603" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
</element>
<element name="C4" library="MyPassives" package="0603" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="TX_OFF">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="P$5"/>
</signal>
<signal name="SPARE">
<contactref element="JP1" pad="5"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="8"/>
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="P$6"/>
<contactref element="JP3" pad="GND"/>
<contactref element="JP3" pad="MT1"/>
<contactref element="JP3" pad="MT2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="C1" pad="P$2"/>
<contactref element="U1" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="C3" pad="P$2"/>
<contactref element="C4" pad="P$2"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="V_BUS">
<contactref element="JP3" pad="VBUS"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="P$1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="USB_DM">
<contactref element="JP3" pad="D-"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="USB_DP">
<contactref element="JP3" pad="D+"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="5"/>
<contactref element="C2" pad="P$1"/>
<contactref element="C3" pad="P$1"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="TRANSPONDER_RX">
<contactref element="JP1" pad="3"/>
<contactref element="U$2" pad="6"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="TRANSPONDER_TX">
<contactref element="JP1" pad="6"/>
<contactref element="U$2" pad="7"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="8"/>
<contactref element="C4" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
