<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="72.5" y1="0" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="58" width="0" layer="20"/>
<wire x1="0" y1="58" x2="2" y2="60" width="0" layer="20" curve="-90"/>
<wire x1="2" y1="60" x2="21" y2="60" width="0" layer="20"/>
<wire x1="72.5" y1="58" x2="72.5" y2="0" width="0" layer="20"/>
<wire x1="48.01" y1="60" x2="70.5" y2="60" width="0" layer="20"/>
<wire x1="70.5" y1="60" x2="72.5" y2="58" width="0" layer="20" curve="-90"/>
<wire x1="47.24" y1="59.23" x2="48.01" y2="60" width="0" layer="20" curve="-90"/>
<text>Bee Snuggler
Main Board
v0.0.1</text>
<text>32 - Ambient
33 - Upper
25 - Center
26 - Lower
14 - Output
13 - Heat
17 - Fan PWM
16 - Fan RPM</text>
<wire x1="21" y1="60" x2="22" y2="59" width="0" layer="20" curve="-90"/>
<wire x1="22" y1="59" x2="22.77" y2="58.23" width="0" layer="20" curve="90"/>
<wire x1="22.77" y1="58.23" x2="46.24" y2="58.23" width="0" layer="20"/>
<wire x1="46.24" y1="58.23" x2="47.24" y2="59.23" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="Donnie">
<packages>
<package name="CAP_PTH-2.54">
</package>
<package name="D32_PRO">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Wurth_Connectors_WR-TBL Pluggable Connector">
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Terminal Blocks - WR-TBL Pluggable Connector &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-02-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="691311500103">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 3pins</description>
</package>
<package name="691311500102">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 2pins</description>
</package>
<package name="691311500104">
<description>&lt;b&gt;WR-TBL Serie 311 - 5.08 mm Close Vertical PCB Header 
&lt;br&gt;&lt;/b&gt;Max Height = 12mm , Pitch 5.08mm , 4pins</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://eagle.componentsearchengine.com&lt;/b&gt;&lt;p&gt;&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="CONSOCJ2155">
<description>&lt;b&gt;CON-SOCJ-2155_1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Donnie" package="CAP_PTH-2.54" value="0.1μF">
<attribute name="NAME"/>
</element>
<element name="C2" library="Donnie" package="CAP_PTH-2.54" value="1.0μF">
<attribute name="NAME"/>
</element>
<element name="D32" library="Donnie" package="D32_PRO" value="Lolin D32"/>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="2.2kΩ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="2.2kΩ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="2.2kΩ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="2.2kΩ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="2.2kΩ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="AMBIENT" library="Wurth_Connectors_WR-TBL Pluggable Connector" package="691311500103" value=" 691311500103 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691311500103.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PART-NUMBER" value=" 691311500103 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="300V (AC)"/>
</element>
<element name="UPPER" library="Wurth_Connectors_WR-TBL Pluggable Connector" package="691311500103" value=" 691311500103 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691311500103.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PART-NUMBER" value=" 691311500103 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="300V (AC)"/>
</element>
<element name="CENTER" library="Wurth_Connectors_WR-TBL Pluggable Connector" package="691311500103" value=" 691311500103 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691311500103.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PART-NUMBER" value=" 691311500103 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="300V (AC)"/>
</element>
<element name="LOWER" library="Wurth_Connectors_WR-TBL Pluggable Connector" package="691311500103" value=" 691311500103 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691311500103.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PART-NUMBER" value=" 691311500103 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="300V (AC)"/>
</element>
<element name="OUTPUT" library="Wurth_Connectors_WR-TBL Pluggable Connector" package="691311500103" value=" 691311500103 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691311500103.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PART-NUMBER" value=" 691311500103 "/>
<attribute name="PINS" value=" 3 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="300V (AC)"/>
</element>
<element name="HEAT" library="Wurth_Connectors_WR-TBL Pluggable Connector" package="691311500102" value=" 691311500102 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691311500102.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PART-NUMBER" value=" 691311500102 "/>
<attribute name="PINS" value=" 2 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="300V (AC)"/>
</element>
<element name="FAN" library="Wurth_Connectors_WR-TBL Pluggable Connector" package="691311500104" value=" 691311500104 ">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/691311500104.pdf"/>
<attribute name="IR-UL" value="20A"/>
<attribute name="IR-VDE" value="20A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="NAME"/>
<attribute name="PART-NUMBER" value=" 691311500104 "/>
<attribute name="PINS" value=" 4 "/>
<attribute name="PITCH" value="5.08mm"/>
<attribute name="TYPE" value="Vertical"/>
<attribute name="WORKING-VOLTAGE-UL" value="300V (AC)"/>
<attribute name="WORKING-VOLTAGE-VDE" value="300V (AC)"/>
</element>
<element name="IC1" library="linear" package="TO220V" value="7805TV">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="57"/>
</element>
<element name="C3" library="Donnie" package="CAP_PTH-2.54" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="Donnie" package="CAP_PTH-2.54" value="1uF">
<attribute name="NAME"/>
</element>
<element name="U$1" library="holes" package="3,0" value=""/>
<element name="U$2" library="holes" package="3,0" value=""/>
<element name="U$3" library="holes" package="3,0" value=""/>
<element name="J1" library="SamacSys_Parts" package="CONSOCJ2155" value="CON-SOCJ-2155">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="DC Power Connectors Power Jack/Connector 2.1mm x 5.5mm"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="MANUFACTURER_NAME" value="Gravitech"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CON-SOCJ-2155"/>
<attribute name="MOUSER_PART_NUMBER" value="992-CON-SOCJ-2155"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Gravitech/CON-SOCJ-2155?qs=fkzBJ5HM%252BdCcpvFQyQZHtA%3D%3D"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="3V3">
<contactref element="D32" pad="VCC"/>
<contactref element="R4" pad="P$1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R5" pad="P$1"/>
<contactref element="AMBIENT" pad="3"/>
<contactref element="UPPER" pad="3"/>
<contactref element="CENTER" pad="3"/>
<contactref element="LOWER" pad="3"/>
<contactref element="OUTPUT" pad="3"/>
</signal>
<signal name="GND">
<contactref element="D32" pad="GND"/>
<contactref element="D32" pad="GND2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="AMBIENT" pad="1"/>
<contactref element="UPPER" pad="1"/>
<contactref element="CENTER" pad="1"/>
<contactref element="LOWER" pad="1"/>
<contactref element="OUTPUT" pad="1"/>
<contactref element="HEAT" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="FAN" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="UDAT">
<contactref element="R2" pad="P$2"/>
<contactref element="D32" pad="IO33"/>
<contactref element="UPPER" pad="2"/>
</signal>
<signal name="ADAT">
<contactref element="R1" pad="P$2"/>
<contactref element="D32" pad="IO32"/>
<contactref element="AMBIENT" pad="2"/>
</signal>
<signal name="CDAT">
<contactref element="R3" pad="P$2"/>
<contactref element="D32" pad="IO25"/>
<contactref element="CENTER" pad="2"/>
</signal>
<signal name="LDAT">
<contactref element="R4" pad="P$2"/>
<contactref element="D32" pad="IO26"/>
<contactref element="LOWER" pad="2"/>
</signal>
<signal name="FAN_PWM">
<contactref element="D32" pad="IO16"/>
<contactref element="FAN" pad="4"/>
</signal>
<signal name="FAN_RPM">
<contactref element="D32" pad="IO17"/>
<contactref element="FAN" pad="3"/>
</signal>
<signal name="HEAT_PWM">
<contactref element="D32" pad="IO13"/>
<contactref element="HEAT" pad="1"/>
</signal>
<signal name="ODAT">
<contactref element="R5" pad="P$2"/>
<contactref element="D32" pad="IO14"/>
<contactref element="OUTPUT" pad="2"/>
</signal>
<signal name="12V">
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="FAN" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="IC1" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="D32" pad="VBUS"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
