<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.4" y2="0" width="0" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="25.4" width="0" layer="20"/>
<wire x1="25.4" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<hole x="12.7" y="14.605" drill="2.9972"/>
<text>Deaf Kids
Code</text>
<text>LDR</text>
<text>LDR</text>
<text>MSRAL</text>
<text>LF v2.0</text>
<text>-</text>
<text>+</text>
<text>LEFT</text>
<text>RIGHT</text>
<text>BAT</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 220 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO214AA">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R_L" library="SparkFun-Passives" package="1206" value="180">
<attribute name="NAME"/>
</element>
<element name="TRAN_L" library="transistor" package="TO220V" value="TIP31C">
<attribute name="NAME"/>
</element>
<element name="R_R" library="SparkFun-Passives" package="1206" value="180">
<attribute name="NAME"/>
</element>
<element name="TRAN_R" library="transistor" package="TO220V" value="TIP31C">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="L2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="DL" library="diode" package="DO214AA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DR" library="diode" package="DO214AA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_PWR" library="SparkFun-Passives" package="1206" value="470">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="">
<attribute name="PROD_ID" value="CONN-08399"/>
</element>
<element name="DP" library="diode" package="DO214AA" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="TRAN_L" pad="3"/>
<contactref element="TRAN_R" pad="3"/>
<contactref element="R_PWR" pad="1"/>
<contactref element="R_L" pad="2"/>
<contactref element="R_R" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="PWR" pad="A"/>
<contactref element="R1" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="DP" pad="C"/>
<contactref element="DL" pad="C"/>
<contactref element="DR" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="TRAN_R" pad="1"/>
<contactref element="R_R" pad="1"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="PWR" pad="K"/>
<contactref element="R_PWR" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="TRAN_L" pad="1"/>
<contactref element="R_L" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="TRAN_L" pad="2"/>
<contactref element="DL" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="J3" pad="1"/>
<contactref element="TRAN_R" pad="2"/>
<contactref element="DR" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="2"/>
<contactref element="DP" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
