<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="38.1" y2="0" width="0" layer="20"/>
<wire x1="38.1" y1="0" x2="38.1" y2="39.37" width="0" layer="20"/>
<wire x1="38.1" y1="39.37" x2="0" y2="39.37" width="0" layer="20"/>
<wire x1="0" y1="39.37" x2="0" y2="0" width="0" layer="20"/>
<text>1</text>
<text>1</text>
<text>SOIC-W
ADAPTER</text>
<text>PIC SOIC-W
PROGRAMMER</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X14">
</package>
<package name="1X05">
</package>
<package name="POWER_JACK_PTH">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X14" value="M14"/>
<element name="JP2" library="SparkFun-Connectors" package="1X14" value="M14"/>
<element name="JP3" library="SparkFun-Connectors" package="1X05" value="INTCONN"/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="10kΩ"/>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="5VDC">
<attribute name="PROD_ID" value="PRT-00119"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="8"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="6"/>
<contactref element="J1" pad="PWR"/>
</signal>
<signal name="N$7">
<contactref element="JP3" pad="5"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="N$2">
<contactref element="JP3" pad="1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="JP3" pad="4"/>
<contactref element="JP2" pad="14"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
