<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33.02" y2="0" width="0" layer="20"/>
<wire x1="33.02" y1="0" x2="33.02" y2="21.26" width="0" layer="20"/>
<wire x1="33.02" y1="21.26" x2="0" y2="21.26" width="0" layer="20"/>
<wire x1="0" y1="21.26" x2="0" y2="0" width="0" layer="20"/>
<text>G Stby
GR Armg
R Armd</text>
<text>G PIN?
GR Wrng
R Alarm</text>
<text>R Time 
since 
alarm. 
15 min
per flash
</text>
<text>LightSafer</text>
<text>Push to arm/disarm
Hold to turn on/off</text>
<text>v1.2</text>
</plain>
<libraries>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="SOP65P780X200-20N">
</package>
<package name="SOT95P264X112-3N">
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JOYSTICK_MINI">
<description>&lt;h3&gt;Small Tactile Joystick w/ Select Switch&lt;/h3&gt;
&lt;p&gt;A 5-way tactile switch allows for a joystick-like interface in a very small package.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/Buttons/SF303GJ26-3.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="andy">
<packages>
<package name="BC-2001">
</package>
<package name="HSMF-C1XX">
</package>
</packages>
</library>
<library name="standardparts">
<packages>
<package name="0603">
<description>http://www.panasonic.com/industrial/components/pdf/AOA0000CE1.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CHIPLED-6">
<description>CHIPLED-6 package &lt;br&gt;
Used by APDS-9301</description>
</package>
</packages>
</library>
<library name="jst-sh-more">
<packages>
<package name="SM06B-SRSS-TB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="Microchip_By_element14_Batch_1" package="SOP65P780X200-20N" value="PIC16LF18345">
<attribute name="MPN" value="PIC18F13k22-I/SS"/>
<attribute name="OC_FARNELL" value="1778460"/>
<attribute name="OC_NEWARK" value="07P9666"/>
<attribute name="PACKAGE" value="SSOP-20"/>
<attribute name="SUPPLIER" value="Microchip"/>
</element>
<element name="SW1" library="SparkFun-Switches" package="JOYSTICK_MINI" value="">
<attribute name="PROD_ID" value="SWCH-09905"/>
<attribute name="SF_SKU" value="COM-10063"/>
<attribute name="VALUE"/>
</element>
<element name="B1" library="andy" package="BC-2001" value="CR2032"/>
<element name="R1" library="standardparts" package="0603" value="1k"/>
<element name="R2" library="standardparts" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="standardparts" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="standardparts" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="standardparts" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="standardparts" package="0603" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="SparkFun-Sensors" package="CHIPLED-6" value="APDS-9300">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-13662"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="standardparts" package="0603" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="standardparts" package="0603" value="2k2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="andy" package="HSMF-C1XX" value="HSMF-C155"/>
<element name="R8" library="standardparts" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="andy" package="HSMF-C1XX" value="HSMF-C155"/>
<element name="LED3" library="andy" package="HSMF-C1XX" value="HSMF-C155"/>
<element name="JP1" library="jst-sh-more" package="SM06B-SRSS-TB" value="SM06B-SRSS-TB">
<attribute name="VALUE"/>
</element>
<element name="R9" library="standardparts" package="0603" value="2k2"/>
<element name="R10" library="standardparts" package="0603" value="2k2"/>
<element name="IC2" library="Microchip_By_element14_Batch_1" package="SOT95P264X112-3N" value="MCP1700T-2502E/TT">
<attribute name="MPN" value="MCP1700T-2502E/TT"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1605553"/>
<attribute name="OC_NEWARK" value="88H9813"/>
<attribute name="PACKAGE" value="SOT-3"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="standardparts" package="0603" value="1u0"/>
<element name="C4" library="standardparts" package="0603" value="1u0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="SW1" pad="GND"/>
<contactref element="B1" pad="3"/>
<contactref element="IC1" pad="20"/>
<contactref element="C1" pad="2"/>
<contactref element="IC3" pad="P2"/>
<contactref element="IC3" pad="P3"/>
<contactref element="JP1" pad="3"/>
<contactref element="LED1" pad="P$2"/>
<contactref element="LED1" pad="P$4"/>
<contactref element="LED2" pad="P$2"/>
<contactref element="LED2" pad="P$4"/>
<contactref element="LED3" pad="P$2"/>
<contactref element="LED3" pad="P$4"/>
<contactref element="R10" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="B1" pad="2"/>
<contactref element="B1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="IC3" pad="P5"/>
<contactref element="R7" pad="2"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="N$6">
<contactref element="IC3" pad="P4"/>
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="P$1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LED1" pad="P$3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="LED2" pad="P$1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="LED2" pad="P$3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="LED3" pad="P$1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="LED3" pad="P$3"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="19"/>
<contactref element="JP1" pad="4"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="18"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="17"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="10"/>
<contactref element="SW1" pad="D"/>
</signal>
<signal name="N$2">
<contactref element="SW1" pad="B"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$5">
<contactref element="SW1" pad="C"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="SW1" pad="A"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="SW1" pad="CTR"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="5"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$23">
<contactref element="IC3" pad="P6"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$25">
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="2V5">
<contactref element="IC3" pad="P1"/>
<contactref element="IC2" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
