<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.75" y2="0" width="0" layer="20"/>
<wire x1="31.75" y1="0" x2="31.75" y2="24.13" width="0" layer="20"/>
<wire x1="31.75" y1="24.13" x2="0" y2="24.13" width="0" layer="20"/>
<wire x1="0" y1="24.13" x2="0" y2="0" width="0" layer="20"/>
<text>Paul MacDougal v1.0
Dual RJ12 breakout</text>
</plain>
<libraries>
<library name="PaulsStuff">
<packages>
<package name="WM9177-ND">
<description>Dual RJ12 right angle connectors
Digikey part WM9177-ND
Molex part 0438146421</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP4">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="PaulsStuff" package="WM9177-ND" value="DUALRJ12"/>
<element name="JP1" library="jumper" package="JP4" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="jumper" package="JP4" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="GREEN">
<attribute name="PROD_ID" value="DIO-00821"/>
<attribute name="VALUE" value="GREEN"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="P$1"/>
<contactref element="JP1" pad="4"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="JP1" pad="3"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$3"/>
<contactref element="JP1" pad="2"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="P$4"/>
<contactref element="JP1" pad="1"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$6"/>
<contactref element="JP2" pad="3"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="P$7"/>
<contactref element="JP2" pad="2"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$8"/>
<contactref element="JP2" pad="1"/>
<contactref element="SJ4" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="D1" pad="A"/>
<contactref element="U$1" pad="P$5"/>
<contactref element="JP2" pad="4"/>
<contactref element="SJ1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
