<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="26.543" y1="15.24" x2="84.435" y2="15.24" width="0" layer="20"/>
<wire x1="84.435" y1="15.24" x2="84.435" y2="40.31" width="0" layer="20"/>
<wire x1="84.435" y1="40.31" x2="26.543" y2="40.31" width="0" layer="20"/>
<wire x1="26.543" y1="40.31" x2="26.543" y2="15.24" width="0" layer="20"/>
<text>Arduino Micro
JTAG adapter v0.2  MK7</text>
<text>USB</text>
</plain>
<libraries>
<library name="BNC_IN">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X17">
<description>&lt;h3&gt;Plated Through Hole -17 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:17&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_17&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="M50-3550542-v1">
<description>&lt;Headers &amp; Wire Housings 5+5 IDC VERT PCTAIL LATCH HEADER, MALE&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SHDR10W40P127_2X5_2083X565X116">
<description>&lt;b&gt;M50-3550542&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="BNC_IN" package="1X17" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="BNC_IN" package="1X17" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="BNC_IN" package="1X17" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="BNC_IN" package="1X17" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="M50-3550542-v1" package="SHDR10W40P127_2X5_2083X565X116" value="M50-3550542">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="Headers &amp; Wire Housings 5+5 IDC VERT PCTAIL LATCH HEADER, MALE"/>
<attribute name="HEIGHT" value="11.6mm"/>
<attribute name="MANUFACTURER_NAME" value="Harwin"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="M50-3550542"/>
<attribute name="MOUSER_PART_NUMBER" value="855-M50-3550542"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Harwin/M50-3550542?qs=gf2s0yP%252B7bcu%2Fijgwq1oDQ%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="D13">
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="3V">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="REF">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="A2-TMS">
<contactref element="J1" pad="6"/>
<contactref element="J2" pad="6"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="A3-TCK">
<contactref element="J1" pad="7"/>
<contactref element="J2" pad="7"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="A4">
<contactref element="J1" pad="8"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="A5">
<contactref element="J1" pad="9"/>
<contactref element="J2" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="10"/>
<contactref element="J2" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="11"/>
<contactref element="J2" pad="11"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="12"/>
<contactref element="J2" pad="12"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="RST">
<contactref element="J1" pad="13"/>
<contactref element="J2" pad="13"/>
<contactref element="J3" pad="13"/>
<contactref element="J4" pad="13"/>
<contactref element="J5" pad="6"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="14"/>
<contactref element="J2" pad="14"/>
<contactref element="J3" pad="12"/>
<contactref element="J4" pad="12"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="10"/>
</signal>
<signal name="VIN">
<contactref element="J1" pad="15"/>
<contactref element="J2" pad="15"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="16"/>
<contactref element="J2" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="17"/>
<contactref element="J2" pad="17"/>
</signal>
<signal name="D12">
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="D11">
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="D10">
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="D9">
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="D8">
<contactref element="J3" pad="5"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="D7">
<contactref element="J3" pad="6"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="D6">
<contactref element="J3" pad="7"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="D5">
<contactref element="J3" pad="8"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="D4">
<contactref element="J3" pad="9"/>
<contactref element="J4" pad="9"/>
</signal>
<signal name="D3">
<contactref element="J3" pad="10"/>
<contactref element="J4" pad="10"/>
</signal>
<signal name="D2">
<contactref element="J3" pad="11"/>
<contactref element="J4" pad="11"/>
</signal>
<signal name="RX1">
<contactref element="J3" pad="14"/>
<contactref element="J4" pad="14"/>
</signal>
<signal name="TX1">
<contactref element="J3" pad="15"/>
<contactref element="J4" pad="15"/>
</signal>
<signal name="SS">
<contactref element="J3" pad="16"/>
<contactref element="J4" pad="16"/>
</signal>
<signal name="MOSI">
<contactref element="J3" pad="17"/>
<contactref element="J4" pad="17"/>
</signal>
<signal name="A0-TDI">
<contactref element="J2" pad="4"/>
<contactref element="J1" pad="4"/>
<contactref element="J5" pad="9"/>
</signal>
<signal name="A1-TDO">
<contactref element="J5" pad="3"/>
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
