<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>LAYER-STACK</text>
<text>01-16</text>
<text>01-20</text>
<text>SV1</text>
<text>SV2</text>
<text>CellarWarden RJ45 4 Port</text>
<hole x="3.81" y="38.1" drill="2.2"/>
<hole x="3.81" y="6.35" drill="2.2"/>
<hole x="73.66" y="6.35" drill="2.2"/>
<hole x="73.66" y="38.1" drill="2.2"/>
<text>SV1</text>
<text>SV2</text>
<text>CellarWarden RJ45 4 Port</text>
<wire x1="1.27" y1="43.18" x2="1.27" y2="2.54" width="0.4064" layer="20"/>
<wire x1="1.27" y1="2.54" x2="76.2" y2="2.54" width="0.4064" layer="20"/>
<wire x1="76.2" y1="2.54" x2="76.2" y2="43.18" width="0.4064" layer="20"/>
<wire x1="76.2" y1="43.18" x2="1.27" y2="43.18" width="0.4064" layer="20"/>
<text>W/Org</text>
<text>Org</text>
<text>W/Grn</text>
<text>Blu</text>
<text>W/Blu</text>
<text>Grn</text>
<text>W/Brn</text>
<text>Brn</text>
<text>JP1</text>
<text>JP2</text>
<text>JP3</text>
<text>JP4</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE08">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="drilegend">
<packages>
<package name="DRILEGEND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="RJ45-8" value="RJ45">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="SV1" library="con-lsta" package="FE08" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="SV2" library="con-lsta" package="FE08" value="">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
</element>
<element name="DRILEGEND" library="drilegend" package="DRILEGEND" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="SV2" pad="1"/>
<contactref element="SV1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="2"/>
<contactref element="SV2" pad="2"/>
<contactref element="SV1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="3"/>
<contactref element="SV2" pad="3"/>
<contactref element="SV1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="4"/>
<contactref element="SV2" pad="4"/>
<contactref element="SV1" pad="4"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="5"/>
<contactref element="SV2" pad="5"/>
<contactref element="SV1" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="5"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="6"/>
<contactref element="SV2" pad="6"/>
<contactref element="SV1" pad="6"/>
<contactref element="J2" pad="6"/>
<contactref element="J3" pad="6"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="7"/>
<contactref element="SV2" pad="7"/>
<contactref element="SV1" pad="7"/>
<contactref element="J2" pad="7"/>
<contactref element="J3" pad="7"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="8"/>
<contactref element="SV2" pad="8"/>
<contactref element="SV1" pad="8"/>
<contactref element="J2" pad="8"/>
<contactref element="J3" pad="8"/>
<contactref element="J4" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
