<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<text>FDL-3 DCP v1.3</text>
<wire x1="0" y1="0" x2="45.72" y2="0" width="0.4064" layer="20"/>
<wire x1="45.72" y1="0" x2="45.72" y2="33.02" width="0.4064" layer="20"/>
<wire x1="45.72" y1="33.02" x2="0" y2="33.02" width="0.4064" layer="20"/>
<wire x1="0" y1="33.02" x2="0" y2="0" width="0.4064" layer="20"/>
<text>+</text>
<text>+</text>
<text>Project FDL</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
</plain>
<libraries>
<library name="Rembrandt Electronics - JST XH Connectors v1-0">
<packages>
<package name="JST-XH-02-PACKAGE-LONG-PAD">
<description>&lt;b&gt;JST XH Connector Long Pads (Package)&lt;/b&gt;&lt;p&gt;

Wire to board connector.

Pitch: 2,54 mm, (0.100")&lt;p&gt;
Number of pins: &lt;b&gt;2&lt;/b&gt;&lt;b&gt;&lt;P&gt;

&lt;b&gt;Created by Rembrandt Electronics&lt;/b&gt;&lt;p&gt;
&lt;b&gt;www.rembrandtelectronics.com&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 220 Vertical&lt;/b&gt; Package works with various parts including N-Channel MOSFET SparkFun SKU: COM-10213</description>
</package>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="DIODE-1N4001">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
<package name="1X02">
</package>
<package name="1X03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BAT" library="Rembrandt Electronics - JST XH Connectors v1-0" package="JST-XH-02-PACKAGE-LONG-PAD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MOT" library="Rembrandt Electronics - JST XH Connectors v1-0" package="JST-XH-02-PACKAGE-LONG-PAD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO220V" value="N-CH">
<attribute name="PROD_ID" value="TRANS-10060"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO220V" value="P-CH">
<attribute name="PROD_ID" value="TRANS-13060"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="TO-92" value="NPN">
<attribute name="PROD_ID" value="TRANS-08447"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4001" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="PSHF" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="PSHR" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="TRG" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="ESC" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NEO" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="1k">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="4.7k">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="100k">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
</elements>
<signals>
<signal name="BRK">
<contactref element="Q3" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="Q2" pad="1"/>
<contactref element="R2" pad="P$1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="MOT" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="Q2" pad="3"/>
<contactref element="BAT" pad="2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="MOT" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="MOT">
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="NEO" pad="3"/>
<contactref element="J1" pad="10"/>
<contactref element="ESC" pad="3"/>
<contactref element="R5" pad="P$2"/>
<contactref element="TRG" pad="2"/>
<contactref element="R7" pad="P$1"/>
<contactref element="BAT" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q3" pad="1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="9"/>
<contactref element="ESC" pad="2"/>
<contactref element="NEO" pad="2"/>
<contactref element="PSHR" pad="2"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="ESCDAT">
<contactref element="ESC" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="NEO">
<contactref element="NEO" pad="1"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="PSH">
<contactref element="J1" pad="3"/>
<contactref element="PSHR" pad="1"/>
<contactref element="PSHF" pad="1"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="P$2"/>
<contactref element="PSHF" pad="2"/>
</signal>
<signal name="TRG">
<contactref element="J1" pad="4"/>
<contactref element="TRG" pad="1"/>
</signal>
<signal name="VLT">
<contactref element="J1" pad="8"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
