<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.1">
<drawing>
<board>
<plain>
<text>12VDC</text>
<text>5VDC</text>
<text>VIN</text>
<text>12v</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>5V Regulator</text>
<text>5v</text>
<text>12v</text>
<text>Indicator
Light Strip</text>
<text>OMSI - After Shock Rescue
Thomas Hudson
07/12/18</text>
<wire x1="63.58" y1="-1.016" x2="1.444" y2="-1.016" width="0.1524" layer="20"/>
<wire x1="1.444" y1="-1.016" x2="-3.556" y2="3.984" width="0.1524" layer="20" curve="-90"/>
<wire x1="-3.556" y1="3.984" x2="-3.556" y2="84.916" width="0.1524" layer="20"/>
<wire x1="-3.556" y1="84.916" x2="1.444" y2="89.916" width="0.1524" layer="20" curve="-90"/>
<wire x1="1.444" y1="89.916" x2="63.58" y2="89.916" width="0.1524" layer="20"/>
<wire x1="63.58" y1="89.916" x2="68.58" y2="84.916" width="0.1524" layer="20" curve="-90"/>
<wire x1="68.58" y1="84.916" x2="68.58" y2="3.984" width="0.1524" layer="20"/>
<wire x1="68.58" y1="3.984" x2="63.58" y2="-1.016" width="0.1524" layer="20" curve="-90"/>
<text>12</text>
<text>N/C</text>
<text>TSR 1-2450</text>
<text>GND</text>
<text>D0</text>
<text>Motor
Sensor</text>
<text>GND</text>
<text>DI</text>
<text>5V</text>
<text>11</text>
<text>GND</text>
<text>Extra Pins</text>
<text>Diorama
 Pixels</text>
<text>GND</text>
<text>D0</text>
<text>Servo 
 PWM</text>
<text>GND</text>
<text>~6</text>
<text>5V</text>
<text>N/C</text>
<text>GND</text>
<text>~3</text>
<text>Transport
   PWM</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector PTH&lt;/h3&gt;
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
<package name="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="th_libraries">
<packages>
<package name="UNO_R3_SHIELD">
<description>Uno R3 Compatible Board Layout</description>
</package>
</packages>
</library>
<library name="con-phoenix-508">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;pho508a.lbr
&lt;li&gt;pho508b.lbr
&lt;li&gt;pho508c.lbr
&lt;li&gt;pho508d.lbr
&lt;li&gt;pho508e.lbr
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MSTBA3">
<description>&lt;b&gt;PHOENIX&lt;/b&gt;</description>
</package>
<package name="MSTBA2">
<description>&lt;b&gt;PHOENIX&lt;/b&gt;</description>
</package>
<package name="MSTBA4">
<description>&lt;b&gt;PHOENIX&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DC-DC_CONVERTER_78XX">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12VOLT" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACK">
<attribute name="PROD_ID" value="CONN-08197"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.3" value="1000">
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.3" value="1000">
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="th_libraries" package="UNO_R3_SHIELD" value="ARDUINO_R3_SHIELD"/>
<element name="J8" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-phoenix-508" package="MSTBA2" value="MSTBA2">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="1757242"/>
<attribute name="OC_FARNELL" value="3705171"/>
<attribute name="OC_NEWARK" value="71C4161"/>
</element>
<element name="JP1" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value="JUMPER-PAD-2-NC_BY_TRACE"/>
<element name="X8" library="con-phoenix-508" package="MSTBA3" value="MSTBA3">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="1757255"/>
<attribute name="OC_FARNELL" value="3705183"/>
<attribute name="OC_NEWARK" value="71C4162"/>
</element>
<element name="R9" library="SparkFun-Passives" package="AXIAL-0.3" value="120"/>
<element name="C2" library="SparkFun-Passives" package="CPOL-RADIAL-1000UF-25V" value=""/>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-1000UF-25V" value=""/>
<element name="U2" library="SparkFun-IC-Power" package="DC-DC_CONVERTER_78XX" value="R-78E5.0-1.0">
<attribute name="PROD_ID" value="COM-13655"/>
</element>
<element name="R12" library="SparkFun-Passives" package="AXIAL-0.3" value="120">
<attribute name="VALUE"/>
</element>
<element name="X9" library="con-phoenix-508" package="MSTBA2" value="MSTBA2">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="1757242"/>
<attribute name="OC_FARNELL" value="3705171"/>
<attribute name="OC_NEWARK" value="71C4161"/>
</element>
<element name="R13" library="SparkFun-Passives" package="AXIAL-0.3" value="120">
<attribute name="VALUE"/>
</element>
<element name="X11" library="con-phoenix-508" package="MSTBA2" value="MSTBA2">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="1757242"/>
<attribute name="OC_FARNELL" value="3705171"/>
<attribute name="OC_NEWARK" value="71C4161"/>
</element>
<element name="X12" library="con-phoenix-508" package="MSTBA2" value="MSTBA2">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="1757242"/>
<attribute name="OC_FARNELL" value="3705171"/>
<attribute name="OC_NEWARK" value="71C4161"/>
</element>
<element name="JP2" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value="JUMPER-PAD-2-NC_BY_TRACE"/>
<element name="X2" library="con-phoenix-508" package="MSTBA3" value="MSTBA3">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="1757255"/>
<attribute name="OC_FARNELL" value="3705183"/>
<attribute name="OC_NEWARK" value="71C4162"/>
</element>
<element name="X3" library="con-phoenix-508" package="MSTBA4" value="MSTBA4">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="1757268"/>
<attribute name="OC_FARNELL" value="3705195"/>
<attribute name="OC_NEWARK" value="71C4163"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="12VOLT" pad="GND"/>
<contactref element="12VOLT" pad="GNDBREAK"/>
<contactref element="D3" pad="K"/>
<contactref element="D4" pad="K"/>
<contactref element="J3" pad="GND@0"/>
<contactref element="J3" pad="GND@1"/>
<contactref element="J3" pad="GND@2"/>
<contactref element="X1" pad="1"/>
<contactref element="J8" pad="1"/>
<contactref element="X8" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="GND"/>
<contactref element="X9" pad="1"/>
<contactref element="X11" pad="1"/>
<contactref element="X12" pad="1"/>
<contactref element="X2" pad="1"/>
<contactref element="X3" pad="1"/>
<contactref element="X3" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="R4" pad="P$2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$31">
<contactref element="R5" pad="P$2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="J3" pad="VIN"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="X12" pad="2"/>
<contactref element="J3" pad="D6"/>
</signal>
<signal name="N$7">
<contactref element="J3" pad="D8"/>
<contactref element="R12" pad="P$1"/>
</signal>
<signal name="N$29">
<contactref element="J3" pad="D9"/>
<contactref element="R13" pad="P$1"/>
</signal>
<signal name="5V">
<contactref element="R5" pad="P$1"/>
<contactref element="J1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="VOUT"/>
<contactref element="JP2" pad="2"/>
<contactref element="X2" pad="3"/>
<contactref element="X3" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="X8" pad="2"/>
<contactref element="J3" pad="D12"/>
</signal>
<signal name="N$34">
<contactref element="J3" pad="D11"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="N$33">
<contactref element="X8" pad="3"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="12V">
<contactref element="U2" pad="VIN"/>
<contactref element="X3" pad="4"/>
<contactref element="12VOLT" pad="PWR"/>
<contactref element="R4" pad="P$1"/>
<contactref element="J9" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="X1" pad="2"/>
<contactref element="R12" pad="P$2"/>
</signal>
<signal name="N$40">
<contactref element="X9" pad="2"/>
<contactref element="R13" pad="P$2"/>
</signal>
<signal name="N$11">
<contactref element="J3" pad="D3"/>
<contactref element="X11" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="J3" pad="5V"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="X2" pad="2"/>
<contactref element="J3" pad="A0"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
