<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="137.16" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="48.26" y2="0" width="0" layer="20"/>
<wire x1="48.26" y1="0" x2="50.8" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="50.8" y1="2.54" x2="50.8" y2="137.16" width="0" layer="20"/>
<wire x1="50.8" y1="137.16" x2="48.26" y2="139.7" width="0" layer="20" curve="90"/>
<wire x1="48.26" y1="139.7" x2="2.54" y2="139.7" width="0" layer="20"/>
<wire x1="2.54" y1="139.7" x2="0" y2="137.16" width="0" layer="20" curve="90"/>
<text>Retro-Pin</text>
</plain>
<libraries>
<library name="ECA-Connectors">
<description>&lt;h3&gt;Eric Conner Apps - Connectors&lt;/h3&gt;
&lt;p&gt;This library contains electrically-functional connectors.&lt;/p&gt;</description>
<packages>
<package name="KK-156-12">
</package>
<package name="KK-156-9">
</package>
<package name="KK-156-3">
</package>
<package name="KK-156-4">
</package>
</packages>
</library>
<library name="ECA-Aesthetics">
<description>&lt;h3&gt;Eric Conner Apps - Aesthetics&lt;/h3&gt;
&lt;p&gt;This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc.&lt;/p&gt;</description>
<packages>
<package name="MOUNT_HOLE-150MIL">
</package>
<package name="ECA_LOGO">
</package>
</packages>
</library>
<library name="ECA-Passives">
<description>&lt;h3&gt;Eric Conner Apps - Passives&lt;/h3&gt;
&lt;p&gt;This library contiains passive items such as ressistors, capacitors, diodes, LEDs, etc.&lt;/p&gt;</description>
<packages>
<package name="RADIAL-CAN-4MM">
</package>
<package name="DPAK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="16V" library="ECA-Connectors" package="KK-156-12" value="1X12-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="28V" library="ECA-Connectors" package="KK-156-9" value="1X9-MOLEX">
<attribute name="DIGIKEY" value="WM2107-ND"/>
</element>
<element name="5V" library="ECA-Connectors" package="KK-156-9" value="1X9-MOLEX">
<attribute name="DIGIKEY" value="WM2107-ND"/>
</element>
<element name="DISPLAY" library="ECA-Connectors" package="KK-156-3" value="1X3-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="DRIVER" library="ECA-Connectors" package="KK-156-3" value="1X3-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="LAMP" library="ECA-Connectors" package="KK-156-3" value="1X3-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="MPU" library="ECA-Connectors" package="KK-156-3" value="1X3-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="SOLENOID" library="ECA-Connectors" package="KK-156-4" value="1X4-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="SOLENOIDS" library="ECA-Connectors" package="KK-156-9" value="1X9-MOLEX">
<attribute name="DIGIKEY" value="WM2107-ND"/>
</element>
<element name="SPECIAL" library="ECA-Connectors" package="KK-156-4" value="1X4-MOLEX">
<attribute name="DIGIKEY" value=""/>
<attribute name="VALUE" value=""/>
</element>
<element name="SWITCH" library="ECA-Connectors" package="KK-156-3" value="1X3-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="AUX_SOLENOID" library="ECA-Connectors" package="KK-156-4" value="1X4-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="AMP" library="ECA-Connectors" package="KK-156-3" value="1X3-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="U$1" library="ECA-Aesthetics" package="MOUNT_HOLE-150MIL" value=""/>
<element name="U$2" library="ECA-Aesthetics" package="MOUNT_HOLE-150MIL" value=""/>
<element name="U$3" library="ECA-Aesthetics" package="MOUNT_HOLE-150MIL" value=""/>
<element name="U$4" library="ECA-Aesthetics" package="MOUNT_HOLE-150MIL" value=""/>
<element name="C1" library="ECA-Passives" package="RADIAL-CAN-4MM" value="10uF">
<attribute name="ATTRIBUTE" value="4mm"/>
<attribute name="DIGIKEY" value=""/>
</element>
<element name="C2" library="ECA-Passives" package="RADIAL-CAN-4MM" value="10uF">
<attribute name="ATTRIBUTE" value="4mm"/>
<attribute name="DIGIKEY" value=""/>
</element>
<element name="X1" library="ECA-Passives" package="DPAK" value="NCP1117">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="U$16" library="ECA-Aesthetics" package="ECA_LOGO" value="">
<attribute name="PROJECT" value="Power Adapter"/>
<attribute name="VERSION" value="1.0.0"/>
<attribute name="YEAR" value="2017"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="28V" pad="2"/>
<contactref element="28V" pad="3"/>
<contactref element="5V" pad="4"/>
<contactref element="5V" pad="3"/>
<contactref element="5V" pad="2"/>
<contactref element="5V" pad="1"/>
<contactref element="16V" pad="1"/>
<contactref element="16V" pad="2"/>
<contactref element="16V" pad="3"/>
<contactref element="16V" pad="4"/>
<contactref element="16V" pad="9"/>
<contactref element="16V" pad="10"/>
<contactref element="16V" pad="11"/>
<contactref element="16V" pad="12"/>
<contactref element="DISPLAY" pad="2"/>
<contactref element="DRIVER" pad="2"/>
<contactref element="MPU" pad="2"/>
<contactref element="SWITCH" pad="2"/>
<contactref element="LAMP" pad="2"/>
<contactref element="SOLENOID" pad="3"/>
<contactref element="SOLENOID" pad="2"/>
<contactref element="SOLENOIDS" pad="2"/>
<contactref element="SOLENOIDS" pad="3"/>
<contactref element="SPECIAL" pad="3"/>
<contactref element="AUX_SOLENOID" pad="3"/>
<contactref element="AUX_SOLENOID" pad="2"/>
<contactref element="AMP" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="5V" pad="6"/>
<contactref element="5V" pad="7"/>
<contactref element="5V" pad="8"/>
<contactref element="5V" pad="9"/>
<contactref element="C1" pad="+"/>
<contactref element="X1" pad="3"/>
<contactref element="MPU" pad="3"/>
<contactref element="DRIVER" pad="3"/>
<contactref element="DISPLAY" pad="3"/>
<contactref element="LAMP" pad="1"/>
<contactref element="SWITCH" pad="1"/>
<contactref element="AMP" pad="1"/>
</signal>
<signal name="16V">
<contactref element="16V" pad="5"/>
<contactref element="16V" pad="6"/>
<contactref element="16V" pad="7"/>
<contactref element="16V" pad="8"/>
<contactref element="LAMP" pad="3"/>
<contactref element="SWITCH" pad="3"/>
<contactref element="AMP" pad="3"/>
</signal>
<signal name="FLIPPER_28V">
<contactref element="SOLENOIDS" pad="4"/>
<contactref element="28V" pad="4"/>
<contactref element="SPECIAL" pad="1"/>
<contactref element="SOLENOIDS" pad="5"/>
<contactref element="28V" pad="5"/>
<contactref element="SPECIAL" pad="2"/>
</signal>
<signal name="SOLENOID_28V">
<contactref element="SOLENOID" pad="1"/>
<contactref element="SOLENOID" pad="4"/>
<contactref element="SPECIAL" pad="4"/>
<contactref element="28V" pad="8"/>
<contactref element="SOLENOIDS" pad="8"/>
<contactref element="SOLENOIDS" pad="7"/>
<contactref element="28V" pad="7"/>
<contactref element="SOLENOIDS" pad="6"/>
<contactref element="28V" pad="6"/>
<contactref element="AUX_SOLENOID" pad="1"/>
<contactref element="AUX_SOLENOID" pad="4"/>
</signal>
<signal name="3.3V">
<contactref element="DRIVER" pad="1"/>
<contactref element="DISPLAY" pad="1"/>
<contactref element="C2" pad="+"/>
<contactref element="X1" pad="4"/>
<contactref element="MPU" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
