<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<polygon width="0.1524" layer="20">
<vertex x="26.4" y="33.7"/>
<vertex x="26.4" y="50.8"/>
<vertex x="44.7" y="50.8"/>
<vertex x="44.7" y="33.7"/>
</polygon>
<text>Backpower Blocker</text>
<text>(c)2022 W7AY</text>
</plain>
<libraries>
<library name="GSB311131HR">
<packages>
<package name="AMPHENOL_GSB311131HR">
</package>
</packages>
</library>
<library name="USB3male">
<packages>
<package name="AMPHENOL_GSB416445CHR">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GSB3111" library="GSB311131HR" package="AMPHENOL_GSB311131HR" value="GSB311131HR">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" USB 3.0, Type A, Receptacle, Right Angle, 9 Pins, Shell with Nickel Plating, 30μinin Gold, Dip 2.4mm, Blue High Temperature Housing, Tray Packaging "/>
<attribute name="MF" value="Amphenol ICC"/>
<attribute name="MP" value="GSB311131HR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/GSB311131HR/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="GSB4164" library="USB3male" package="AMPHENOL_GSB416445CHR" value="GSB416445CHR">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" USB 3.1 GEN 2, Type A, Plug, Right Angle SMT, 9 Pins, Offset 0.3mm, 1.9mm Height, Shell Dip with Nickel Plating, 30μinin Gold, Blue High Temperature Housing, Tape and Reel Packaging "/>
<attribute name="MF" value="Amphenol ICC"/>
<attribute name="MP" value="GSB416445CHR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/GSB416445CHR/?ref=eda"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="GSB3111" pad="2"/>
<contactref element="GSB4164" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="GSB3111" pad="3"/>
<contactref element="GSB4164" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="GSB3111" pad="5"/>
<contactref element="GSB4164" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="GSB3111" pad="6"/>
<contactref element="GSB4164" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="GSB3111" pad="8"/>
<contactref element="GSB4164" pad="8"/>
</signal>
<signal name="GND">
<contactref element="GSB4164" pad="S1"/>
<contactref element="GSB4164" pad="S2"/>
<contactref element="GSB3111" pad="SH1"/>
<contactref element="GSB3111" pad="SH2"/>
</signal>
<signal name="N$1">
<contactref element="GSB3111" pad="4"/>
<contactref element="GSB4164" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="GSB4164" pad="7"/>
<contactref element="GSB3111" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="GSB4164" pad="9"/>
<contactref element="GSB3111" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
