<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.78" y2="0" width="0" layer="20"/>
<wire x1="17.78" y1="0" x2="17.78" y2="21.59" width="0" layer="20"/>
<wire x1="17.78" y1="21.59" x2="0" y2="21.59" width="0" layer="20"/>
<wire x1="0" y1="21.59" x2="0" y2="0" width="0" layer="20"/>
<text>3.0-4.2v</text>
<text>3.3v</text>
<text>VOUT</text>
<text>VIN</text>
<text>VIN</text>
<text>EN</text>
<text>GND</text>
<text>GND</text>
</plain>
<libraries>
<library name="Murata_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 21/03/2012 17:47:01</description>
<packages>
<package name="CAPC1608X85N">
</package>
</packages>
</library>
<library name="Kemet_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 28/03/2012 12:54:09</description>
<packages>
<package name="CAPC1005X60N">
</package>
</packages>
</library>
<library name="32bits">
<packages>
<package name="PERIODIC_SYMBOL_BACK">
</package>
<package name="AISC-1008">
</package>
<package name="RMW12">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Dialight_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 13/06/2012 13:59:22</description>
<packages>
<package name="LED_597-3311-407F">
</package>
</packages>
</library>
<library name="Yageo_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 21/03/2012 16:17:53</description>
<packages>
<package name="RESC1005X40N">
</package>
</packages>
</library>
<library name="Vishay_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 16:36:08</description>
<packages>
<package name="RESC1608X60N">
</package>
<package name="SOT95P237X112-3N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CIN" library="Murata_By_element14_Batch_1" package="CAPC1608X85N" value="10uF">
<attribute name="OC_NEWARK" value="24R6334"/>
<attribute name="SUPPLIER" value="Murata"/>
<attribute name="OC_FARNELL" value="1735528"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VOLTAGERATING" value="6.3V"/>
<attribute name="MPN" value="GRM188R60J106ME47D "/>
<attribute name="NAME"/>
</element>
<element name="COUT" library="Murata_By_element14_Batch_1" package="CAPC1608X85N" value="10uF">
<attribute name="OC_NEWARK" value="24R6334"/>
<attribute name="SUPPLIER" value="Murata"/>
<attribute name="OC_FARNELL" value="1735528"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VOLTAGERATING" value="6.3V"/>
<attribute name="MPN" value="GRM188R60J106ME47D "/>
<attribute name="NAME"/>
</element>
<element name="COUTX" library="Murata_By_element14_Batch_1" package="CAPC1608X85N" value="10uF">
<attribute name="OC_NEWARK" value="24R6334"/>
<attribute name="SUPPLIER" value="Murata"/>
<attribute name="OC_FARNELL" value="1735528"/>
<attribute name="TOLERANCE" value="±20%"/>
<attribute name="VOLTAGERATING" value="6.3V"/>
<attribute name="MPN" value="GRM188R60J106ME47D "/>
<attribute name="NAME"/>
</element>
<element name="CSS" library="Kemet_By_element14_Batch_1" package="CAPC1005X60N" value="1.3nF">
<attribute name="OC_NEWARK" value="29T8930"/>
<attribute name="SUPPLIER" value="KEMET"/>
<attribute name="OC_FARNELL" value="1865439"/>
<attribute name="TOLERANCE" value="±5%"/>
<attribute name="VOLTAGERATING" value="50V"/>
<attribute name="MPN" value="C0402C132J5GACTU"/>
<attribute name="NAME"/>
</element>
<element name="HE" library="32bits" package="PERIODIC_SYMBOL_BACK" value="2">
<attribute name="DESC" value="rev.0"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="L1" library="32bits" package="AISC-1008" value="AISC-1008-1R5J-T">
<attribute name="VENDOR" value="Abracon"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AISC10081R5JT"/>
</element>
<element name="PG" library="Dialight_By_element14_Batch_1" package="LED_597-3311-407F" value="597-3311-407F">
<attribute name="PACKAGE" value="1206- Green LED"/>
<attribute name="OC_NEWARK" value="30K4957"/>
<attribute name="SUPPLIER" value="Dialight"/>
<attribute name="OC_FARNELL" value="1519493"/>
<attribute name="COLOR" value="Green"/>
<attribute name="MPN" value="597-3311-407F"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="Yageo_By_element14_Batch_1" package="RESC1005X40N" value="100 Ohms">
<attribute name="WATTAGE" value="0.0625 W"/>
<attribute name="OC_NEWARK" value="68H9765"/>
<attribute name="SUPPLIER" value="YAGEO"/>
<attribute name="OC_FARNELL" value="-"/>
<attribute name="TOLERANCE" value="±1%"/>
<attribute name="MPN" value="9C04021A1000FLHF3"/>
<attribute name="NAME"/>
</element>
<element name="RPG" library="Vishay_By_element14_Batch_1" package="RESC1608X60N" value="100K Ohms">
<attribute name="WATTAGE" value="0.1W"/>
<attribute name="OC_NEWARK" value="42K3668"/>
<attribute name="SUPPLIER" value="Vishay"/>
<attribute name="OC_FARNELL" value="1469649"/>
<attribute name="TOLERANCE" value="± 1.0 %"/>
<attribute name="MPN" value="CRCW0603100KFKEA"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="32bits" package="RMW12" value="TPS63051RMW"/>
<element name="U2" library="Vishay_By_element14_Batch_1" package="SOT95P237X112-3N" value="SI2301BDS-T1-E3">
<attribute name="PACKAGE" value="SOT-23-3"/>
<attribute name="OC_NEWARK" value="06J7561"/>
<attribute name="SUPPLIER" value="VISHAY"/>
<attribute name="OC_FARNELL" value="1470099"/>
<attribute name="MPN" value="SI2301BDS-T1-E3"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="L1">
<contactref element="U1" pad="P$1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="L2">
<contactref element="L1" pad="1"/>
<contactref element="U1" pad="P$3"/>
</signal>
<signal name="NPG">
<contactref element="U1" pad="P$8"/>
<contactref element="RPG" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="RPG" pad="1"/>
<contactref element="COUT" pad="2"/>
<contactref element="U1" pad="P$5"/>
<contactref element="U1" pad="P$4"/>
<contactref element="COUTX" pad="2"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="GND">
<contactref element="COUTX" pad="1"/>
<contactref element="COUT" pad="1"/>
<contactref element="U1" pad="P$2"/>
<contactref element="U1" pad="P$9"/>
<contactref element="CSS" pad="1"/>
<contactref element="U1" pad="P$6"/>
<contactref element="CIN" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="SS">
<contactref element="U1" pad="P$7"/>
<contactref element="CSS" pad="2"/>
</signal>
<signal name="EN">
<contactref element="U1" pad="P$11"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="P$10"/>
<contactref element="U1" pad="P$12"/>
<contactref element="CIN" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="PG" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="PG" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
