<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19.99" y2="0" width="0" layer="20"/>
<wire x1="19.99" y1="0" x2="19.99" y2="35.55" width="0" layer="20"/>
<wire x1="19.99" y1="35.55" x2="0" y2="35.55" width="0" layer="20"/>
<wire x1="0" y1="35.55" x2="0" y2="0" width="0" layer="20"/>
<text>28-pin 0.3" to 0.6" adapter</text>
</plain>
<libraries>
<library name="ic-package">
<description>&lt;b&gt;IC Packages an Sockets&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="ic-package" package="DIL28-6" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="ic-package" package="DIL28-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="P1">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="P2">
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="P3">
<contactref element="IC1" pad="3"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="P4">
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="P5">
<contactref element="IC1" pad="5"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="P6">
<contactref element="IC1" pad="6"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="P7">
<contactref element="IC1" pad="7"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="P8">
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="P10">
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="P11">
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="P12">
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="P13">
<contactref element="IC1" pad="13"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="P14">
<contactref element="IC1" pad="14"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="P9">
<contactref element="IC2" pad="9"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="P28">
<contactref element="IC1" pad="28"/>
<contactref element="IC2" pad="28"/>
</signal>
<signal name="P27">
<contactref element="IC1" pad="27"/>
<contactref element="IC2" pad="27"/>
</signal>
<signal name="P26">
<contactref element="IC1" pad="26"/>
<contactref element="IC2" pad="26"/>
</signal>
<signal name="P25">
<contactref element="IC1" pad="25"/>
<contactref element="IC2" pad="25"/>
</signal>
<signal name="P24">
<contactref element="IC1" pad="24"/>
<contactref element="IC2" pad="24"/>
</signal>
<signal name="P23">
<contactref element="IC1" pad="23"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="P22">
<contactref element="IC1" pad="22"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="P21">
<contactref element="IC1" pad="21"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="P20">
<contactref element="IC1" pad="20"/>
<contactref element="IC2" pad="20"/>
</signal>
<signal name="P19">
<contactref element="IC1" pad="19"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="P18">
<contactref element="IC1" pad="18"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="P17">
<contactref element="IC1" pad="17"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="P16">
<contactref element="IC1" pad="16"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="P15">
<contactref element="IC1" pad="15"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="GND">
</signal>
</signals>
</board>
</drawing>
</eagle>
