<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="3" x2="3" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3" y1="0" x2="62" y2="0" width="0" layer="20"/>
<wire x1="62" y1="0" x2="65" y2="3" width="0" layer="20" curve="90"/>
<wire x1="65" y1="3" x2="65" y2="53" width="0" layer="20"/>
<wire x1="65" y1="53" x2="62" y2="56" width="0" layer="20" curve="90"/>
<wire x1="62" y1="56" x2="3" y2="56" width="0" layer="20"/>
<wire x1="3" y1="56" x2="0" y2="53" width="0" layer="20" curve="90"/>
<wire x1="0" y1="53" x2="0" y2="3" width="0" layer="20"/>
<hole x="3.5" y="3.5" drill="2.8"/>
<hole x="3.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="3.5" drill="2.8"/>
<text>TOP</text>
<text>BOTTOM</text>
<text>IO-A6</text>
<text>Power Board</text>
<text>Rev 1.0
AGW Dec 2017</text>
<text>Batt 1</text>
<text>Batt 2</text>
<text>12V Load</text>
<text>12V Bat</text>
<text>Charging</text>
<text>DC OK</text>
<text>+5V</text>
</plain>
<libraries>
<library name="FLYFISH">
<packages>
<package name="PIN_20X2">
</package>
<package name="SOIC8">
</package>
<package name="PIN_W_2">
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="QFN50P400X500X100-29N">
<description>&lt;b&gt;QFN28&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SON65P300X300X100-9N">
<description>&lt;b&gt;SON65P300X300X100-9N&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOP65P640X120-16N">
<description>&lt;b&gt;TSSOP 16&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOT65P280X145-8N">
<description>&lt;b&gt;DCN (R-PDSO-G8)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOP65P780X200-20N">
<description>&lt;b&gt;20-Lead Plastic Shrink Small Outline (SS) - 5.30 mm Body [SSOP]&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="5-PIN-TO-263(U)">
<description>&lt;b&gt;5-Pin TO-263 (U)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SMC_E">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="inductors">
<description>&lt;b&gt;Inductors and Filters&lt;/b&gt;&lt;p&gt;
Based on the previous library ind-a.lbr&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DR127">
<description>&lt;b&gt;High Power Density, High Efficiency, Shielded Inductors&lt;/b&gt;&lt;p&gt;
Source: coiltronics_dr_series.pdf</description>
</package>
<package name="DR74">
<description>&lt;b&gt;High Power Density, High Efficiency, Shielded Inductors&lt;/b&gt;&lt;p&gt;
Source: coiltronics_dr_series.pdf</description>
</package>
</packages>
</library>
<library name="transistor-fet">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,81/1,4">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="K1" library="FLYFISH" package="PIN_20X2" value="PIN20X2">
<attribute name="VALUE"/>
</element>
<element name="U1" library="FLYFISH" package="SOIC8" value="EEPROM24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="M0805" value="3k9">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="TOLERANCE" value="5%"/>
<attribute name="VALUE"/>
</element>
<element name="CFG" library="FLYFISH" package="PIN_W_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H2" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="C5" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PS1" library="SamacSys_Parts" package="QFN50P400X500X100-29N" value="MP2619EV-LF-P">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="Battery Management 2A,24V Switching Li-lon Charger With Power Path Management"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Monolithic Power Systems (MPS)"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MP2619EV-LF-P"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="R4" library="rcl" package="R1206" value="266mR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0805" value="2k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0805" value="750">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="resistor" package="C0805K" value="2n2">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="resistor" package="C0805K" value="2n2">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C7" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="Q1" library="transistor-fet" package="TO252" value="FDD4141TO252">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-fet" package="TO252" value="FDD4141TO252"/>
<element name="R7" library="rcl" package="R0805" value="20m">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0805" value="51">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="51">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="resistor" package="C0805K" value="1u">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="transistor-fet" package="TO252" value="FDD4141TO252">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="resistor" package="C0805K" value="1u">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0805" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0805" value="510">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0805" value="280">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0805" value="280">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="SMC_D" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="SMC_E" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="SMC_D" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="SMC_D" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="SMC_D" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SMB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SamacSys_Parts" package="SON65P300X300X100-9N" value="BQ29200DRBR">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="Voltage Protection with Automatic Cell Balance For 2-Cell Li-Ion Batteries, OVP=4.35V"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="BQ29200DRBR"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="Q5" library="SparkFun-DiscreteSemi" package="SOT23-3" value="5.8A/30V/35mΩ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-12988"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="SparkFun-DiscreteSemi" package="SOT23-3" value="4.3A/20V/54mΩ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-11153"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0805" value="280">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="resistor" package="C0805K" value="2n2">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="jumper" package="SJ_2" value=""/>
<element name="R17" library="rcl" package="R1206" value="280">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R1206" value="280">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R1206" value="280">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R1206" value="280">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="resistor" package="C0805K" value="2n2">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="resistor" package="C0805K" value="2n2">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="resistor" package="C0805K" value="2n2">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="SamacSys_Parts" package="SOP65P640X120-16N" value="INA260AIPW">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="High/Low-Side Digital Current/Power Monitor with Integrated 2m Shunt Resistor"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="INA260AIPW"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="IC4" library="SamacSys_Parts" package="SOT65P280X145-8N" value="INA219BIDCNT">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="INA219BIDCNT, Intelligent Power Switch High Side Current Shunt, Power Monitor, 0.01A, 5.5V, 8-Pin, SOT-23"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="INA219BIDCNT"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7300556P"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="IC5" library="SamacSys_Parts" package="SOT65P280X145-8N" value="INA219BIDCNT">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="INA219BIDCNT, Intelligent Power Switch High Side Current Shunt, Power Monitor, 0.01A, 5.5V, 8-Pin, SOT-23"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="INA219BIDCNT"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7300556P"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="R21" library="rcl" package="R0805" value="110m">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ4" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ5" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ6" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ7" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ8" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ9" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
</element>
<element name="C21" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="SamacSys_Parts" package="SOP65P780X200-20N" value="MCP23008-E_SS">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="8-Bit I/O Port Expander I2C 1.7M SSOP20 Microchip MCP23008-E/SS, 8-channel 8bit I/O Expander 1.7MHz, I2C, 20-Pin SSOP"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP23008-E/SS"/>
<attribute name="NAME"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="7709707"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="R28" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rcl" package="R1206" value="110m">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="SamacSys_Parts" package="5-PIN-TO-263(U)" value="MIC29302AWU_TR">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="LDO Reg Adj 1.24-15V 3A 6-Pin TO-263 Micrel MIC29302AWU TR, LDO Voltage Regulator, Adjustable 3A, 1.25  15 V 2%, 5-Pin TO-263"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Micrel"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MIC29302AWU TR"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value="8855990"/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="R33" library="rcl" package="R0805" value="110m">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="rcl" package="R0805" value="110m">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="R1206" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="SamacSys_Parts" package="5-PIN-TO-263(U)" value="LM2596S-12"/>
<element name="D2" library="diode" package="SMB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="R0805" value="110m">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="SMC_E" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="SMC_E" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="SMC_E" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="SMC_E" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ10" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ11" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="inductors" package="DR127" value="DR127">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="inductors" package="DR74" value="DR74"/>
<element name="R39" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ12" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="SMC_E" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="SMC_E" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rcl" package="SMC_E" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rcl" package="SMC_E" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD6" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD7" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD8" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD17" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD18" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD1" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD9" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD10" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD11" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD12" library="wirepad" package="3,81/1,4" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$28">
</signal>
<signal name="S$33">
</signal>
<signal name="S$39">
</signal>
<signal name="S$40">
</signal>
<signal name="S$60">
</signal>
<signal name="S$61">
</signal>
<signal name="S$213">
</signal>
<signal name="S$234">
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="CFG" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="K1" pad="9"/>
<contactref element="K1" pad="25"/>
<contactref element="K1" pad="39"/>
<contactref element="K1" pad="6"/>
<contactref element="K1" pad="14"/>
<contactref element="K1" pad="20"/>
<contactref element="K1" pad="30"/>
<contactref element="K1" pad="34"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="PS1" pad="29"/>
<contactref element="C9" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="PS1" pad="21"/>
<contactref element="C14" pad="-"/>
<contactref element="C10" pad="-"/>
<contactref element="C11" pad="-"/>
<contactref element="C12" pad="-"/>
<contactref element="C13" pad="-"/>
<contactref element="D1" pad="A"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="5"/>
<contactref element="C15" pad="2"/>
<contactref element="SJ3" pad="1"/>
<contactref element="Q6" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="11"/>
<contactref element="C19" pad="2"/>
<contactref element="SJ4" pad="1"/>
<contactref element="SJ5" pad="1"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC4" pad="3"/>
<contactref element="SJ9" pad="3"/>
<contactref element="SJ8" pad="3"/>
<contactref element="SJ7" pad="3"/>
<contactref element="SJ6" pad="3"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="IC6" pad="3"/>
<contactref element="IC6" pad="6"/>
<contactref element="IC7" pad="6"/>
<contactref element="IC7" pad="3"/>
<contactref element="D2" pad="A"/>
<contactref element="IC7" pad="5"/>
<contactref element="C25" pad="2"/>
<contactref element="C23" pad="-"/>
<contactref element="C24" pad="-"/>
<contactref element="C27" pad="-"/>
<contactref element="C26" pad="-"/>
<contactref element="C28" pad="2"/>
<contactref element="SJ10" pad="1"/>
<contactref element="SJ11" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="PS1" pad="17"/>
<contactref element="IC3" pad="9"/>
<contactref element="PS1" pad="11"/>
<contactref element="R39" pad="1"/>
<contactref element="R40" pad="1"/>
<contactref element="C30" pad="-"/>
<contactref element="C31" pad="-"/>
<contactref element="C32" pad="-"/>
<contactref element="C33" pad="-"/>
<contactref element="C34" pad="2"/>
<contactref element="PAD6" pad="1"/>
<contactref element="PAD18" pad="1"/>
<contactref element="PAD3" pad="1"/>
<contactref element="PAD4" pad="1"/>
<contactref element="PAD9" pad="1"/>
<contactref element="PAD10" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="U1" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="K1" pad="1"/>
<contactref element="K1" pad="17"/>
<contactref element="C22" pad="1"/>
<contactref element="IC2" pad="10"/>
<contactref element="C19" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="IC4" pad="4"/>
<contactref element="IC5" pad="4"/>
<contactref element="R26" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="R24" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="IC3" pad="20"/>
<contactref element="C29" pad="1"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="CFG" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="K1" pad="2"/>
<contactref element="K1" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="IC4" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="PAD5" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="K1" pad="3"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC4" pad="6"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="K1" pad="5"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="CLK_32KHZ">
<contactref element="K1" pad="29"/>
</signal>
<signal name="CLK_INT">
<contactref element="K1" pad="31"/>
</signal>
<signal name="CLK_RST">
<contactref element="K1" pad="33"/>
</signal>
<signal name="N$17">
<contactref element="K1" pad="28"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$23">
<contactref element="K1" pad="27"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="INTA">
<contactref element="K1" pad="37"/>
</signal>
<signal name="INTB">
<contactref element="K1" pad="38"/>
</signal>
<signal name="BATT">
<contactref element="Q3" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="C10" pad="+"/>
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="IC5" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="PS1" pad="16"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="PS1" pad="18"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="C4" pad="1"/>
<contactref element="PS1" pad="23"/>
</signal>
<signal name="EN">
<contactref element="PS1" pad="7"/>
<contactref element="SJ1" pad="2"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="SW">
<contactref element="C7" pad="1"/>
<contactref element="PS1" pad="26"/>
<contactref element="PS1" pad="25"/>
<contactref element="D1" pad="C"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="C7" pad="2"/>
<contactref element="PS1" pad="24"/>
</signal>
<signal name="N$10">
<contactref element="R4" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="PS1" pad="15"/>
<contactref element="Q1" pad="3"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="Q2" pad="3"/>
<contactref element="PS1" pad="28"/>
<contactref element="C8" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="C13" pad="+"/>
<contactref element="IC2" pad="14"/>
<contactref element="IC2" pad="15"/>
<contactref element="IC2" pad="16"/>
<contactref element="PAD11" pad="1"/>
<contactref element="PAD12" pad="1"/>
</signal>
<signal name="PIN">
<contactref element="Q2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="PS1" pad="27"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="C14" pad="+"/>
</signal>
<signal name="ACOK">
<contactref element="PS1" pad="3"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="SYS">
<contactref element="R7" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="C11" pad="+"/>
<contactref element="IC7" pad="1"/>
<contactref element="C12" pad="+"/>
<contactref element="C34" pad="1"/>
</signal>
<signal name="VREF33">
<contactref element="PS1" pad="5"/>
<contactref element="C9" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R10" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="PS1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="LED1" pad="A"/>
<contactref element="R12" pad="1"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="LED2" pad="A"/>
<contactref element="R13" pad="1"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="CHGOK">
<contactref element="PS1" pad="4"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$15">
<contactref element="PS1" pad="19"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="PS1" pad="20"/>
<contactref element="R14" pad="2"/>
<contactref element="PS1" pad="13"/>
</signal>
<signal name="RG2">
<contactref element="PS1" pad="14"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="RG1">
<contactref element="PS1" pad="9"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R16" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="6"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="Q5" pad="2"/>
<contactref element="Q6" pad="3"/>
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R19" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="PAD8" pad="1"/>
<contactref element="PAD17" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="IC1" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="IC1" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="Q6" pad="1"/>
<contactref element="Q5" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="4"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="BAT_12V">
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="12"/>
<contactref element="PAD2" pad="1"/>
<contactref element="PAD1" pad="1"/>
</signal>
<signal name="BATT_U_+">
<contactref element="Q5" pad="3"/>
<contactref element="R21" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="PAD7" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="IC2" pad="5"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="IC2" pad="4"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="SJ4" pad="3"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R23" pad="1"/>
<contactref element="SJ5" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="SJ9" pad="2"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="N$33">
<contactref element="SJ6" pad="2"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="N$34">
<contactref element="SJ8" pad="2"/>
<contactref element="IC5" pad="8"/>
</signal>
<signal name="N$35">
<contactref element="SJ7" pad="2"/>
<contactref element="IC5" pad="7"/>
</signal>
<signal name="VOUT_REG">
<contactref element="IC4" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="IC6" pad="4"/>
<contactref element="R33" pad="1"/>
<contactref element="R35" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C27" pad="+"/>
<contactref element="C26" pad="+"/>
<contactref element="C33" pad="+"/>
<contactref element="C32" pad="+"/>
</signal>
<signal name="N$30">
<contactref element="SJ7" pad="1"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="SJ8" pad="1"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="R24" pad="2"/>
<contactref element="SJ6" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="R25" pad="2"/>
<contactref element="SJ9" pad="1"/>
</signal>
<signal name="ACOK_IN">
<contactref element="R29" pad="1"/>
<contactref element="R31" pad="2"/>
<contactref element="IC3" pad="18"/>
</signal>
<signal name="CHGOK_IN">
<contactref element="R28" pad="1"/>
<contactref element="R30" pad="2"/>
<contactref element="IC3" pad="19"/>
</signal>
<signal name="CB_EN">
<contactref element="SJ3" pad="3"/>
<contactref element="IC3" pad="17"/>
</signal>
<signal name="ADJ">
<contactref element="IC6" pad="5"/>
<contactref element="R34" pad="1"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="VOUT">
<contactref element="IC6" pad="2"/>
<contactref element="R35" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C23" pad="+"/>
<contactref element="C24" pad="+"/>
<contactref element="L3" pad="2"/>
<contactref element="C30" pad="+"/>
<contactref element="C31" pad="+"/>
</signal>
<signal name="N$37">
<contactref element="IC7" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="IC7" pad="4"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="SJ10" pad="3"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="IC3" pad="4"/>
<contactref element="SJ10" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="IC3" pad="5"/>
<contactref element="SJ11" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="SJ11" pad="3"/>
<contactref element="R38" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC3" pad="16"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC3" pad="15"/>
<contactref element="SJ12" pad="1"/>
</signal>
<signal name="SHDN">
<contactref element="PS1" pad="8"/>
<contactref element="SJ12" pad="2"/>
<contactref element="R40" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
