<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="93.98" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="36.83" y2="0" width="0" layer="20"/>
<wire x1="36.83" y1="0" x2="38.1" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="38.1" y1="1.27" x2="38.1" y2="93.98" width="0" layer="20"/>
<wire x1="38.1" y1="93.98" x2="36.83" y2="95.25" width="0" layer="20" curve="90"/>
<wire x1="36.83" y1="95.25" x2="1.27" y2="95.25" width="0" layer="20"/>
<wire x1="1.27" y1="95.25" x2="0" y2="93.98" width="0" layer="20" curve="90"/>
<text>wadesherman/micromacro</text>
<text>2018-08-12</text>
<text>v1</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains footprints for SparkFun breakout boards, microcontrollers (Arduino, Particle, Teensy, etc.),  breadboards, non-RF modules, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SPARKFUN_PRO_MICRO">
<description>&lt;h3&gt;SparkFun Pro Mico Footprint (with USB connector)&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 24&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:0.7x1.3"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;SparkFun Pro Micro&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
</packages>
</library>
<library name="Wade-SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CHERRY-MX-LED">
<description>&lt;h3&gt;Cherry MX Switch - Electromechanical Swith w/ LED&lt;/h3&gt;

&lt;p&gt;Cherry MX Keyswitches are top-of-the-line mechanical keyboard switches. They’re satisfyingly “clicky”, reliable up to tens-of-millions of key presses, and a standard in gaming and programming keyboards across the globe. This ‘blue’ version Cherry MX Switch is favored by most due to its secondary internal actuator making it less likely to “double-tap.” If you are looking for a noticeably audible and high-quality key switch, this is the perfect option for you!&lt;/p&gt;

&lt;p&gt;&lt;a href="https://www.sparkfun.com/products/13834"&gt;SparkFun Product Link&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Components/Switches/MX%20Series.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="wade">
<packages>
<package name="BEAR">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B1" library="SparkFun-Boards" package="SPARKFUN_PRO_MICRO" value="SPARKFUN_PRO_MICRO"/>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="D4" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="D5" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="D6" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="D7" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="D8" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
</element>
<element name="S1" library="Wade-SparkFun-Switches" package="CHERRY-MX-LED" value="MOMENTARY-SWITCH-SPST-LED-PTH-CHERRY">
<attribute name="SF_ID" value="COM-13834"/>
</element>
<element name="S2" library="Wade-SparkFun-Switches" package="CHERRY-MX-LED" value="MOMENTARY-SWITCH-SPST-LED-PTH-CHERRY">
<attribute name="SF_ID" value="COM-13834"/>
</element>
<element name="S3" library="Wade-SparkFun-Switches" package="CHERRY-MX-LED" value="MOMENTARY-SWITCH-SPST-LED-PTH-CHERRY">
<attribute name="SF_ID" value="COM-13834"/>
</element>
<element name="S4" library="Wade-SparkFun-Switches" package="CHERRY-MX-LED" value="MOMENTARY-SWITCH-SPST-LED-PTH-CHERRY">
<attribute name="SF_ID" value="COM-13834"/>
</element>
<element name="S5" library="Wade-SparkFun-Switches" package="CHERRY-MX-LED" value="MOMENTARY-SWITCH-SPST-LED-PTH-CHERRY">
<attribute name="SF_ID" value="COM-13834"/>
</element>
<element name="S6" library="Wade-SparkFun-Switches" package="CHERRY-MX-LED" value="MOMENTARY-SWITCH-SPST-LED-PTH-CHERRY">
<attribute name="SF_ID" value="COM-13834"/>
</element>
<element name="S7" library="Wade-SparkFun-Switches" package="CHERRY-MX-LED" value="MOMENTARY-SWITCH-SPST-LED-PTH-CHERRY">
<attribute name="SF_ID" value="COM-13834"/>
</element>
<element name="S8" library="Wade-SparkFun-Switches" package="CHERRY-MX-LED" value="MOMENTARY-SWITCH-SPST-LED-PTH-CHERRY">
<attribute name="SF_ID" value="COM-13834"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
<element name="U$2" library="wade" package="BEAR" value=""/>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="R4" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="R5" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="R6" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="R7" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="R8" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value=""/>
<element name="R9" library="SparkFun-Passives" package="0603-RES" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="B1" pad="4"/>
<contactref element="B1" pad="23"/>
<contactref element="B1" pad="3"/>
<contactref element="S4" pad="K"/>
<contactref element="S3" pad="K"/>
<contactref element="S2" pad="K"/>
<contactref element="S1" pad="K"/>
<contactref element="S5" pad="K"/>
<contactref element="S6" pad="K"/>
<contactref element="S7" pad="K"/>
<contactref element="S8" pad="K"/>
</signal>
<signal name="RAW">
<contactref element="B1" pad="24"/>
</signal>
<signal name="VCC">
<contactref element="B1" pad="21"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="COL_1">
<contactref element="S4" pad="S1"/>
<contactref element="S1" pad="S1"/>
<contactref element="S2" pad="S1"/>
<contactref element="S3" pad="S1"/>
<contactref element="B1" pad="20"/>
</signal>
<signal name="COL_2">
<contactref element="S8" pad="S1"/>
<contactref element="S7" pad="S1"/>
<contactref element="S6" pad="S1"/>
<contactref element="S5" pad="S1"/>
<contactref element="B1" pad="19"/>
</signal>
<signal name="ROW_1">
<contactref element="D5" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="B1" pad="10"/>
</signal>
<signal name="ROW_2">
<contactref element="D6" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="B1" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="S1" pad="S2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="S2" pad="S2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="S3" pad="S2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="S4" pad="S2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="S5" pad="S2"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="S6" pad="S2"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="S7" pad="S2"/>
<contactref element="D7" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="S8" pad="S2"/>
<contactref element="D8" pad="A"/>
</signal>
<signal name="ROW_3">
<contactref element="D7" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="B1" pad="8"/>
</signal>
<signal name="ROW_4">
<contactref element="D8" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="B1" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="S1" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="S2" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="S3" pad="A"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="S4" pad="A"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="S5" pad="A"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="S6" pad="A"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="S7" pad="A"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="S8" pad="A"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="LED">
<contactref element="B1" pad="7"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="Q1" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="LED_POWER">
<contactref element="Q1" pad="3"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
