<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.5" y2="0" width="0" layer="20"/>
<wire x1="22.5" y1="0" x2="22.5" y2="15.5" width="0" layer="20"/>
<wire x1="22.5" y1="15.5" x2="0" y2="15.5" width="0" layer="20"/>
<wire x1="0" y1="15.5" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>V+</text>
<text>RF</text>
<text>RF+DC</text>
</plain>
<libraries>
<library name="newlib">
<packages>
<package name="CONSMA013.062-ND">
</package>
<package name="MOLEX0732512120">
</package>
<package name="PAD1.5X3">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="newlib" package="CONSMA013.062-ND" value="CONSMA013.062-ND"/>
<element name="U$2" library="newlib" package="MOLEX0732512120" value="MOLEX732512120"/>
<element name="U$3" library="newlib" package="PAD1.5X3" value="PAD1.5X3"/>
<element name="GND" library="newlib" package="PAD1.5X3" value="PAD1.5X3"/>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="1nF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0805" value="2.2uH"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="SIG"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="SIG"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="P$1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="GND@1"/>
<contactref element="U$2" pad="GND@2"/>
<contactref element="U$2" pad="GND@3"/>
<contactref element="U$2" pad="GND@4"/>
<contactref element="U$1" pad="GND@1"/>
<contactref element="U$1" pad="GND@2"/>
<contactref element="U$1" pad="GND@3"/>
<contactref element="U$1" pad="GND@4"/>
<contactref element="GND" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
