<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="8" x2="16" y2="8" width="0" layer="20" curve="-180"/>
<wire x1="16" y1="8" x2="0" y2="8" width="0" layer="20" curve="-180"/>
<text>&gt;VERSION</text>
<text>OMTEN-1288</text>
<text>16mm</text>
<text>&gt;VERSION</text>
</plain>
<libraries>
<library name="a_parts">
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
<package name="1X01_NOSILK_NOSTOP">
</package>
<package name="OMTEN-1288-LESS2-NS">
</package>
<package name="BATTCON_4.8MM">
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="LFPAK33">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOD323-SCHOTTKY">
</package>
<package name="SOT23-TIGHTER">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="VERSION" value="v1.1"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="a_parts" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="sean@yak.net"/>
<attribute name="VERSION" value="v1.1"/>
</element>
<element name="GND" library="a_parts" package="1X01_NOSILK_NOSTOP" value="M01NOT-A-VIA-NOPE"/>
<element name="SW1" library="a_parts" package="OMTEN-1288-LESS2-NS" value="SWITCH-SPSTOMTEN-1288-SMD-NS"/>
<element name="BAT1" library="a_parts" package="BATTCON_4.8MM" value=""/>
<element name="R1" library="a_parts" package="R0402" value="2K2">
<attribute name="NAME"/>
</element>
<element name="R2" library="a_parts" package="R0402" value="100R">
<attribute name="NAME"/>
</element>
<element name="R3" library="a_parts" package="R0402" value="1M">
<attribute name="NAME"/>
</element>
<element name="Q1" library="a_parts" package="LFPAK33" value="LFPAK33">
<attribute name="NAME"/>
</element>
<element name="C1" library="a_parts" package="C0402" value="1uF">
<attribute name="NAME"/>
</element>
<element name="D1" library="a_parts" package="SOD323-SCHOTTKY" value="">
<attribute name="NAME"/>
</element>
<element name="U1" library="a_parts" package="SOT23-TIGHTER" value="AP2210N">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="GND" pad="P$1"/>
<contactref element="Q1" pad="PAD"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="VBATT-">
<contactref element="BAT1" pad="-"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="COIN+">
<contactref element="BAT1" pad="A1"/>
<contactref element="SW1" pad="1"/>
<contactref element="BAT1" pad="A2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GATE">
<contactref element="R3" pad="2"/>
<contactref element="Q1" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="PULLUP">
<contactref element="SW1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="D1" pad="A"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="CHARGE+">
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
