<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="49.5175" y2="0" width="0" layer="20"/>
<wire x1="49.5175" y1="0" x2="49.5175" y2="63.49" width="0" layer="20"/>
<wire x1="49.5175" y1="63.49" x2="0" y2="63.49" width="0" layer="20"/>
<wire x1="0" y1="63.49" x2="0" y2="0" width="0" layer="20"/>
<text>1R</text>
<text>+5V</text>
<text>GND</text>
<text>Tx</text>
<text>Rx</text>
<text>Console</text>
<text>16 Rows</text>
<text>32 Rows</text>
<text>16x32 RGB LED Matrix</text>
<text>Macedon Engineering</text>
<text>Ver 1.2</text>
<text>Macedon Engineering</text>
<text>16x32 RGB LED Matrix</text>
<text>Ver 1.2</text>
<hole x="46.355" y="60.325" drill="3.2"/>
<hole x="46.355" y="3.175" drill="3.2"/>
<text>SDA</text>
<text>SDA</text>
<text>SCL</text>
<text>SCL</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>3.3V</text>
<text>5V</text>
<text>+5V</text>
<text>GND</text>
<text>+5V</text>
<text>GND</text>
<text>+5V</text>
<text>+5V</text>
<text>GND</text>
<text>GND</text>
<text>D16</text>
<text>D17</text>
<text>D4</text>
<text>3.3V</text>
<text>3.3V</text>
<text>D12</text>
<text>D13</text>
<text>A4</text>
<text>A5</text>
<text>GND</text>
<text>GND</text>
</plain>
<libraries>
<library name="me">
<packages>
<package name="LINKIT-DUO">
</package>
<package name="TERMINALBLOCK-5MM-2POS">
</package>
<package name="CAPPOL-4.5MM-ROUND">
</package>
<package name="SMT-1206-BOTTOM">
</package>
<package name="TSSOP8-B">
<description>&lt;b&gt;Plastic Small Outline&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X8">
</package>
<package name="1X03">
</package>
<package name="1X04">
</package>
<package name="1X02">
</package>
<package name="1X06">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="adafruit" package="C0603" value=".1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0603" value=".1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="C0603" value=".1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="me" package="LINKIT-DUO" value="LINKIT-DUO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="74xx-us" package="SO20W" value="74LS245DW">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="IC3" library="74xx-us" package="SO20W" value="74LS245DW">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X8" value="16Pin">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03" value="3Pin">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TB1" library="me" package="TERMINALBLOCK-5MM-2POS" value="TERMINALBLOCK-5MM-2POS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X03" value="3Pin">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="me" package="CAPPOL-4.5MM-ROUND" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X04" value="I2C">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X04" value="I2C">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TB2" library="me" package="TERMINALBLOCK-5MM-2POS" value="TERMINALBLOCK-5MM-2POS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X02" value="PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="me" package="SMT-1206-BOTTOM" value="2.2K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="me" package="SMT-1206-BOTTOM" value="2.2K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="me" package="SMT-1206-BOTTOM" value="2.2K"/>
<element name="R4" library="me" package="SMT-1206-BOTTOM" value="2.2K"/>
<element name="R5" library="me" package="SMT-1206-BOTTOM" value="100K"/>
<element name="IC4" library="me" package="TSSOP8-B" value="PCA9306-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X06" value="SPARES">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X06" value="SPARES">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC2" pad="10"/>
<contactref element="IC3" pad="10"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="16"/>
<contactref element="J2" pad="3"/>
<contactref element="IC1" pad="P$11"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="19"/>
<contactref element="IC3" pad="19"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="C1" pad="P$2"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC3" pad="2"/>
<contactref element="J5" pad="4"/>
<contactref element="J4" pad="4"/>
<contactref element="J6" pad="2"/>
<contactref element="TB2" pad="P$3"/>
<contactref element="TB2" pad="P$2"/>
<contactref element="TB1" pad="P$3"/>
<contactref element="TB1" pad="P$2"/>
<contactref element="IC4" pad="8"/>
<contactref element="J7" pad="6"/>
<contactref element="J8" pad="6"/>
<contactref element="J7" pad="5"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="P$15"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="P$16"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="A2">
<contactref element="IC1" pad="P$17"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="A3">
<contactref element="IC1" pad="P$18"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="D15">
<contactref element="IC1" pad="P$39"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="D8">
<contactref element="IC1" pad="P$28"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="D9">
<contactref element="IC1" pad="P$27"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="D10">
<contactref element="IC1" pad="P$26"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="D11">
<contactref element="IC1" pad="P$25"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="D5">
<contactref element="IC1" pad="P$31"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="D6">
<contactref element="IC1" pad="P$30"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="D7">
<contactref element="IC1" pad="P$29"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="D14">
<contactref element="IC1" pad="P$40"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="R1">
<contactref element="J1" pad="1"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="G1">
<contactref element="J1" pad="2"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="B1">
<contactref element="J1" pad="3"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="R2">
<contactref element="J1" pad="5"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="G2">
<contactref element="J1" pad="6"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="B2">
<contactref element="J1" pad="7"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="OE">
<contactref element="J1" pad="15"/>
<contactref element="IC3" pad="16"/>
</signal>
<signal name="A">
<contactref element="J1" pad="9"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="B">
<contactref element="J1" pad="10"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="C">
<contactref element="J1" pad="11"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="D">
<contactref element="J2" pad="1"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="CLK">
<contactref element="J1" pad="13"/>
<contactref element="IC3" pad="17"/>
</signal>
<signal name="LATCH">
<contactref element="J1" pad="14"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="P$10"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="P$9"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$1">
<contactref element="J1" pad="12"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$8">
<contactref element="J5" pad="2"/>
<contactref element="R4" pad="P$2"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="J5" pad="3"/>
<contactref element="R3" pad="P$2"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="J4" pad="2"/>
<contactref element="IC1" pad="P$33"/>
<contactref element="R1" pad="P$1"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="SDA">
<contactref element="J4" pad="3"/>
<contactref element="IC1" pad="P$34"/>
<contactref element="R2" pad="P$1"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="P$12"/>
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="J4" pad="1"/>
<contactref element="IC4" pad="7"/>
<contactref element="IC1" pad="P$21"/>
<contactref element="J8" pad="1"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="N$11">
</signal>
<signal name="N$7">
<contactref element="R5" pad="P$1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC2" pad="20"/>
<contactref element="IC3" pad="20"/>
<contactref element="TB1" pad="P$1"/>
<contactref element="TB1" pad="P$4"/>
<contactref element="IC1" pad="P$14"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="C1" pad="P$1"/>
<contactref element="TB2" pad="P$1"/>
<contactref element="TB2" pad="P$4"/>
<contactref element="J6" pad="1"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R4" pad="P$1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="J5" pad="1"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="D16">
<contactref element="IC1" pad="P$38"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="D17">
<contactref element="IC1" pad="P$37"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="D4">
<contactref element="IC1" pad="P$32"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="D12">
<contactref element="IC1" pad="P$24"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="D13">
<contactref element="IC1" pad="P$23"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="A4">
<contactref element="IC1" pad="P$19"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="A5">
<contactref element="IC1" pad="P$20"/>
<contactref element="J8" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
