<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<hole x="16.54018125" y="18.2241125" drill="3.2"/>
<hole x="16.24136875" y="77.910265625" drill="3.2"/>
<hole x="-37.53065" y="18.479928125" drill="3.2"/>
<text>Created by Brandon Satrom</text>
<text>Brew Buddy</text>
<hole x="-38.187975" y="78.298965625" drill="3.2"/>
<wire x1="-40.64" y1="81.28" x2="-40.64" y2="12.7" width="0.2032" layer="20"/>
<wire x1="-40.64" y1="12.7" x2="19.05" y2="12.7" width="0.2032" layer="20"/>
<wire x1="19.05" y1="12.7" x2="19.05" y2="81.28" width="0.2032" layer="20"/>
<wire x1="19.05" y1="81.28" x2="-40.64" y2="81.28" width="0.2032" layer="20"/>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>Brew Buddy</text>
</plain>
<libraries>
<library name="Adafruit_2.2_SPI_240x320">
<description>Generated from &lt;b&gt;Adafruit_2.2_SPI_240x320.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="MICROBUILDER_1X10_ROUND_2MM">
<description>1x10 2.0mm Header Pins</description>
</package>
</packages>
</library>
<library name="SparkFun_Thermocouple_Breakout">
<description>Generated from &lt;b&gt;SparkFun_Thermocouple_Breakout.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="1X06_LONGPADS">
</package>
</packages>
</library>
<library name="Particle-Mesh">
<packages>
<package name="FEATHERWING_SMT2">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="2.2TFT" library="Adafruit_2.2_SPI_240x320" package="MICROBUILDER_1X10_ROUND_2MM" value="TFT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MAX31855K" library="SparkFun_Thermocouple_Breakout" package="1X06_LONGPADS" value="6 Pad">
<attribute name="NAME"/>
</element>
<element name="MS1" library="Particle-Mesh" package="FEATHERWING_SMT2" value="FEATHERWING_SMTDUAL"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value=" 1M">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="KNOCK">
<attribute name="NAME"/>
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="TC_GND">
<contactref element="MAX31855K" pad="1"/>
<contactref element="MS1" pad="20"/>
<contactref element="MS1" pad="20'"/>
</signal>
<signal name="VCC">
<contactref element="MAX31855K" pad="2"/>
<contactref element="MS1" pad="22'"/>
<contactref element="MS1" pad="22"/>
</signal>
<signal name="SCK">
<contactref element="MAX31855K" pad="3"/>
<contactref element="MS1" pad="11"/>
<contactref element="MS1" pad="11'"/>
<contactref element="2.2TFT" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="MAX31855K" pad="4"/>
<contactref element="MS1" pad="13"/>
<contactref element="MS1" pad="13'"/>
<contactref element="2.2TFT" pad="8"/>
</signal>
<signal name="MOSI">
<contactref element="MAX31855K" pad="5"/>
<contactref element="MS1" pad="12'"/>
<contactref element="MS1" pad="12"/>
<contactref element="2.2TFT" pad="7"/>
</signal>
<signal name="TC_CS">
<contactref element="MAX31855K" pad="6"/>
<contactref element="MS1" pad="21"/>
<contactref element="MS1" pad="21'"/>
</signal>
<signal name="GND">
<contactref element="MS1" pad="4"/>
<contactref element="MS1" pad="4'"/>
<contactref element="2.2TFT" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="2.2TFT" pad="2"/>
<contactref element="MS1" pad="2'"/>
<contactref element="MS1" pad="2"/>
</signal>
<signal name="TFT_RST">
<contactref element="MS1" pad="5"/>
<contactref element="MS1" pad="5'"/>
<contactref element="2.2TFT" pad="4"/>
</signal>
<signal name="TFT_DC">
<contactref element="MS1" pad="6"/>
<contactref element="MS1" pad="6'"/>
<contactref element="2.2TFT" pad="3"/>
</signal>
<signal name="TFT_CS">
<contactref element="MS1" pad="7'"/>
<contactref element="MS1" pad="7"/>
<contactref element="2.2TFT" pad="6"/>
</signal>
<signal name="SD_CS">
<contactref element="2.2TFT" pad="5"/>
<contactref element="MS1" pad="19'"/>
<contactref element="MS1" pad="19"/>
</signal>
<signal name="KNOCK">
<contactref element="JP1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="MS1" pad="9"/>
<contactref element="MS1" pad="9'"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
