<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<circle x="31" y="32" radius="31" width="0.001" layer="20"/>
<circle x="15.844559375" y="23.25" radius="7" width="0.2" layer="20"/>
<circle x="46.155440625" y="23.25" radius="7" width="0.2" layer="20"/>
<circle x="31" y="49.5" radius="7" width="0.2" layer="20"/>
<text>A</text>
<text>B</text>
<text>C</text>
<text>D</text>
<text>E</text>
<text>F</text>
<text>G</text>
<text>H</text>
<text>I</text>
<text>J</text>
<text>K</text>
<text>L</text>
<wire x1="29" y1="59.71" x2="33" y2="59.71" width="0.2" layer="20"/>
<wire x1="29" y1="59.71" x2="29" y2="55" width="0.2" layer="20"/>
<wire x1="29" y1="55" x2="33" y2="55" width="0.2" layer="20"/>
<wire x1="33" y1="55" x2="33" y2="59.71" width="0.2" layer="20"/>
<text>B</text>
<text>C</text>
<text>A</text>
<text>D</text>
<text>E</text>
<text>F</text>
<text>G</text>
<text>I</text>
<text>H</text>
<text>J</text>
<text>K</text>
<text>L</text>
<text>NC</text>
<text>NC</text>
<text>UTM v1.0</text>
<text>FARM.BOT</text>
<text>OSHW</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
<description>&lt;h3&gt;Plated Through Hole - 2x4&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
</elements>
<signals>
<signal name="D">
<contactref element="J1" pad="1"/>
</signal>
<signal name="E">
<contactref element="J1" pad="3"/>
</signal>
<signal name="F">
<contactref element="J1" pad="5"/>
</signal>
<signal name="G">
<contactref element="J1" pad="7"/>
</signal>
<signal name="B">
<contactref element="J1" pad="2"/>
</signal>
<signal name="C">
<contactref element="J1" pad="4"/>
</signal>
<signal name="A">
<contactref element="J1" pad="6"/>
</signal>
<signal name="L">
<contactref element="J2" pad="1"/>
</signal>
<signal name="I">
<contactref element="J2" pad="3"/>
</signal>
<signal name="H">
<contactref element="J2" pad="5"/>
</signal>
<signal name="J">
<contactref element="J2" pad="4"/>
</signal>
<signal name="K">
<contactref element="J2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="8"/>
<contactref element="J2" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
