<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<circle x="40.64" y="40.64" radius="40.64" width="0.000253125" layer="20"/>
<text>-</text>
<text>+</text>
<hole x="19.05" y="24.892" drill="3.2"/>
<hole x="19.05" y="29.21" drill="3.2"/>
<hole x="61.976" y="29.21" drill="3.2"/>
<hole x="61.976" y="24.892" drill="3.2"/>
<hole x="14.478" y="29.21" drill="3.2"/>
<hole x="14.478" y="24.892" drill="3.2"/>
<hole x="66.548" y="29.21" drill="3.2"/>
<hole x="66.548" y="24.892" drill="3.2"/>
<text>+</text>
<text>-</text>
<text>10uF</text>
<text>REV B</text>
<text>Duncan Young</text>
<text>Fire Fly</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="1X02">
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X02_2.54_SCREWTERM">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="SparkFun" package="DIP08" value="ATTINY85">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="PIEZO" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistor" package="0204/7" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SparkFun" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="SparkFun" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="SparkFun" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="SparkFun" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="0207/2V" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="0204/7" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="0207/2V" value="150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH" value="POWER_JACKPTH">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-08352"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V" value="10uF">
<attribute name="NAME"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value="M022.54MM_SCREWTERM"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="PIEZO" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="J3" pad="P2"/>
</signal>
<signal name="PORTB">
<contactref element="IC1" pad="6"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="PORTA">
<contactref element="IC1" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="PWR"/>
<contactref element="J2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="J3" pad="P1"/>
</signal>
<signal name="PORTC">
<contactref element="IC1" pad="7"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="PIEZO">
<contactref element="PIEZO" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED3" pad="K"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED5" pad="K"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="LED4" pad="K"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED6" pad="K"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
