<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="-5" y1="14.25" x2="-5" y2="21" width="0.3" layer="20"/>
<wire x1="-5" y1="-21" x2="-5" y2="-14.25" width="0.3" layer="20"/>
<wire x1="-5" y1="-14.25" x2="5" y2="-14.25" width="0.3" layer="20"/>
<wire x1="5" y1="-14.25" x2="5" y2="-21" width="0.3" layer="20"/>
<wire x1="5" y1="21" x2="5" y2="14.25" width="0.3" layer="20"/>
<wire x1="5" y1="14.25" x2="-5" y2="14.25" width="0.3" layer="20"/>
<wire x1="-5" y1="-21" x2="-21.5" y2="0" width="0.1524" layer="20" curve="-76.607502"/>
<wire x1="-21.5" y1="0" x2="-5" y2="21" width="0.1524" layer="20" curve="-76.607502"/>
<wire x1="5" y1="21" x2="21.5" y2="0" width="0.1524" layer="20" curve="-76.607502"/>
<wire x1="21.5" y1="0" x2="5" y2="-21" width="0.1524" layer="20" curve="-76.607502"/>
</plain>
<libraries>
<library name="BlueForsCoaxProbe2">
<packages>
<package name="MILLMAX6">
</package>
<package name="MILLMAX4">
</package>
</packages>
</library>
<library name="con-dil">
<description>&lt;b&gt;DIL Ribbon Cable Connectors&lt;/b&gt;&lt;p&gt;
Based on Harting material.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="16P">
<description>&lt;b&gt;DIL CABLE CONNECTOR&lt;/b&gt;</description>
</package>
<package name="8P_HALF">
</package>
</packages>
</library>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="BU-SMA-V-PER">
</package>
<package name="SMA-HALF">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="BlueForsCoaxProbe2" package="MILLMAX6" value="MILLMAX6"/>
<element name="U$2" library="BlueForsCoaxProbe2" package="MILLMAX6" value="MILLMAX6"/>
<element name="SV1" library="con-dil" package="16P" value="">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="X" library="con-coax" package="BU-SMA-V-PER" value="BU-SMA-V-PER">
<attribute name="NAME"/>
</element>
<element name="Z" library="con-coax" package="BU-SMA-V-PER" value="BU-SMA-V-PER">
<attribute name="NAME"/>
</element>
<element name="Y" library="con-coax" package="BU-SMA-V-PER" value="BU-SMA-V-PER">
<attribute name="NAME"/>
</element>
<element name="15K" library="SparkFun-Capacitors" package="0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-Capacitors" package="0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RB" library="SparkFun-Capacitors" package="0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CBIAS" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MW" library="con-coax" package="SMA-HALF" value="SMA-HALF">
<attribute name="NAME"/>
</element>
<element name="U$4" library="con-dil" package="8P_HALF" value="8P_HALF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="BlueForsCoaxProbe2" package="MILLMAX4" value="MILLMAX4"/>
<element name="C9" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X04_1.27MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1M" library="SparkFun-Resistors" package="0603" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="Y" pad="3"/>
<contactref element="Y" pad="2"/>
<contactref element="Y" pad="5"/>
<contactref element="Y" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="X" pad="2"/>
<contactref element="X" pad="3"/>
<contactref element="X" pad="5"/>
<contactref element="X" pad="4"/>
<contactref element="MW" pad="2"/>
<contactref element="MW" pad="3"/>
<contactref element="U$4" pad="3"/>
<contactref element="Z" pad="2"/>
<contactref element="Z" pad="3"/>
<contactref element="Z" pad="5"/>
<contactref element="Z" pad="4"/>
<contactref element="SV1" pad="5"/>
<contactref element="SV1" pad="3"/>
<contactref element="MW" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="C5" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="SV1" pad="16"/>
<contactref element="SV1" pad="12"/>
<contactref element="SV1" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="Y" pad="1"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="P$6"/>
<contactref element="RB" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="X" pad="1"/>
<contactref element="CBIAS" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="CBIAS" pad="2"/>
<contactref element="RB" pad="2"/>
<contactref element="SV1" pad="14"/>
</signal>
<signal name="N$12">
<contactref element="SV1" pad="7"/>
<contactref element="U$4" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="SV1" pad="2"/>
<contactref element="SV1" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U$5" pad="P$4"/>
</signal>
<signal name="N$14">
<contactref element="U$4" pad="7"/>
<contactref element="C8" pad="1"/>
<contactref element="U$5" pad="P$3"/>
</signal>
<signal name="N$15">
<contactref element="U$2" pad="P$4"/>
<contactref element="C9" pad="1"/>
<contactref element="SV1" pad="10"/>
</signal>
<signal name="N$4">
<contactref element="C5" pad="1"/>
<contactref element="D1" pad="2"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="C2" pad="2"/>
<contactref element="SV1" pad="11"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="P$5"/>
<contactref element="C6" pad="1"/>
<contactref element="SV1" pad="13"/>
</signal>
<signal name="N$7">
<contactref element="C3" pad="1"/>
<contactref element="U$1" pad="P$6"/>
<contactref element="SV1" pad="15"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$2"/>
<contactref element="15K" pad="1"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="C10" pad="1"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="1M" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="15K" pad="2"/>
<contactref element="U$4" pad="5"/>
<contactref element="Z" pad="1"/>
<contactref element="1M" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="1"/>
<contactref element="U$2" pad="P$5"/>
</signal>
<signal name="N$16">
<contactref element="J1" pad="2"/>
<contactref element="U$2" pad="P$3"/>
</signal>
<signal name="N$18">
<contactref element="J1" pad="3"/>
<contactref element="U$2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
