<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21.26" y2="0" width="0" layer="20"/>
<wire x1="21.26" y1="0" x2="21.26" y2="85.08" width="0" layer="20"/>
<wire x1="21.26" y1="85.08" x2="0" y2="85.08" width="0" layer="20"/>
<wire x1="0" y1="85.08" x2="0" y2="0" width="0" layer="20"/>
<hole x="11.43" y="3.81" drill="1.4"/>
<hole x="11.43" y="20.32" drill="1.4"/>
<text>S</text>
<text>G</text>
<text>D</text>
<text>EWB Austin Petrifilm Incubator V0.1</text>
<text>by Robert L. Read</text>
<text>GND</text>
<text>T1</text>
<text>T2</text>
<text>T3</text>
<text>T4</text>
<text>+5V</text>
<text>- FROM HEAT</text>
<text>MOSFET
CTL</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_ROUND">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TEMP1" library="adafruit" package="1X03" value=""/>
<element name="TEMP2" library="adafruit" package="1X03" value=""/>
<element name="TEMP3" library="adafruit" package="1X03" value=""/>
<element name="TEMP4" library="adafruit" package="1X03" value=""/>
<element name="JP1" library="SparkFun-Connectors" package="1X08_ROUND" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.6" value="10K Ohm"/>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="FRAME2" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER">
<attribute name="TITLE" value="Petriflm"/>
</element>
<element name="TEMP5" library="adafruit" package="1X03" value="MOSFET"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="TEMP4" pad="3"/>
<contactref element="TEMP3" pad="3"/>
<contactref element="TEMP2" pad="3"/>
<contactref element="TEMP1" pad="3"/>
<contactref element="R1" pad="P$1"/>
<contactref element="TEMP5" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="7"/>
<contactref element="TEMP4" pad="1"/>
<contactref element="TEMP3" pad="1"/>
<contactref element="TEMP2" pad="1"/>
<contactref element="TEMP1" pad="1"/>
<contactref element="JP1" pad="8"/>
<contactref element="TEMP5" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="2"/>
<contactref element="TEMP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="3"/>
<contactref element="TEMP2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="4"/>
<contactref element="TEMP3" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="5"/>
<contactref element="TEMP4" pad="2"/>
</signal>
<signal name="MOSFET">
<contactref element="JP1" pad="6"/>
<contactref element="R1" pad="P$2"/>
<contactref element="TEMP5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
