<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="66.04" y1="52.2732" x2="66.04" y2="70.231" width="0" layer="20"/>
<wire x1="83.8454" y1="70.231" x2="83.8454" y2="52.2732" width="0" layer="20"/>
<wire x1="83.8454" y1="52.2732" x2="66.04" y2="52.2732" width="0" layer="20"/>
<text>FF MJK 13</text>
<text>G</text>
<text>c</text>
<text>c</text>
<text>B</text>
<text>B</text>
<text>e</text>
<text>e</text>
</plain>
<libraries>
<library name="gm-trans">
<description>&lt;b&gt;Transistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;small signal amps (e.g., 2N508x)
&lt;li&gt;switching transistors (e.g., 2N2222, 2N390x)
&lt;li&gt;JFETs (e.g., J201, 2N3819, 2N5457)
&lt;li&gt;MOSFETs (e.g., BS170, BS250)
&lt;li&gt;mostly copied from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="TO92-">
</package>
</packages>
</library>
<library name="gm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="gm-caps-film-box">
<description>&lt;b&gt;Capacitors, Film, Box&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;1000pF - 2.2uF  (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors because they are small
&lt;li&gt;these have short leads so that pad spacing equals lead spacing
&lt;li&gt;e.g., WIMA capacitors
&lt;/ul&gt;</description>
<packages>
<package name="072X025">
<description>&lt;b&gt;7.2mm x 2.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKS2, MKP2</description>
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="ROUND">
<description>&lt;b&gt;Round Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="gm-trans" package="TO92-" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="Q2" library="gm-trans" package="TO92-" value="2N5088">
<attribute name="NAME"/>
</element>
<element name="33K" library="gm-resistors" package="R0207/3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="330" library="gm-resistors" package="R0207/3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="100K" library="gm-resistors" package="R0207/3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name=".01" library="gm-caps-film-box" package="072X025" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2.2" library="gm-caps-electro-pol" package="050_020_1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V1" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="B1" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="B2" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="GND" library="gm-supply" package="ROUND" value=""/>
<element name="F1" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="IN" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="9V" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="F2" library="gm-supply" package="ROUND" value="">
<attribute name="NAME"/>
</element>
<element name="22" library="gm-caps-electro-pol" package="050_020_1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND1" library="gm-supply" package="ROUND" value=""/>
<element name="9V1" library="gm-supply" package="ROUND" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="33K" pad="1"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="33K" pad="2"/>
<contactref element="330" pad="2"/>
<contactref element="9V" pad="1"/>
<contactref element="9V" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="330" pad="1"/>
<contactref element=".01" pad="1"/>
<contactref element="B1" pad="1"/>
<contactref element="B1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="2.2" pad="+"/>
<contactref element="Q1" pad="2"/>
<contactref element="100K" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="100K" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element=".01" pad="2"/>
<contactref element="V1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="Q2" pad="1"/>
<contactref element="B2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="3"/>
<contactref element="GND" pad="1"/>
<contactref element="22" pad="-"/>
</signal>
<signal name="N$9">
<contactref element="2.2" pad="-"/>
<contactref element="IN" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="F2" pad="1"/>
<contactref element="22" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
