<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="53.518" y2="0" width="0" layer="20"/>
<wire x1="53.518" y1="0" x2="53.518" y2="46.98" width="0" layer="20"/>
<wire x1="53.518" y1="46.98" x2="1.27" y2="46.98" width="0" layer="20"/>
<wire x1="1.27" y1="46.98" x2="1.27" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="Murata_NMG1205SC">
<packages>
<package name="NMG1205SC">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUEMILANOVE_VIAS">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2021">
<description>.100" (2.54mm) Center Headers - 2 Pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value=""/>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D4" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D5" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D6" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D7" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="D8" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="DC/DC_CONVERTER" library="Murata_NMG1205SC" package="NMG1205SC" value="12/5"/>
<element name="G_LED" library="SparkFun-LED" package="LED-0603" value="12V"/>
<element name="R_LED" library="SparkFun-LED" package="LED-0603" value="5V"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="3k3"/>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="1k"/>
<element name="T1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-11480"/>
</element>
<element name="T2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-11480"/>
</element>
<element name="T3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-11480"/>
</element>
<element name="T4" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-11480"/>
</element>
<element name="T5" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-11480"/>
</element>
<element name="T6" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-11480"/>
</element>
<element name="T7" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-11480"/>
</element>
<element name="T8" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="PROD_ID" value="TRANS-11480"/>
</element>
<element name="U1" library="SparkFun-Boards" package="DUEMILANOVE_VIAS" value="ARDUINO_SHIELDNO_SILK"/>
<element name="X1" library="con-molex" package="22-23-2021" value="12V IN">
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
<element name="M3" library="con-molex" package="22-23-2021" value="M2">
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
<element name="M6" library="con-molex" package="22-23-2021" value="M5">
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
<element name="M10" library="con-molex" package="22-23-2021" value="M8">
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
<element name="M2" library="con-molex" package="22-23-2021" value="M1">
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
<element name="M5" library="con-molex" package="22-23-2021" value="M4">
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
<element name="M9" library="con-molex" package="22-23-2021" value="M7">
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
<element name="M4" library="con-molex" package="22-23-2021" value="M3">
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
<element name="M7" library="con-molex" package="22-23-2021" value="M6">
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="OC_NEWARK" value="25C3832"/>
</element>
</elements>
<signals>
<signal name="12V">
<contactref element="DC/DC_CONVERTER" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="VIN"/>
</signal>
<signal name="GND">
<contactref element="DC/DC_CONVERTER" pad="2"/>
<contactref element="DC/DC_CONVERTER" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="G_LED" pad="C"/>
<contactref element="R_LED" pad="C"/>
<contactref element="U1" pad="GND@2"/>
<contactref element="U1" pad="GND@1"/>
<contactref element="U1" pad="GND@0"/>
<contactref element="T2" pad="2"/>
<contactref element="T3" pad="2"/>
<contactref element="T4" pad="2"/>
<contactref element="T8" pad="2"/>
<contactref element="T7" pad="2"/>
<contactref element="T6" pad="2"/>
<contactref element="T5" pad="2"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="5V">
<contactref element="DC/DC_CONVERTER" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="M3" pad="1"/>
<contactref element="M5" pad="1"/>
<contactref element="M6" pad="1"/>
<contactref element="M9" pad="1"/>
<contactref element="M10" pad="1"/>
<contactref element="M2" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="C"/>
<contactref element="D7" pad="C"/>
<contactref element="D8" pad="C"/>
<contactref element="M4" pad="1"/>
<contactref element="M7" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="G_LED" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="2"/>
<contactref element="R_LED" pad="A"/>
</signal>
<signal name="IO1">
<contactref element="U1" pad="D2"/>
<contactref element="T6" pad="1"/>
</signal>
<signal name="PWM1">
<contactref element="U1" pad="D3"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="IO2">
<contactref element="U1" pad="D4"/>
<contactref element="T7" pad="1"/>
</signal>
<signal name="PWM2">
<contactref element="U1" pad="D5"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="PWM3">
<contactref element="U1" pad="D6"/>
<contactref element="T3" pad="1"/>
</signal>
<signal name="IO3">
<contactref element="U1" pad="D7"/>
<contactref element="T8" pad="1"/>
</signal>
<signal name="PWM4">
<contactref element="U1" pad="D9"/>
<contactref element="T4" pad="1"/>
</signal>
<signal name="PWM5">
<contactref element="U1" pad="D10"/>
<contactref element="T5" pad="1"/>
</signal>
<signal name="T1">
<contactref element="M3" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="T2">
<contactref element="M5" pad="2"/>
<contactref element="T2" pad="3"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="T3">
<contactref element="M6" pad="2"/>
<contactref element="T3" pad="3"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="T4">
<contactref element="M9" pad="2"/>
<contactref element="D4" pad="A"/>
<contactref element="T4" pad="3"/>
</signal>
<signal name="T5">
<contactref element="M10" pad="2"/>
<contactref element="T5" pad="3"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="T6">
<contactref element="M2" pad="2"/>
<contactref element="D6" pad="A"/>
<contactref element="T6" pad="3"/>
</signal>
<signal name="T8">
<contactref element="T8" pad="3"/>
<contactref element="D8" pad="A"/>
<contactref element="M7" pad="2"/>
</signal>
<signal name="T7">
<contactref element="T7" pad="3"/>
<contactref element="D7" pad="A"/>
<contactref element="M4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
