<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="20.32" y1="30.48" x2="30.48" y2="30.48" width="0" layer="20"/>
<wire x1="30.48" y1="30.48" x2="30.48" y2="20.32" width="0" layer="20"/>
<wire x1="30.48" y1="20.32" x2="20.32" y2="20.32" width="0" layer="20"/>
<wire x1="20.32" y1="20.32" x2="20.32" y2="30.48" width="0" layer="20"/>
<text>PCA9617A</text>
<text>v1</text>
<text>11Aug16</text>
</plain>
<libraries>
<library name="KEMET">
<packages>
<package name="0805_B">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK_ALL_ROUND">
</package>
</packages>
</library>
<library name="ERIC">
<description>CDS Photoconductive Photocell.
PDV-P7002
Digikey part PDV-P7002-ND</description>
<packages>
<package name="MSOP_8_LEAD">
<description>Based off of Microchip packaging document. with of pads geometric mean of largest and smallest. Pad extends beyond largest width by 0.03, while centered on 2.2mm&lt;br&gt;
70% cream coverage</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="KEMET" package="0805_B" value=""/>
<element name="C2" library="KEMET" package="0805_B" value=""/>
<element name="J1" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="ERIC" package="MSOP_8_LEAD" value="PCA9617A"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="J1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="5"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="6"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="7"/>
<contactref element="J2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
