<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0.5" y1="0.5" x2="41.9" y2="0.5" width="0" layer="20" grouprefs="PCB"/>
<wire x1="41.9" y1="0.5" x2="41.9" y2="47.6" width="0" layer="20" grouprefs="PCB"/>
<wire x1="41.9" y1="47.6" x2="0.5" y2="47.6" width="0" layer="20" grouprefs="PCB"/>
<wire x1="0.5" y1="47.6" x2="0.5" y2="0.5" width="0" layer="20" grouprefs="PCB"/>
<text>PCT2075DP</text>
<text>Thomas Snyder 2020</text>
<text>Sensor Processing Board Rev 4.0</text>
</plain>
<libraries>
<library name="con-JST SH">
<description>
&lt;b&gt;JST Connectors&lt;/b&gt; - SH Series, 1.00mm pitch disconnectable crimp style connectors&lt;p&gt;

&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;

&lt;author&gt;Author: kylie &lt;/author&gt;, 04/2018&lt;p&gt;

&lt;a href="http://www.jst-mfg.com/product/detail_e.php?series=231"&gt;
&lt;img src="http://www.jst-mfg.com/product/images/pict/sh.jpg"  &gt;&lt;/a&gt;&lt;p&gt;
&lt;a href="http://www.jst-mfg.com/product/pdf/eng/eSH.pdf"&gt; Data sheet (PDF)&lt;/a&gt;&lt;p&gt;
&lt;p&gt; similar to:&lt;p&gt;
</description>
<packages>
<package name="BM06B-SRSS-TB">
<description>

&lt;b&gt;JST SH series header&lt;/b&gt; 1.00mm pitch disconnectable crimp style connectors, SMT vertical (top entry type), 6 pins&lt;p&gt;

</description>
</package>
</packages>
</library>
<library name="BG125-04-A-1-1-0420-N-C-BOTTOM">
<packages>
<package name="GCT_BG125-04-A-1-1-0420-N-C-BOTTOM">
</package>
</packages>
</library>
<library name="BG125-02-A-1-1-0440-N-C-BOTTOM (1)">
<packages>
<package name="GCT_BG125-02-A-1-1-0440-N-C-BOTTOM">
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="STM32H743VIT6">
<packages>
<package name="QFP50P1600X1600X160-100N">
</package>
</packages>
</library>
<library name="SM04B-SRSS-TB_LF__SN_">
<description>JST-SH 4pos 1mm pitch</description>
<packages>
<package name="JST_SM04B-SRSS-TB(LF)(SN)">
</package>
</packages>
</library>
<library name="microSDslot">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="503398-1892">
<description>&lt;b&gt;503398-1892&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="IPT1-110-01-L-D-RA">
<packages>
<package name="SAMTEC_IPT1-110-01-L-D-RA">
</package>
</packages>
</library>
<library name="PCT2075">
<packages>
<package name="PCT2075D-TSSOP8">
<description>A TSSOP-8 Footprint</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP15R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="DMG1012UW-7">
<packages>
<package name="SOT323">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="VIN" library="BG125-04-A-1-1-0420-N-C-BOTTOM" package="GCT_BG125-04-A-1-1-0420-N-C-BOTTOM" value="BG125-04-A-1-1-0420-N-C-BOTTOM">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" "/>
<attribute name="MF" value="Global Connector Technology"/>
<attribute name="MP" value="BG125-04-A-1-1-0420-N-C"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="MN_RST" library="BG125-02-A-1-1-0440-N-C-BOTTOM (1)" package="GCT_BG125-02-A-1-1-0440-N-C-BOTTOM" value="BG125-02-A-1-1-0440-N-C-BOTTOM">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" BG125 - 2.54mm pitch Socket Board to Board Connector "/>
<attribute name="MF" value="Global Connector Technology"/>
<attribute name="MP" value="BG125-02-A-1-1-0440-N-C"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="GND" library="BG125-02-A-1-1-0440-N-C-BOTTOM (1)" package="GCT_BG125-02-A-1-1-0440-N-C-BOTTOM" value="BG125-02-A-1-1-0440-N-C-BOTTOM">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" BG125 - 2.54mm pitch Socket Board to Board Connector "/>
<attribute name="MF" value="Global Connector Technology"/>
<attribute name="MP" value="BG125-02-A-1-1-0440-N-C"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="CHRG" library="BG125-02-A-1-1-0440-N-C-BOTTOM (1)" package="GCT_BG125-02-A-1-1-0440-N-C-BOTTOM" value="BG125-02-A-1-1-0440-N-C-BOTTOM">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" BG125 - 2.54mm pitch Socket Board to Board Connector "/>
<attribute name="MF" value="Global Connector Technology"/>
<attribute name="MP" value="BG125-02-A-1-1-0440-N-C"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="I2C" library="BG125-02-A-1-1-0440-N-C-BOTTOM (1)" package="GCT_BG125-02-A-1-1-0440-N-C-BOTTOM" value="BG125-02-A-1-1-0440-N-C-BOTTOM">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" BG125 - 2.54mm pitch Socket Board to Board Connector "/>
<attribute name="MF" value="Global Connector Technology"/>
<attribute name="MP" value="BG125-02-A-1-1-0440-N-C"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="PROGRAMMER" library="con-JST SH" package="BM06B-SRSS-TB" value="BM06B-SRSS-TB">
<attribute name="NAME"/>
</element>
<element name="U2" library="STM32H743VIT6" package="QFP50P1600X1600X160-100N" value="STM32H743VIT6">
<attribute name="AVAILABILITY" value="Warning"/>
<attribute name="DESCRIPTION" value=" ARM® Cortex®-M7 STM32H7 Microcontroller IC 32-Bit 480MHz 2MB (2M x 8) FLASH 100-LQFP (14x14) "/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MP" value="STM32H743VIT6"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="LQFP-100 STMicroelectronics"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/STM32H743VIT6/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SM04B-SRSS-TB_LF__SN_" package="JST_SM04B-SRSS-TB(LF)(SN)" value="SM04B-SRSS-TB(LF)(SN)">
<attribute name="DESCRIPTION" value=" Connector Header Surface Mount, Right Angle 4 position 0.039 (1.00mm) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="455-1804-1-ND"/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="SM04B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SM04B-SRSS-TB(LF)(SN)/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SM04B-SRSS-TB_LF__SN_" package="JST_SM04B-SRSS-TB(LF)(SN)" value="SM04B-SRSS-TB(LF)(SN)">
<attribute name="DESCRIPTION" value=" Connector Header Surface Mount, Right Angle 4 position 0.039 (1.00mm) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="455-1804-1-ND"/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="SM04B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SM04B-SRSS-TB(LF)(SN)/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SM04B-SRSS-TB_LF__SN_" package="JST_SM04B-SRSS-TB(LF)(SN)" value="SM04B-SRSS-TB(LF)(SN)">
<attribute name="DESCRIPTION" value=" Connector Header Surface Mount, Right Angle 4 position 0.039 (1.00mm) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="455-1804-1-ND"/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="SM04B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SM04B-SRSS-TB(LF)(SN)/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SM04B-SRSS-TB_LF__SN_" package="JST_SM04B-SRSS-TB(LF)(SN)" value="SM04B-SRSS-TB(LF)(SN)">
<attribute name="DESCRIPTION" value=" Connector Header Surface Mount, Right Angle 4 position 0.039 (1.00mm) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="455-1804-1-ND"/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="SM04B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SM04B-SRSS-TB(LF)(SN)/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SM04B-SRSS-TB_LF__SN_" package="JST_SM04B-SRSS-TB(LF)(SN)" value="SM04B-SRSS-TB(LF)(SN)">
<attribute name="DESCRIPTION" value=" Connector Header Surface Mount, Right Angle 4 position 0.039 (1.00mm) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="455-1804-1-ND"/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="SM04B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SM04B-SRSS-TB(LF)(SN)/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="microSDslot" package="503398-1892" value="503398-1892">
<attribute name="DESCRIPTION" value="MicroSD SMT Push-Push 1.28mm height MicroSD SMT Push-Push 1.28mm height"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="503398-1892"/>
<attribute name="MOUSER_PART_NUMBER" value="538-503398-1892"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Molex/503398-1892?qs=b0v8CoHHvSMxV%252BW12iKaSg%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SM04B-SRSS-TB_LF__SN_" package="JST_SM04B-SRSS-TB(LF)(SN)" value="SM04B-SRSS-TB(LF)(SN)">
<attribute name="DESCRIPTION" value=" Connector Header Surface Mount, Right Angle 4 position 0.039 (1.00mm) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="455-1804-1-ND"/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="SM04B-SRSS-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/SM04B-SRSS-TB(LF)(SN)/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="IPT1-110-01-L-D-RA" package="SAMTEC_IPT1-110-01-L-D-RA" value="IPT1-110-01-L-D-RA">
<attribute name="DESCRIPTION" value=" Connector Header Through Hole, Right Angle 20 position 0.100 (2.54mm) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="IPT1-110-01-L-D-RA-FL-ND"/>
<attribute name="MF" value="Samtec Inc."/>
<attribute name="MP" value="IPT1-110-01-L-D-RA"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/IPT1-110-01-L-D-RA/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0805" value="0.01 uf">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="63"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0805" value="0.01u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="63"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0805" value="0.01u">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="63"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="PCT2075" package="PCT2075D-TSSOP8" value="PCT2075D"/>
<element name="R7" library="rcl" package="R0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP11" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP12" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP13" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP14" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP15" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP18" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP19" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP20" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP21" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP22" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP23" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP24" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP25" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP26" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP16" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP17" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP27" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP28" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP29" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP30" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP31" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP32" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP33" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP34" library="testpad" package="TP15R" value="TPTP15R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="DMG1012UW-7" package="SOT323" value="DMG1012UW-7">
<attribute name="DESCRIPTION" value=" N-Channel 20V 1A (Ta) 290mW (Ta) Surface Mount SOT-323 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="DMG1012UW-7DICT-ND"/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMG1012UW-7"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-323 Diodes Inc."/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMG1012UW-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="DMG1012UW-7" package="SOT323" value="DMG1012UW-7">
<attribute name="DESCRIPTION" value=" N-Channel 20V 1A (Ta) 290mW (Ta) Surface Mount SOT-323 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="DMG1012UW-7DICT-ND"/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMG1012UW-7"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-323 Diodes Inc."/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMG1012UW-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="DMG1012UW-7" package="SOT323" value="DMG1012UW-7">
<attribute name="DESCRIPTION" value=" N-Channel 20V 1A (Ta) 290mW (Ta) Surface Mount SOT-323 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="DMG1012UW-7DICT-ND"/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMG1012UW-7"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-323 Diodes Inc."/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMG1012UW-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="DMG1012UW-7" package="SOT323" value="DMG1012UW-7">
<attribute name="DESCRIPTION" value=" N-Channel 20V 1A (Ta) 290mW (Ta) Surface Mount SOT-323 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="DMG1012UW-7DICT-ND"/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMG1012UW-7"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-323 Diodes Inc."/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMG1012UW-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="DMG1012UW-7" package="SOT323" value="DMG1012UW-7">
<attribute name="DESCRIPTION" value=" N-Channel 20V 1A (Ta) 290mW (Ta) Surface Mount SOT-323 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="DMG1012UW-7DICT-ND"/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMG1012UW-7"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-323 Diodes Inc."/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMG1012UW-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="DMG1012UW-7" package="SOT323" value="DMG1012UW-7">
<attribute name="DESCRIPTION" value=" N-Channel 20V 1A (Ta) 290mW (Ta) Surface Mount SOT-323 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="DMG1012UW-7DICT-ND"/>
<attribute name="MF" value="Diodes Inc."/>
<attribute name="MP" value="DMG1012UW-7"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-323 Diodes Inc."/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/DMG1012UW-7/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0805" value=""/>
<element name="D2" library="SparkFun-LED" package="LED-0805" value=""/>
<element name="R22" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="85"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="U2" pad="20"/>
<contactref element="U2" pad="27"/>
<contactref element="U2" pad="11"/>
<contactref element="U2" pad="50"/>
<contactref element="U2" pad="75"/>
<contactref element="U2" pad="100"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="J10" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="VIN" pad="4"/>
<contactref element="PROGRAMMER" pad="5"/>
<contactref element="U2" pad="21"/>
<contactref element="J7" pad="01"/>
<contactref element="R6" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="TP3" pad="TP"/>
<contactref element="J10" pad="9"/>
<contactref element="J1" pad="4"/>
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="4"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="GND">
<contactref element="VIN" pad="2"/>
<contactref element="PROGRAMMER" pad="6"/>
<contactref element="U2" pad="19"/>
<contactref element="U2" pad="26"/>
<contactref element="U2" pad="74"/>
<contactref element="U2" pad="99"/>
<contactref element="U2" pad="10"/>
<contactref element="U2" pad="49"/>
<contactref element="GND" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="CHRG" pad="1"/>
<contactref element="J10" pad="6"/>
<contactref element="J7" pad="19"/>
<contactref element="R5" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q4" pad="3"/>
<contactref element="Q5" pad="3"/>
<contactref element="Q6" pad="3"/>
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U2" pad="92"/>
<contactref element="R2" pad="1"/>
<contactref element="J7" pad="09"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="SWCLK">
<contactref element="PROGRAMMER" pad="1"/>
<contactref element="U2" pad="76"/>
<contactref element="TP20" pad="TP"/>
</signal>
<signal name="SCLEX">
<contactref element="R3" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J6" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="TP5" pad="TP"/>
<contactref element="U2" pad="46"/>
</signal>
<signal name="SDAEX">
<contactref element="R4" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="TP6" pad="TP"/>
<contactref element="U2" pad="47"/>
</signal>
<signal name="SWDIO">
<contactref element="PROGRAMMER" pad="2"/>
<contactref element="U2" pad="72"/>
<contactref element="R6" pad="2"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="NRST">
<contactref element="PROGRAMMER" pad="4"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="SWO">
<contactref element="PROGRAMMER" pad="3"/>
</signal>
<signal name="SDACOM">
<contactref element="I2C" pad="2"/>
<contactref element="TP2" pad="TP"/>
<contactref element="U2" pad="66"/>
</signal>
<signal name="SCLCOM">
<contactref element="I2C" pad="1"/>
<contactref element="U2" pad="67"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="VCAP">
<contactref element="U2" pad="48"/>
<contactref element="U2" pad="73"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="6"/>
</signal>
<signal name="VCHRG">
<contactref element="CHRG" pad="2"/>
<contactref element="J7" pad="20"/>
<contactref element="TP30" pad="TP"/>
</signal>
<signal name="5V_VIN">
<contactref element="VIN" pad="3"/>
<contactref element="J7" pad="18"/>
<contactref element="TP4" pad="TP"/>
<contactref element="J2" pad="4"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="SD_DETECT">
<contactref element="J10" pad="10"/>
<contactref element="U2" pad="1"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="SDMMC2_D3">
<contactref element="U2" pad="90"/>
<contactref element="J10" pad="2"/>
<contactref element="TP24" pad="TP"/>
</signal>
<signal name="SDMMC2_D2">
<contactref element="U2" pad="89"/>
<contactref element="J10" pad="1"/>
<contactref element="TP23" pad="TP"/>
</signal>
<signal name="SDMMC2_CMD">
<contactref element="U2" pad="88"/>
<contactref element="J10" pad="3"/>
<contactref element="TP25" pad="TP"/>
</signal>
<signal name="SDMMC2_CK">
<contactref element="U2" pad="87"/>
<contactref element="J10" pad="5"/>
<contactref element="TP26" pad="TP"/>
</signal>
<signal name="SDMMC2_D1">
<contactref element="U2" pad="54"/>
<contactref element="J10" pad="8"/>
<contactref element="TP22" pad="TP"/>
</signal>
<signal name="SDMMC2_D0">
<contactref element="U2" pad="53"/>
<contactref element="J10" pad="7"/>
<contactref element="TP21" pad="TP"/>
</signal>
<signal name="SCA">
<contactref element="J7" pad="07"/>
<contactref element="U2" pad="93"/>
<contactref element="R1" pad="1"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="IO1">
<contactref element="J7" pad="11"/>
<contactref element="U2" pad="37"/>
<contactref element="TP11" pad="TP"/>
</signal>
<signal name="IO2">
<contactref element="J7" pad="13"/>
<contactref element="U2" pad="38"/>
<contactref element="TP12" pad="TP"/>
</signal>
<signal name="IO3">
<contactref element="J7" pad="15"/>
<contactref element="U2" pad="39"/>
<contactref element="TP13" pad="TP"/>
</signal>
<signal name="IO4">
<contactref element="J7" pad="17"/>
<contactref element="U2" pad="40"/>
<contactref element="TP14" pad="TP"/>
</signal>
<signal name="WKUP">
<contactref element="J7" pad="14"/>
</signal>
<signal name="OW">
<contactref element="J7" pad="16"/>
<contactref element="U2" pad="41"/>
<contactref element="TP15" pad="TP"/>
</signal>
<signal name="N_CHRG_SENSE">
<contactref element="U2" pad="28"/>
<contactref element="J7" pad="12"/>
<contactref element="TP31" pad="TP"/>
</signal>
<signal name="TX_UART4">
<contactref element="J7" pad="02"/>
<contactref element="U2" pad="22"/>
<contactref element="TP19" pad="TP"/>
</signal>
<signal name="RX_UART4">
<contactref element="J7" pad="04"/>
<contactref element="U2" pad="23"/>
<contactref element="TP18" pad="TP"/>
</signal>
<signal name="RX2">
<contactref element="U2" pad="25"/>
<contactref element="J7" pad="03"/>
<contactref element="TP16" pad="TP"/>
</signal>
<signal name="TX2">
<contactref element="U2" pad="24"/>
<contactref element="J7" pad="05"/>
<contactref element="TP17" pad="TP"/>
</signal>
<signal name="SPI1_SCK">
<contactref element="U2" pad="29"/>
<contactref element="J7" pad="06"/>
<contactref element="TP27" pad="TP"/>
</signal>
<signal name="SPI1_MISO">
<contactref element="U2" pad="30"/>
<contactref element="J7" pad="08"/>
<contactref element="TP28" pad="TP"/>
</signal>
<signal name="SPI1_MOSI">
<contactref element="U2" pad="31"/>
<contactref element="J7" pad="10"/>
<contactref element="TP29" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="94"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="3"/>
</signal>
<signal name="TEMP_A0">
<contactref element="U2" pad="34"/>
<contactref element="U1" pad="7"/>
<contactref element="R7" pad="1"/>
<contactref element="TP32" pad="TP"/>
</signal>
<signal name="TEMP_A1">
<contactref element="U2" pad="35"/>
<contactref element="U1" pad="6"/>
<contactref element="R8" pad="1"/>
<contactref element="TP33" pad="TP"/>
</signal>
<signal name="TEMP_A2">
<contactref element="U2" pad="36"/>
<contactref element="U1" pad="5"/>
<contactref element="R9" pad="1"/>
<contactref element="TP34" pad="TP"/>
</signal>
<signal name="1_SEN_ON">
<contactref element="Q1" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="2_SEN_ON">
<contactref element="Q2" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="3_SEN_ON">
<contactref element="Q3" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="4_SEN_ON">
<contactref element="Q4" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="5_SEN_ON">
<contactref element="Q5" pad="2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="6_SEN_ON">
<contactref element="Q6" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="4_SEN_EN">
<contactref element="U2" pad="51"/>
<contactref element="R13" pad="1"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="5_SEN_EN">
<contactref element="U2" pad="43"/>
<contactref element="R14" pad="1"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="6_SEN_EN">
<contactref element="U2" pad="42"/>
<contactref element="R15" pad="1"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="1_SEN_EN">
<contactref element="U2" pad="55"/>
<contactref element="R10" pad="1"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="2_SEN_EN">
<contactref element="U2" pad="56"/>
<contactref element="R11" pad="1"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="3_SEN_EN">
<contactref element="U2" pad="52"/>
<contactref element="R12" pad="1"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="GND_SEN6">
<contactref element="J6" pad="3"/>
<contactref element="J6" pad="S1"/>
<contactref element="J6" pad="S2"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="GND_SEN1">
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="S1"/>
<contactref element="J1" pad="S2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="GND_SEN2">
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="S1"/>
<contactref element="J2" pad="S2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="GND_SEN3">
<contactref element="J3" pad="3"/>
<contactref element="J3" pad="S1"/>
<contactref element="J3" pad="S2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="GND_SEN5">
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="S1"/>
<contactref element="J5" pad="S2"/>
<contactref element="Q5" pad="1"/>
</signal>
<signal name="GND_SEN4">
<contactref element="J4" pad="3"/>
<contactref element="J4" pad="S1"/>
<contactref element="J4" pad="S2"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D2" pad="CATHODE"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="CATHODE"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="ST1">
<contactref element="D1" pad="ANODE"/>
<contactref element="U2" pad="95"/>
</signal>
<signal name="ST2">
<contactref element="D2" pad="ANODE"/>
<contactref element="U2" pad="96"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
