<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="0" x2="26.34" y2="0" width="0" layer="20"/>
<wire x1="26.34" y1="0" x2="26.34" y2="86.35" width="0" layer="20"/>
<wire x1="26.34" y1="86.35" x2="-1.27" y2="86.35" width="0" layer="20"/>
<wire x1="-1.27" y1="86.35" x2="-1.27" y2="0" width="0" layer="20"/>
<text>5V</text>
<text>RX</text>
<text>TX</text>
<text>GND</text>
<text>Rev B 3/29/16</text>
<text>BB-8 Builders</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
<package name="PROTRINKET">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X10">
</package>
<package name="1X04_NO_SILK_ALL_ROUND">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JOYSTICK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CN1" library="adafruit" package="JST-PH-2-SMT-RA" value=""/>
<element name="CN2" library="adafruit" package="DCJACK_2MM_PTH" value=""/>
<element name="J1" library="SparkFun-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04_NO_SILK_ALL_ROUND" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="U$2" library="adafruit" package="PROTRINKET" value="PRO_TRINKET"/>
<element name="U1" library="SparkFun-Electromechanical" package="JOYSTICK" value="JOYSTICKPTH"/>
</elements>
<signals>
<signal name="USB">
<contactref element="U$2" pad="USB"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="VCC"/>
<contactref element="U1" pad="V1"/>
<contactref element="U1" pad="H1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="A0"/>
<contactref element="U1" pad="V2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="H2"/>
<contactref element="U$2" pad="A1"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="3"/>
<contactref element="U1" pad="B1A"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="GND"/>
<contactref element="U1" pad="V3"/>
<contactref element="U1" pad="H3"/>
<contactref element="U1" pad="B2A"/>
<contactref element="J1" pad="4"/>
<contactref element="CN1" pad="2"/>
<contactref element="CN2" pad="GND"/>
<contactref element="CN2" pad="GNDBREAK"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="TX"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="RX"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="J2" pad="2"/>
<contactref element="CN1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="CN2" pad="PWR"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="J2" pad="3"/>
<contactref element="U$2" pad="BAT+"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
