<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="22.86" y1="59.69" x2="24.13" y2="58.42" width="0.0254" layer="20" curve="-90"/>
<wire x1="24.13" y1="54.61" x2="22.86" y2="53.34" width="0.0254" layer="20" curve="-90"/>
<wire x1="19.05" y1="53.34" x2="17.78" y2="54.61" width="0.0254" layer="20" curve="-90"/>
<wire x1="17.78" y1="58.42" x2="17.78" y2="54.61" width="0.0254" layer="20"/>
<wire x1="19.05" y1="53.34" x2="22.86" y2="53.34" width="0.0254" layer="20"/>
<wire x1="24.13" y1="54.61" x2="24.13" y2="58.42" width="0.0254" layer="20"/>
<wire x1="22.86" y1="59.69" x2="19.05" y2="59.69" width="0.0254" layer="20"/>
<text>JST-SH</text>
<text>JST-SH</text>
<text>cross</text>
<text>JST-SH</text>
<text>SH2-0.1-H
JST-SH
2.54</text>
<text>BM02B-SRSS-TB</text>
<wire x1="17.78" y1="58.42" x2="19.05" y2="59.69" width="0.0254" layer="20" curve="-90"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-jst2-2">
<description>&lt;b&gt;J.S.T. Connectors&lt;/b&gt;&lt;p&gt;
J.S.T Mfg Co.,Ltd.&lt;p&gt;
http://www.jst-mfg.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="BM02B-SRSS-TB">
<description>&lt;b&gt;Shrouded Header, top entry type&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-jst2-2" package="BM02B-SRSS-TB" value="BM02B-SRSS-TB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="J1" pad="2"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="1"/>
<contactref element="X2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
