<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="38.1" x2="0" y2="6.4008" width="0.2032" layer="20"/>
<wire x1="0" y1="6.4008" x2="17.78" y2="6.4008" width="0.2032" layer="20"/>
<wire x1="17.78" y1="6.4008" x2="17.78" y2="38.1" width="0.2032" layer="20"/>
<wire x1="17.78" y1="38.1" x2="0" y2="38.1" width="0.2032" layer="20"/>
<text>9</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>GND</text>
<text>RST</text>
<text>RXI</text>
<text>TXO</text>
<text>RAW</text>
<text>GND</text>
<text>RST</text>
<text>VCC</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>10</text>
<text>Vishnu V1</text>
<text>Achuthan 2014</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X12">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP6" library="SparkFun" package="1X12" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun" package="1X12" value="">
<attribute name="VALUE"/>
</element>
<element name="NRF24" library="SparkFun-Connectors" package="2X4" value="*">
<attribute name="VALUE"/>
</element>
<element name="G|A2|V" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G|A1|V" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G|A0|V" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G|D3" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="NAME"/>
</element>
<element name="G|D4" library="SparkFun-Connectors" package="1X02" value="M02PTH">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP7" pad="9"/>
<contactref element="JP6" pad="2"/>
<contactref element="NRF24" pad="1"/>
<contactref element="G|A0|V" pad="1"/>
<contactref element="G|A1|V" pad="1"/>
<contactref element="G|A2|V" pad="1"/>
<contactref element="G|D4" pad="1"/>
<contactref element="G|D3" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="JP7" pad="10"/>
<contactref element="JP6" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="JP6" pad="9"/>
<contactref element="NRF24" pad="5"/>
</signal>
<signal name="MISO">
<contactref element="JP6" pad="10"/>
<contactref element="NRF24" pad="7"/>
</signal>
<signal name="MOSI">
<contactref element="JP6" pad="11"/>
<contactref element="NRF24" pad="6"/>
</signal>
<signal name="TXO">
<contactref element="JP7" pad="12"/>
</signal>
<signal name="VCC">
<contactref element="JP6" pad="4"/>
<contactref element="NRF24" pad="2"/>
<contactref element="G|A0|V" pad="3"/>
<contactref element="G|A1|V" pad="3"/>
<contactref element="G|A2|V" pad="3"/>
</signal>
<signal name="RAW">
<contactref element="JP6" pad="1"/>
</signal>
<signal name="D9">
<contactref element="JP7" pad="1"/>
<contactref element="NRF24" pad="3"/>
</signal>
<signal name="D8">
<contactref element="JP7" pad="2"/>
</signal>
<signal name="A3">
<contactref element="JP6" pad="5"/>
</signal>
<signal name="A2">
<contactref element="JP6" pad="6"/>
<contactref element="G|A2|V" pad="2"/>
</signal>
<signal name="A1">
<contactref element="JP6" pad="7"/>
<contactref element="G|A1|V" pad="2"/>
</signal>
<signal name="A0">
<contactref element="JP6" pad="8"/>
<contactref element="G|A0|V" pad="2"/>
</signal>
<signal name="D2">
<contactref element="JP7" pad="8"/>
<contactref element="NRF24" pad="8"/>
</signal>
<signal name="D3">
<contactref element="JP7" pad="7"/>
<contactref element="G|D3" pad="2"/>
</signal>
<signal name="D4">
<contactref element="JP7" pad="6"/>
<contactref element="G|D4" pad="2"/>
</signal>
<signal name="D5">
<contactref element="JP7" pad="5"/>
</signal>
<signal name="D6">
<contactref element="JP7" pad="4"/>
</signal>
<signal name="D7">
<contactref element="JP7" pad="3"/>
</signal>
<signal name="D10">
<contactref element="JP6" pad="12"/>
<contactref element="NRF24" pad="4"/>
</signal>
<signal name="RXI">
<contactref element="JP7" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
