<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="1.4224" y1="-0.4064" x2="17.3736" y2="-0.4064" width="0.1778" layer="20"/>
<wire x1="17.3736" y1="-0.4064" x2="17.3736" y2="11.684" width="0.1778" layer="20"/>
<wire x1="17.3736" y1="11.684" x2="1.4224" y2="11.684" width="0.1778" layer="20"/>
<wire x1="1.4224" y1="11.684" x2="1.4224" y2="-0.4064" width="0.1778" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>CCS811</text>
<text>WAKE</text>
<text>INT</text>
<text>Designed by</text>
<text>AKstudios</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="CCS811">
<packages>
<package name="LGA">
<description>CCS811 is available in a lead 2.7 x 4.0mm, 0.6mm pitch LGA package.

Designed by Akram Ali
September 2016</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U10" library="CCS811" package="LGA" value="CCS811"/>
<element name="C5" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="100K">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U10" pad="11"/>
<contactref element="C5" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U10" pad="6"/>
<contactref element="C5" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U10" pad="10"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="U10" pad="9"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U10" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="WAKE">
<contactref element="J1" pad="5"/>
<contactref element="U10" pad="7"/>
</signal>
<signal name="INT">
<contactref element="J1" pad="6"/>
<contactref element="U10" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="U10" pad="5"/>
<contactref element="U10" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
