<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<text>GND</text>
<text>GND</text>
<wire x1="0" y1="0" x2="56" y2="0" width="0" layer="20"/>
<wire x1="56" y1="0" x2="56" y2="20" width="0" layer="20"/>
<wire x1="56" y1="20" x2="0" y2="20" width="0" layer="20"/>
<wire x1="0" y1="20" x2="0" y2="0" width="0" layer="20"/>
<text>ULP 433MHz Wakeup Receiver
Breakout, Rev. A
Clemson University
Josiah Hester
</text>
<text>ULP 433MHz Wakeup Receiver
Breakout, Rev. A
Clemson University
Josiah Hester
</text>
<text>DAT</text>
<text>DAT</text>
<text>WAKE</text>
<text>WAKE</text>
<text>CS</text>
<text>CS</text>
<text>SCL</text>
<text>SCL</text>
<text>SDI</text>
<text>SDI</text>
<text>SDO</text>
<text>SDO</text>
<text>VCC</text>
<text>VCC</text>
</plain>
<libraries>
<library name="AS3932">
<packages>
<package name="TSSOP16">
<description>&lt;b&gt;16-Lead Thin Shrink Small Outline Package&lt;/b&gt; [TSSOP] (RU-16)&lt;p&gt;
Source: 8x ADG1408_1409.pdf</description>
</package>
</packages>
</library>
<library name="tiny_passives">
<packages>
<package name="0603L">
</package>
<package name="0402">
</package>
</packages>
</library>
<library name="HSMS285C">
<packages>
<package name="SOT-323">
</package>
</packages>
</library>
<library name="ANT1204">
<packages>
<package name="CHIP-ANT">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U3" library="AS3932" package="TSSOP16" value="AS3932">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="AS3932-BTSTCT-ND"/>
</element>
<element name="L3" library="tiny_passives" package="0603L" value="180nH">
<attribute name="FARNELL" value="0603HP-R18XGLU"/>
<attribute name="COILCRAFT" value="0603HP-R18XGLU"/>
</element>
<element name="L1" library="tiny_passives" package="0603L" value="39nH">
<attribute name="FARNELL" value="0603HP-39NXGLU"/>
<attribute name="COILCRAFT" value="0603HP-39NXGLU"/>
</element>
<element name="C1" library="tiny_passives" package="0402" value="6pF">
<attribute name="DIGIKEY" value="490-11230-1-ND"/>
</element>
<element name="C21" library="tiny_passives" package="0402" value="7pF">
<attribute name="DIGIKEY" value="490-11234-1-ND"/>
</element>
<element name="C22" library="tiny_passives" package="0402" value="6pF">
<attribute name="DIGIKEY" value="490-11230-1-ND"/>
</element>
<element name="C3" library="tiny_passives" package="0402" value="18pF">
<attribute name="DIGIKEY" value="490-6203-1-ND"/>
</element>
<element name="C6" library="tiny_passives" package="0402" value="220pF">
<attribute name="DIGIKEY" value="490-10684-1-ND"/>
</element>
<element name="R1" library="tiny_passives" package="0402" value="330k">
<attribute name="MANAFACTURER" value="MC00625W04021330K"/>
<attribute name="NEWARK" value="58K4329"/>
</element>
<element name="D1D2" library="HSMS285C" package="SOT-323" value="HSMS-285C">
<attribute name="DIGIKEY" value="516-2558-ND"/>
</element>
<element name="U$1" library="ANT1204" package="CHIP-ANT" value="ANT1204">
<attribute name="DIGIKEY" value="311-1570-1-ND"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="tiny_passives" package="0402" value="0">
<attribute name="DIGIKEY" value="311-0.0JRCT-ND"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="D1D2" pad="P1"/>
<contactref element="C3" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="U3" pad="13"/>
<contactref element="U3" pad="6"/>
<contactref element="JP1" pad="7"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VBAT">
</signal>
<signal name="VCC">
<contactref element="U3" pad="5"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$10">
</signal>
<signal name="XT1_GND">
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$1">
<contactref element="L1" pad="1"/>
<contactref element="U$1" pad="S1"/>
</signal>
<signal name="N$2">
<contactref element="L1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="2"/>
<contactref element="L3" pad="1"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="L3" pad="2"/>
<contactref element="D1D2" pad="P3"/>
</signal>
<signal name="N$7">
<contactref element="D1D2" pad="P2"/>
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U3" pad="9"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="DAT">
<contactref element="U3" pad="15"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="WAKE">
<contactref element="U3" pad="14"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="CS">
<contactref element="U3" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U3" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SDI">
<contactref element="U3" pad="3"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SDO">
<contactref element="U3" pad="4"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
