<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="34" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2" y1="0" x2="34" y2="0" width="0" layer="20"/>
<wire x1="34" y1="0" x2="36" y2="2" width="0" layer="20" curve="90"/>
<wire x1="36" y1="2" x2="36" y2="9.16" width="0" layer="20"/>
<wire x1="36" y1="9.16" x2="35" y2="10.16" width="0" layer="20" curve="90"/>
<wire x1="35" y1="10.16" x2="20.32" y2="10.16" width="0" layer="20"/>
<wire x1="2" y1="36" x2="34" y2="36" width="0" layer="20"/>
<wire x1="34" y1="36" x2="36" y2="34" width="0" layer="20" curve="-90"/>
<wire x1="36" y1="34" x2="36" y2="26.4" width="0" layer="20"/>
<wire x1="36" y1="26.4" x2="35" y2="25.4" width="0" layer="20" curve="-90"/>
<wire x1="35" y1="25.4" x2="20.32" y2="25.4" width="0" layer="20"/>
<wire x1="2" y1="36" x2="0" y2="34" width="0" layer="20" curve="90"/>
<hole x="2.75" y="33.25" drill="3.2"/>
<hole x="33.25" y="33.25" drill="3.2"/>
<hole x="33.25" y="2.75" drill="3.2"/>
<hole x="2.75" y="2.75" drill="3.2"/>
<wire x1="20.32" y1="10.16" x2="20.32" y2="25.4" width="0" layer="20"/>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>VIN</text>
<text>VOUT</text>
<text>CAM</text>
<text>VTX</text>
<text>TX</text>
<text>RX</text>
<hole x="4" y="24" drill="3.2"/>
<hole x="4" y="12" drill="3.2"/>
<text>5V</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>VBAT</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>1</text>
<text>3</text>
<text>4</text>
<text>2</text>
<text>RX</text>
<text>TX</text>
<text>-</text>
<text>VIN</text>
<text>VOUT</text>
<text>GND</text>
<text>5V</text>
<text>S</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X02">
</package>
<package name="1X03">
</package>
</packages>
</library>
<library name="00_PERSONAL">
<packages>
<package name="6X4">
<description>6mm x 4mm pad</description>
</package>
<package name="3X1.75">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MINIMOSD_VID" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="MINIMOSD_PWR" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="MINIMOSD_SIG" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="5V_HDR" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="5V_REG" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$2" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$3" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$4" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$5" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$6" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$7" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$8" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$9" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$10" library="00_PERSONAL" package="6X4" value=""/>
<element name="U$11" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$12" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$13" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$14" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$15" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$16" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$17" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$18" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$19" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$20" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$21" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$22" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$23" library="00_PERSONAL" package="3X1.75" value=""/>
<element name="U$24" library="00_PERSONAL" package="3X1.75" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="MINIMOSD_VID" pad="2"/>
<contactref element="MINIMOSD_VID" pad="4"/>
<contactref element="MINIMOSD_PWR" pad="1"/>
<contactref element="5V_HDR" pad="1"/>
<contactref element="5V_REG" pad="2"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="U$8" pad="P$1"/>
<contactref element="U$10" pad="P$1"/>
<contactref element="U$15" pad="P$1"/>
<contactref element="U$16" pad="P$1"/>
<contactref element="U$17" pad="P$1"/>
<contactref element="U$18" pad="P$1"/>
<contactref element="U$20" pad="P$1"/>
<contactref element="U$19" pad="P$1"/>
</signal>
<signal name="RX">
<contactref element="MINIMOSD_SIG" pad="2"/>
<contactref element="U$23" pad="P$1"/>
</signal>
<signal name="TX">
<contactref element="MINIMOSD_SIG" pad="1"/>
<contactref element="U$24" pad="P$1"/>
</signal>
<signal name="VOUT">
<contactref element="MINIMOSD_VID" pad="1"/>
<contactref element="U$22" pad="P$1"/>
</signal>
<signal name="VIN">
<contactref element="MINIMOSD_VID" pad="3"/>
<contactref element="U$21" pad="P$1"/>
</signal>
<signal name="5V">
<contactref element="MINIMOSD_PWR" pad="2"/>
<contactref element="5V_HDR" pad="2"/>
<contactref element="5V_REG" pad="3"/>
</signal>
<signal name="VBAT">
<contactref element="5V_REG" pad="1"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
<contactref element="U$9" pad="P$1"/>
</signal>
<signal name="S1">
<contactref element="U$11" pad="P$1"/>
</signal>
<signal name="S2">
<contactref element="U$12" pad="P$1"/>
</signal>
<signal name="S3">
<contactref element="U$13" pad="P$1"/>
</signal>
<signal name="S4">
<contactref element="U$14" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
