<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<hole x="2.413" y="11.557" drill="3"/>
<text>by LowPowerLab</text>
<hole x="30.48" y="11.557" drill="3"/>
<text>GarageMote</text>
<text>Moteino shield</text>
<text>HALL</text>
<text>OPENER</text>
<text>SENSOR</text>
<text>A0</text>
<text>A1</text>
<text>D4</text>
<text>-</text>
<text>-</text>
<text>D5</text>
<text>GarageMote</text>
<text>Garage door controller
Moteino shield</text>
<text>LowPowerLab.com</text>
<text>D5</text>
<text>D4</text>
<text>A0</text>
<text>A1</text>
<text>D6</text>
<text>D7</text>
<text>XXXXXXXXXXXX</text>
<text>OPN</text>
<text>CLS</text>
<wire x1="53.34" y1="1.905" x2="51.435" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="51.435" y1="25.654" x2="53.34" y2="23.749" width="0" layer="20" curve="-90"/>
<wire x1="0.762" y1="0" x2="51.435" y2="0" width="0" layer="20"/>
<wire x1="51.435" y1="25.654" x2="0.762" y2="25.654" width="0" layer="20"/>
<wire x1="0.762" y1="25.654" x2="0" y2="24.892" width="0" layer="20"/>
<wire x1="0" y1="24.892" x2="0" y2="0.762" width="0" layer="20"/>
<wire x1="0" y1="0.762" x2="0.762" y2="0" width="0" layer="20"/>
<wire x1="53.34" y1="23.749" x2="53.34" y2="1.905" width="0" layer="20"/>
<text>R2</text>
<text>BTN
(D3)</text>
<text>relay</text>
<text>A1</text>
<text>A0</text>
<text>VIN</text>
<text>3v3</text>
<text>RST</text>
<text>D4</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>relayPWR</text>
<text>4007</text>
<text>VIN</text>
<text>2.1mm Jack</text>
<text>Power via</text>
<text>R2</text>
<text>R2</text>
<text>R2</text>
<text>GarageMote</text>
<text>RELAY</text>
<text>OPEN</text>
<text>HALL</text>
<text>CLS</text>
<text>SENSOR</text>
</plain>
<libraries>
<library name="LowPowerLab">
<packages>
<package name="JRC-23F">
</package>
<package name="0603-RES">
</package>
<package name="AXIAL-1/4W">
</package>
<package name="TACTILE-PTH-SIDEEZ">
</package>
<package name="DIODEPTH">
</package>
<package name="LOGO_LOWPOWERLAB">
</package>
<package name="2.1MM_JACK">
</package>
<package name="1X02_NS">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X13">
</package>
<package name="1X08">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JRC-2F" library="LowPowerLab" package="JRC-23F" value="JRC-23F"/>
<element name="JP1" library="SparkFun-Connectors" package="1X13" value="M13"/>
<element name="JP2" library="SparkFun-Connectors" package="1X13" value="M13"/>
<element name="JP3" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="LowPowerLab" package="0603-RES" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R1" library="LowPowerLab" package="0603-RES" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R4" library="LowPowerLab" package="AXIAL-1/4W" value=""/>
<element name="R3" library="LowPowerLab" package="AXIAL-1/4W" value=""/>
<element name="S1" library="LowPowerLab" package="TACTILE-PTH-SIDEEZ" value="SWITCH-MOMENTARY-2SIDE_EZ"/>
<element name="U$4" library="LowPowerLab" package="DIODEPTH" value="DIODEPTH"/>
<element name="U$5" library="LowPowerLab" package="LOGO_LOWPOWERLAB" value=""/>
<element name="U$6" library="LowPowerLab" package="LOGO_LOWPOWERLAB" value=""/>
<element name="2.1MM_BARREL_JACK" library="LowPowerLab" package="2.1MM_JACK" value="2.1MMJACKTH_NOSILK"/>
<element name="JP4" library="SparkFun-Connectors" package="1X13" value="M13"/>
<element name="JP5" library="SparkFun-Connectors" package="1X13" value="M13"/>
<element name="U$9" library="LowPowerLab" package="1X02_NS" value="HDR_2PIN"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JRC-2F" pad="COIL2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="7"/>
<contactref element="JP3" pad="4"/>
<contactref element="U$4" pad="ANODE_PLUS"/>
<contactref element="S1" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="2.1MM_BARREL_JACK" pad="RING"/>
<contactref element="U$9" pad="2"/>
<contactref element="U$9" pad="2"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="2.1MM_BARREL_JACK" pad="TIP"/>
<contactref element="U$9" pad="1"/>
<contactref element="U$9" pad="1"/>
</signal>
<signal name="A0">
<contactref element="JP1" pad="13"/>
<contactref element="JP3" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="P$1"/>
<contactref element="JP4" pad="13"/>
<contactref element="JP5" pad="13"/>
</signal>
<signal name="A1">
<contactref element="JP1" pad="12"/>
<contactref element="JP3" pad="8"/>
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="P$1"/>
<contactref element="JP4" pad="12"/>
<contactref element="JP5" pad="12"/>
</signal>
<signal name="D4">
<contactref element="JP3" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="D5">
<contactref element="JP3" pad="6"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="P$2"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="D6">
<contactref element="JRC-2F" pad="COIL1"/>
<contactref element="JP2" pad="8"/>
<contactref element="JP2" pad="7"/>
<contactref element="U$4" pad="CATHODE_MINUS"/>
</signal>
<signal name="RELAYIN">
<contactref element="JP3" pad="1"/>
<contactref element="JRC-2F" pad="COM2"/>
</signal>
<signal name="RELAYOUT">
<contactref element="JP3" pad="2"/>
<contactref element="JRC-2F" pad="SW1"/>
</signal>
<signal name="N$1">
<contactref element="JP2" pad="11"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="3"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="4"/>
<contactref element="JP4" pad="4"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="5"/>
<contactref element="JP4" pad="5"/>
<contactref element="JP5" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="6"/>
<contactref element="JP4" pad="6"/>
<contactref element="JP5" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="7"/>
<contactref element="JP4" pad="7"/>
<contactref element="JP5" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="JP1" pad="8"/>
<contactref element="JP4" pad="8"/>
<contactref element="JP5" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="9"/>
<contactref element="JP4" pad="9"/>
<contactref element="JP5" pad="9"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="10"/>
<contactref element="JP4" pad="10"/>
<contactref element="JP5" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="11"/>
<contactref element="JP4" pad="11"/>
<contactref element="JP5" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
