<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="5.08" x2="5.08" y2="0" width="0" layer="20" curve="90"/>
<wire x1="5.08" y1="0" x2="10.16" y2="5.08" width="0" layer="20" curve="90"/>
<wire x1="10.16" y1="5.08" x2="5.08" y2="10.16" width="0" layer="20" curve="90"/>
<wire x1="5.08" y1="10.16" x2="0" y2="5.08" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="0402">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD.03X.05">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED10" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED11" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED12" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED13" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED14" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED15" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED16" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED17" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED18" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED19" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED20" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="LED9" library="led" package="0402" value="">
<attribute name="VALUE"/>
</element>
<element name="TP1" library="SparkFun-Passives" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP2" library="SparkFun-Passives" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP3" library="SparkFun-Passives" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP4" library="SparkFun-Passives" package="PAD.03X.05" value="TEST-POINT3X5"/>
<element name="TP5" library="SparkFun-Passives" package="PAD.03X.05" value="TEST-POINT3X5"/>
</elements>
<signals>
<signal name="PIN3">
<contactref element="LED11" pad="A"/>
<contactref element="LED12" pad="C"/>
<contactref element="LED9" pad="C"/>
<contactref element="LED10" pad="A"/>
<contactref element="LED16" pad="A"/>
<contactref element="LED15" pad="C"/>
<contactref element="LED17" pad="A"/>
<contactref element="LED18" pad="C"/>
<contactref element="TP3" pad="P$1"/>
</signal>
<signal name="PIN5">
<contactref element="LED7" pad="A"/>
<contactref element="LED8" pad="C"/>
<contactref element="LED6" pad="A"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED11" pad="C"/>
<contactref element="LED12" pad="A"/>
<contactref element="LED13" pad="A"/>
<contactref element="LED14" pad="C"/>
<contactref element="TP5" pad="P$1"/>
</signal>
<signal name="PIN4">
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED19" pad="A"/>
<contactref element="LED20" pad="C"/>
<contactref element="LED17" pad="C"/>
<contactref element="LED18" pad="A"/>
<contactref element="TP4" pad="P$1"/>
</signal>
<signal name="PIN2">
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED7" pad="C"/>
<contactref element="LED8" pad="A"/>
<contactref element="LED9" pad="A"/>
<contactref element="LED10" pad="C"/>
<contactref element="LED19" pad="C"/>
<contactref element="LED20" pad="A"/>
<contactref element="TP2" pad="P$1"/>
</signal>
<signal name="PIN1">
<contactref element="LED3" pad="A"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED16" pad="C"/>
<contactref element="LED15" pad="A"/>
<contactref element="LED13" pad="C"/>
<contactref element="LED14" pad="A"/>
<contactref element="TP1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
