<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="16.51" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="12.319" y2="0" width="0" layer="20"/>
<wire x1="12.319" y1="0" x2="13.589" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="13.589" y1="1.27" x2="13.589" y2="16.51" width="0" layer="20"/>
<wire x1="13.589" y1="16.51" x2="12.319" y2="17.78" width="0" layer="20" curve="90"/>
<wire x1="12.319" y1="17.78" x2="1.27" y2="17.78" width="0" layer="20"/>
<wire x1="1.27" y1="17.78" x2="0" y2="16.51" width="0" layer="20" curve="90"/>
<text>vin</text>
<text>batok</text>
<text>gnd</text>
<text>vstor</text>
<text>vbat</text>
<text>BQ25504 Eval rev 1
(c) Scalz 2016</text>
<text>Openhardware.io</text>
<text>gnd</text>
<text>batok</text>
<text>vbat</text>
<text>vstor</text>
<text>vin</text>
</plain>
<libraries>
<library name="LowPowerLab">
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="0805-CAP">
</package>
</packages>
</library>
<library name="solar">
<packages>
<package name="QFN50P300X300X100-17N">
</package>
</packages>
</library>
<library name="inductors">
<packages>
<package name="LPS4018-223MRB">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
</packages>
</library>
<library name="pmo_graphics">
<packages>
<package name="OPENHW_SMALL_OSHPARK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="solar" package="QFN50P300X300X100-17N" value="BQ25504RGTT">
<attribute name="PACKAGE" value="QFN-16"/>
<attribute name="OC_NEWARK" value="76T8906 "/>
<attribute name="MPN" value="BQ25504RGTT"/>
<attribute name="SUPPLIER" value="TEXAS INSTRUMENTS "/>
<attribute name="OC_FARNELL" value="2144306 "/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="LowPowerLab" package="0603-CAP" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="inductors" package="LPS4018-223MRB" value="LPS4018-223MRB">
<attribute name="NAME"/>
</element>
<element name="C4" library="LowPowerLab" package="0603-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="LowPowerLab" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="LowPowerLab" package="0805-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="LowPowerLab" package="0603-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="pmo_graphics" package="OPENHW_SMALL_OSHPARK" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="13"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="VBAT">
<contactref element="U1" pad="14"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="16"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VSTOR">
<contactref element="U1" pad="15"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="VBAT_OK">
<contactref element="U1" pad="11"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="U1" pad="10"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="U1" pad="9"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="VRDIV">
<contactref element="U1" pad="7"/>
<contactref element="R4" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="VBATOV">
<contactref element="U1" pad="6"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="VBATUV">
<contactref element="U1" pad="8"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="C1" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
