<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="75.87" y2="0" width="0" layer="20"/>
<wire x1="75.87" y1="0" x2="75.87" y2="49.52" width="0" layer="20"/>
<wire x1="75.87" y1="49.52" x2="0" y2="49.52" width="0" layer="20"/>
<wire x1="0" y1="49.52" x2="0" y2="0" width="0" layer="20"/>
<hole x="5.08" y="45.72" drill="3.2"/>
<hole x="71.12" y="45.72" drill="3.2"/>
<hole x="71.12" y="3.81" drill="3.2"/>
<hole x="5.08" y="3.81" drill="3.2"/>
<text>Mouse Piano - Scanner Board - PDIPV1</text>
<text>CyberAntics 2015
Ramon Yvarra
ryvarra@cyberantics.net
Amelia's happiest moments were
those shared with others. She
loved hearing other's make music
with her home.  </text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-SHROUDED">
</package>
<package name="1X03">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="switch-dil">
<description>&lt;b&gt;DIL Switches and Code Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CTS-219-08">
<description>&lt;b&gt;Surface Mount DIP Switch Series 219 SMT&lt;/b&gt;&lt;p&gt;
CTS Electronic Components&lt;br&gt;
Sourc: www.ctscorp.com</description>
</package>
</packages>
</library>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP254P1524X635-24">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ANALOG-IN" library="SparkFun-Connectors" package="2X3-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-10681"/>
</element>
<element name="ANALOG-OUT" library="SparkFun-Connectors" package="2X3-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-10681"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="0.1uF"/>
<element name="C4" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value="0.1uF"/>
<element name="JP1" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="JP10" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP12" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP13" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP14" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP15" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP16" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X03" value="JP2">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGIC-IN" library="SparkFun-Connectors" package="2X3-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-10681"/>
</element>
<element name="LOGIC-OUT" library="SparkFun-Connectors" package="2X3-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-10681"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3" value="10k"/>
<element name="S1" library="switch-dil" package="CTS-219-08" value="219-08">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="POWER" library="SparkFun-AnalogIC" package="DIP254P1524X635-24" value="MUX-74HC4067">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ANALOG" library="SparkFun-AnalogIC" package="DIP254P1524X635-24" value="MUX-74HC4067">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="2"/>
<contactref element="POWER" pad="9"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="1"/>
<contactref element="ANALOG" pad="9"/>
</signal>
<signal name="N$4">
<contactref element="JP2" pad="2"/>
<contactref element="POWER" pad="8"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="1"/>
<contactref element="ANALOG" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="JP3" pad="2"/>
<contactref element="POWER" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="JP3" pad="1"/>
<contactref element="ANALOG" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="JP4" pad="2"/>
<contactref element="POWER" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="JP4" pad="1"/>
<contactref element="ANALOG" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="JP5" pad="2"/>
<contactref element="POWER" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="JP5" pad="1"/>
<contactref element="ANALOG" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="JP6" pad="1"/>
<contactref element="ANALOG" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="JP6" pad="2"/>
<contactref element="POWER" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="JP7" pad="1"/>
<contactref element="ANALOG" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="JP7" pad="2"/>
<contactref element="POWER" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="JP8" pad="1"/>
<contactref element="ANALOG" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="JP8" pad="2"/>
<contactref element="POWER" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="JP9" pad="1"/>
<contactref element="ANALOG" pad="23"/>
</signal>
<signal name="N$19">
<contactref element="JP9" pad="2"/>
<contactref element="POWER" pad="23"/>
</signal>
<signal name="N$20">
<contactref element="JP10" pad="1"/>
<contactref element="ANALOG" pad="22"/>
</signal>
<signal name="N$21">
<contactref element="JP10" pad="2"/>
<contactref element="POWER" pad="22"/>
</signal>
<signal name="N$22">
<contactref element="JP11" pad="1"/>
<contactref element="ANALOG" pad="21"/>
</signal>
<signal name="N$23">
<contactref element="JP11" pad="2"/>
<contactref element="POWER" pad="21"/>
</signal>
<signal name="GND">
<contactref element="JP11" pad="3"/>
<contactref element="JP10" pad="3"/>
<contactref element="JP9" pad="3"/>
<contactref element="JP8" pad="3"/>
<contactref element="JP7" pad="3"/>
<contactref element="JP6" pad="3"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="ANALOG" pad="12"/>
<contactref element="C3" pad="1"/>
<contactref element="POWER" pad="12"/>
<contactref element="C4" pad="2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="JP12" pad="3"/>
<contactref element="JP13" pad="3"/>
<contactref element="JP14" pad="3"/>
<contactref element="JP15" pad="3"/>
<contactref element="JP16" pad="3"/>
<contactref element="LOGIC-IN" pad="2"/>
<contactref element="LOGIC-OUT" pad="2"/>
</signal>
<signal name="ANALOG1">
<contactref element="S1" pad="1"/>
<contactref element="ANALOG-IN" pad="1"/>
<contactref element="ANALOG-OUT" pad="1"/>
</signal>
<signal name="ANALOG2">
<contactref element="S1" pad="2"/>
<contactref element="ANALOG-IN" pad="2"/>
<contactref element="ANALOG-OUT" pad="2"/>
</signal>
<signal name="ANALOG3">
<contactref element="S1" pad="3"/>
<contactref element="ANALOG-IN" pad="3"/>
<contactref element="ANALOG-OUT" pad="3"/>
</signal>
<signal name="ANALOG4">
<contactref element="S1" pad="4"/>
<contactref element="ANALOG-IN" pad="4"/>
<contactref element="ANALOG-OUT" pad="4"/>
</signal>
<signal name="ANALOG5">
<contactref element="S1" pad="5"/>
<contactref element="ANALOG-IN" pad="5"/>
<contactref element="ANALOG-OUT" pad="5"/>
</signal>
<signal name="ANALOG6">
<contactref element="S1" pad="6"/>
<contactref element="ANALOG-IN" pad="6"/>
<contactref element="ANALOG-OUT" pad="6"/>
</signal>
<signal name="COM">
<contactref element="ANALOG" pad="1"/>
<contactref element="S1" pad="11"/>
<contactref element="S1" pad="12"/>
<contactref element="S1" pad="13"/>
<contactref element="S1" pad="14"/>
<contactref element="S1" pad="15"/>
<contactref element="S1" pad="16"/>
</signal>
<signal name="ENABLE">
<contactref element="ANALOG" pad="15"/>
<contactref element="R2" pad="P$2"/>
<contactref element="POWER" pad="15"/>
</signal>
<signal name="VCC">
<contactref element="ANALOG" pad="24"/>
<contactref element="C3" pad="2"/>
<contactref element="POWER" pad="24"/>
<contactref element="C4" pad="1"/>
<contactref element="POWER" pad="1"/>
<contactref element="LOGIC-IN" pad="1"/>
<contactref element="LOGIC-OUT" pad="1"/>
</signal>
<signal name="S0">
<contactref element="ANALOG" pad="10"/>
<contactref element="POWER" pad="10"/>
<contactref element="LOGIC-IN" pad="3"/>
<contactref element="LOGIC-OUT" pad="3"/>
</signal>
<signal name="S2">
<contactref element="ANALOG" pad="14"/>
<contactref element="POWER" pad="14"/>
<contactref element="LOGIC-IN" pad="5"/>
<contactref element="LOGIC-OUT" pad="5"/>
</signal>
<signal name="S1">
<contactref element="ANALOG" pad="11"/>
<contactref element="POWER" pad="11"/>
<contactref element="LOGIC-IN" pad="4"/>
<contactref element="LOGIC-OUT" pad="4"/>
</signal>
<signal name="S3">
<contactref element="ANALOG" pad="13"/>
<contactref element="POWER" pad="13"/>
<contactref element="LOGIC-IN" pad="6"/>
<contactref element="LOGIC-OUT" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="JP16" pad="1"/>
<contactref element="ANALOG" pad="16"/>
</signal>
<signal name="N$24">
<contactref element="JP15" pad="1"/>
<contactref element="ANALOG" pad="17"/>
</signal>
<signal name="N$25">
<contactref element="JP14" pad="1"/>
<contactref element="ANALOG" pad="18"/>
</signal>
<signal name="N$26">
<contactref element="JP13" pad="1"/>
<contactref element="ANALOG" pad="19"/>
</signal>
<signal name="N$27">
<contactref element="JP12" pad="1"/>
<contactref element="ANALOG" pad="20"/>
</signal>
<signal name="N$28">
<contactref element="JP12" pad="2"/>
<contactref element="POWER" pad="20"/>
</signal>
<signal name="N$29">
<contactref element="JP13" pad="2"/>
<contactref element="POWER" pad="19"/>
</signal>
<signal name="N$30">
<contactref element="JP14" pad="2"/>
<contactref element="POWER" pad="18"/>
</signal>
<signal name="N$31">
<contactref element="JP15" pad="2"/>
<contactref element="POWER" pad="17"/>
</signal>
<signal name="N$32">
<contactref element="JP16" pad="2"/>
<contactref element="POWER" pad="16"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
