<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.15" y2="0" width="0" layer="20"/>
<wire x1="30.15" y1="0" x2="30.15" y2="20.31" width="0" layer="20"/>
<wire x1="30.15" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
<text>V+</text>
<text>L</text>
<text>T1</text>
<text>T2</text>
<text>S</text>
<text>s</text>
<text>+</text>
</plain>
<libraries>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL-08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
</package>
<package name="1X03_LOCK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="SparkFun-AnalogIC" package="DIL-08" value="NE555P">
<attribute name="OC_NEWARK" value="89K1486"/>
<attribute name="MPN" value="NE555N"/>
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="OC_FARNELL" value="1467742"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="15K"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value="27K"/>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value="220K"/>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALLEZ" value=""/>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value=""/>
<element name="LIMIT" library="SparkFun-Connectors" package="1X02_LOCK" value=""/>
<element name="TOGGLE1" library="SparkFun-Connectors" package="1X03_LOCK" value=""/>
<element name="TOGGLE2" library="SparkFun-Connectors" package="1X03_LOCK" value=""/>
<element name="VCC" library="SparkFun-Connectors" package="1X02_LOCK" value=""/>
<element name="SERVO" library="SparkFun-Connectors" package="1X03_LOCK" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="VCC" pad="2"/>
<contactref element="SERVO" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="R3" pad="P$1"/>
<contactref element="C1" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="M2">
<contactref element="IC1" pad="7"/>
<contactref element="R3" pad="P$2"/>
<contactref element="D1" pad="A"/>
<contactref element="TOGGLE2" pad="2"/>
</signal>
<signal name="M1">
<contactref element="LIMIT" pad="1"/>
<contactref element="TOGGLE1" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="SERVO" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="TOGGLE1" pad="3"/>
<contactref element="VCC" pad="1"/>
<contactref element="LIMIT" pad="2"/>
</signal>
<signal name="T21">
<contactref element="R1" pad="P$2"/>
<contactref element="TOGGLE2" pad="1"/>
</signal>
<signal name="T22">
<contactref element="R2" pad="P$2"/>
<contactref element="TOGGLE2" pad="3"/>
</signal>
<signal name="SS">
<contactref element="SERVO" pad="3"/>
<contactref element="IC1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
