<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="106.66" y2="0" width="0" layer="20"/>
<wire x1="106.66" y1="0" x2="106.66" y2="37.77" width="0" layer="20"/>
<wire x1="106.66" y1="37.77" x2="0" y2="37.77" width="0" layer="20"/>
<wire x1="0" y1="37.77" x2="0" y2="0" width="0" layer="20"/>
<text>wjaxxx@gmail.com</text>
<text>wjaxxx@gmail.com</text>
<text>GND CTRL</text>
<text>AC IN</text>
<text>AC OUT</text>
<text>GND 5V</text>
<text>cutout in milling layer</text>
<text>PSU CONTROL 4 3D PRINTER</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
</packages>
</library>
<library name="octoprintpsu">
<packages>
<package name="KEYES">
</package>
<package name="TPS-05">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="5VOUT" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="AC_IN" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="AC_OUT" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="CTRL" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="RELAY" library="octoprintpsu" package="KEYES" value="SS_RELAY"/>
<element name="5V" library="octoprintpsu" package="TPS-05" value="ACDV5V"/>
</elements>
<signals>
<signal name="FASE_IN">
<contactref element="5V" pad="AC1"/>
<contactref element="RELAY" pad="SS1_A"/>
<contactref element="AC_IN" pad="1"/>
</signal>
<signal name="NEUTRO">
<contactref element="5V" pad="AC2"/>
<contactref element="AC_OUT" pad="2"/>
<contactref element="AC_IN" pad="2"/>
</signal>
<signal name="5V">
<contactref element="5V" pad="VO+"/>
<contactref element="5VOUT" pad="2"/>
<contactref element="RELAY" pad="DC+"/>
</signal>
<signal name="GNDDC">
<contactref element="5V" pad="VO-"/>
<contactref element="5VOUT" pad="1"/>
<contactref element="RELAY" pad="DC-"/>
<contactref element="CTRL" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="CTRL" pad="2"/>
<contactref element="RELAY" pad="CTRL1"/>
<contactref element="RELAY" pad="CTRL2"/>
</signal>
<signal name="FASE_OUT">
<contactref element="RELAY" pad="SS1_B"/>
<contactref element="AC_OUT" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
