<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="24.13" y1="26.67" x2="34.29" y2="26.67" width="0" layer="20"/>
<wire x1="34.29" y1="26.67" x2="34.29" y2="16.51" width="0" layer="20"/>
<wire x1="34.29" y1="16.51" x2="24.13" y2="16.51" width="0" layer="20"/>
<wire x1="24.13" y1="16.51" x2="24.13" y2="26.67" width="0" layer="20"/>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>VCC</text>
<text>VEML6075</text>
<text>16Oct16</text>
<text>V1</text>
</plain>
<libraries>
<library name="VISHAY">
<packages>
<package name="VEML6075">
<description>Footprint for CWML6075 UV sensor</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK">
</package>
</packages>
</library>
<library name="KEMET">
<packages>
<package name="0805_B">
</package>
</packages>
</library>
<library name="ERIC">
<description>CDS Photoconductive Photocell.
PDV-P7002
Digikey part PDV-P7002-ND</description>
<packages>
<package name="FIDUCIAL_0.5MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="VISHAY" package="VEML6075" value="VEML6075"/>
<element name="JP1" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="KEMET" package="0805_B" value=""/>
<element name="U$2" library="ERIC" package="FIDUCIAL_0.5MM" value="FIDUCIAL"/>
<element name="U$3" library="ERIC" package="FIDUCIAL_0.5MM" value="FIDUCIAL"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP3" pad="4"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
