<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="-0.0254" y2="29.4386" width="0.2032" layer="20"/>
<wire x1="-0.0254" y1="29.4386" x2="63.5" y2="29.4386" width="0.2032" layer="20"/>
<wire x1="63.5" y1="29.4386" x2="63.5" y2="0" width="0.2032" layer="20"/>
<wire x1="63.5" y1="0" x2="0" y2="0" width="0.2032" layer="20"/>
<text>SCL</text>
<text>SDA</text>
<text>3V3</text>
<text>GND</text>
<text>DTR</text>
<text>TXO</text>
<text>RXI</text>
<text>3V3</text>
<text>GND</text>
<text>GND</text>
<text>0</text>
<text>4</text>
<text>13</text>
<text>12</text>
<text>XPD</text>
<text>ADC</text>
<text>EN</text>
<text>NC</text>
<text>I2C PU</text>
<text>FTDI
VCC</text>
<text>DTR</text>
<text>RST</text>
<text>!CS!</text>
<text>SO</text>
<text>!WP!</text>
<text>!HD!</text>
<text>CLK</text>
<text>SI</text>
<text>CHG</text>
<text>+</text>
<text>-</text>
<text>GND</text>
<text>VIN</text>
<text>0</text>
<text>4</text>
<text>13</text>
<text>12</text>
<text>XPD</text>
<text>ADC</text>
<text>EN</text>
<text>SCL</text>
<text>SDA</text>
<text>3V3</text>
<text>GND</text>
<text>DTR</text>
<text>TXO</text>
<text>PWR</text>
<text>5</text>
<text>5</text>
<text>VIN</text>
<text>5</text>
<text>RXI</text>
<text>1-cell
LiPo</text>
<text>1-cell
LiPo</text>
<text>MST Rocket Design Team</text>
<text>First Use: Genesis 2016</text>
<text>Jack Reiher</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
</package>
<package name="PAD-JUMPER-3-3OF3_NC_BY_TRACE_YES_SILK_FULL_BOX">
</package>
<package name="0603-RES">
</package>
<package name="PAD.03X.05">
</package>
<package name="PAD-JUMPER-2-NO_YES_SILK">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="PTH-JUMPER-NC_BOTTOM_NO_SILK">
</package>
<package name="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FIDUCIAL-1X2">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
<package name="0603">
</package>
</packages>
</library>
<library name="esp8266-development-board">
<packages>
<package name="QFN32">
</package>
<package name="UDFN8">
</package>
<package name="SO08">
<description>&lt;p&gt;8-pin SOIC package&lt;/p&gt;</description>
</package>
<package name="TRACE_ANTENNA_2.4GHZ_25.7MM">
</package>
<package name="FN-6">
</package>
</packages>
</library>
<library name="things">
<packages>
<package name="CRYSTAL-SMD-3.2X2.5">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FTDI_BASIC">
</package>
<package name="U.FL">
</package>
<package name="1X04">
</package>
<package name="USB-B-MICRO-SMD_V03">
</package>
<package name="JST-2-PTH">
</package>
<package name="1X10">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT563-2">
</package>
</packages>
</library>
<library name="Adafruit_LSM303DLHC">
<description>Generated from &lt;b&gt;Adafruit_LSM303DLHC.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
<package name="SOT23-WIDE">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FN-6">
</package>
</packages>
</library>
<library name="MPL3115A2_breakout">
<description>Generated from &lt;b&gt;MPL3115A2_breakout.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="LGA8">
<description>&lt;h4&gt;LGA8 Package&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt; 5.0x3.0x1.2mm&lt;/li&gt;
&lt;li&gt;8-pad&lt;/li&gt;&lt;br&gt;&lt;/ul&gt;
Used in MPL115A1</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="10uF">
<attribute name="PROD_ID" value="CAP-11015"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="U1" library="esp8266-development-board" package="QFN32" value="ESP8266"/>
<element name="Y1" library="things" package="CRYSTAL-SMD-3.2X2.5" value="26MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="XTAL-12454"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="FTDI_BASIC" value="FTDI_BASICPTH"/>
<element name="L1" library="SparkFun-Passives" package="0603" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="SparkFun-Passives" package="0603" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0603-CAP" value="5.6pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="U.FL" value="DNP">
<attribute name="PROD_ID" value="CONN-09193"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0603-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-00868"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X04" value="I2C"/>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0603-RES" value="1K">
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="esp8266-development-board" package="SO08" value="AT25SF041-SOIC8"/>
<element name="U5" library="esp8266-development-board" package="UDFN8" value="DNP"/>
<element name="R13" library="SparkFun-Resistors" package="0603-RES" value="2.2k">
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0603-RES" value="2.2k">
<attribute name="PROD_ID" value="RES-08272"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0603-CAP" value="2.2uF">
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="USB-B-MICRO-SMD_V03" value="USB">
<attribute name="PROD_ID" value="CONN-11752"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="4.7uF">
<attribute name="PROD_ID" value="CAP-08280"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SOD-323" value="BAT20J">
<attribute name="PROD_ID" value="DIO-11623"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="JST-2-PTH" value="LiPo">
<attribute name="SKU" value="PRT-09914"/>
</element>
<element name="SJ2" library="SparkFun-Passives" package="PAD-JUMPER-3-3OF3_NC_BY_TRACE_YES_SILK_FULL_BOX" value=""/>
<element name="R9" library="SparkFun-Resistors" package="0603" value="0">
<attribute name="PROD_ID" value="RES-08609"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Passives" package="0603-RES" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FID2" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FID1" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="YELLOW">
<attribute name="PROD_ID" value="DIO-09003"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="E1" library="esp8266-development-board" package="TRACE_ANTENNA_2.4GHZ_25.7MM" value="ANTENNATRACE"/>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="10pF">
<attribute name="PROD_ID" value="CAP-11812"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="10pF">
<attribute name="PROD_ID" value="CAP-11812"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="12k">
<attribute name="PROD_ID" value="RES-10327"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0603-RES" value="200">
<attribute name="PROD_ID" value="RES-08220"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="200">
<attribute name="PROD_ID" value="RES-08220"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="200">
<attribute name="PROD_ID" value="RES-08220"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP5" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP1" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP2" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP3" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="TP4" library="SparkFun-Passives" package="PAD.03X.05" value=""/>
<element name="U4" library="SparkFun-PowerIC" package="SOT23-5" value="AP2112K-3.3V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="VREG-12457"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0603-CAP" value="DNP">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="2.5A/30V">
<attribute name="PROD_ID" value="TRANS-11308"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0603-RES" value="200">
<attribute name="PROD_ID" value="RES-08220"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X10" value="M10&quot;"/>
<element name="R17" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="U6" library="SparkFun-Sensors" package="SOT563-2" value="DNP"/>
<element name="D5" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="SJ4" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value=""/>
<element name="SJ3" library="SparkFun-Passives" package="PTH-JUMPER-NC_BOTTOM_NO_SILK" value=""/>
<element name="U7" library="esp8266-development-board" package="FN-6" value="DNP"/>
<element name="C12" library="SparkFun-Capacitors" package="0603-CAP" value="DNP">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="GREEN">
<attribute name="PROD_ID" value="DIO-00821"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_TRACE_YES_SILK" value=""/>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="2.0k">
<attribute name="PROD_ID" value="RES-08296"/>
</element>
<element name="U9" library="Adafruit_LSM303DLHC" package="SOT23-5" value="RT9193"/>
<element name="C17" library="Adafruit_LSM303DLHC" package="_0805" value="10µF"/>
<element name="R12" library="Adafruit_LSM303DLHC" package="_0805" value="10K"/>
<element name="R14" library="Adafruit_LSM303DLHC" package="_0805" value="10K"/>
<element name="R18" library="Adafruit_LSM303DLHC" package="_0805" value="10K"/>
<element name="R19" library="Adafruit_LSM303DLHC" package="_0805" value="10K"/>
<element name="Q2" library="Adafruit_LSM303DLHC" package="SOT23-WIDE" value="BSS138"/>
<element name="Q3" library="Adafruit_LSM303DLHC" package="SOT23-WIDE" value="BSS138"/>
<element name="U10" library="SparkFun-DigitalIC" package="FN-6" value="TSL2561FN">
<attribute name="PROD_ID" value="IC-11791"/>
</element>
<element name="C13" library="Adafruit_LSM303DLHC" package="_0805" value="10µF"/>
<element name="U8" library="MPL3115A2_breakout" package="LGA8" value="MPL3115A2LGA8"/>
<element name="C14" library="MPL3115A2_breakout" package="0402-CAP" value="0.1uF"/>
<element name="R20" library="MPL3115A2_breakout" package="0402-RES" value="1K"/>
<element name="R21" library="MPL3115A2_breakout" package="0402-RES" value="1K"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="30"/>
<contactref element="U1" pad="29"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="17"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U3" pad="8"/>
<contactref element="C9" pad="1"/>
<contactref element="SJ2" pad="2"/>
<contactref element="U4" pad="5"/>
<contactref element="C10" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="SJ4" pad="2"/>
<contactref element="U7" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U5" pad="8"/>
<contactref element="U6" pad="5"/>
<contactref element="C12" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="U8" pad="1"/>
<contactref element="U8" pad="4"/>
<contactref element="R20" pad="2"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="EP"/>
<contactref element="Y1" pad="2"/>
<contactref element="Y1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP4" pad="GND"/>
<contactref element="L1" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="J1" pad="P$2"/>
<contactref element="J1" pad="P$1"/>
<contactref element="JP5" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="U5" pad="4"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="JP1" pad="GND1"/>
<contactref element="JP1" pad="SHIELD3"/>
<contactref element="JP1" pad="SHIELD1"/>
<contactref element="JP1" pad="SHIELD2"/>
<contactref element="U2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="E1" pad="GND"/>
<contactref element="E1" pad="GND2"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="U6" pad="4"/>
<contactref element="C11" pad="2"/>
<contactref element="U7" pad="3"/>
<contactref element="U6" pad="2"/>
<contactref element="U7" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U9" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="U10" pad="3"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U8" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="31"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="28"/>
<contactref element="Y1" pad="3"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="27"/>
<contactref element="Y1" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="CHIP_EN">
<contactref element="U1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="FTDI_VCC">
<contactref element="JP4" pad="VCC"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="U0RXI">
<contactref element="U1" pad="25"/>
<contactref element="JP4" pad="TXO"/>
</signal>
<signal name="U0TXO">
<contactref element="U1" pad="26"/>
<contactref element="JP4" pad="RXI"/>
</signal>
<signal name="RESET">
<contactref element="R6" pad="1"/>
<contactref element="U1" pad="32"/>
<contactref element="TP7" pad="P$1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="LNA">
<contactref element="U1" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C8" pad="2"/>
<contactref element="L2" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="DTR">
<contactref element="C6" pad="2"/>
<contactref element="JP4" pad="DTR"/>
<contactref element="SJ3" pad="1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="GPIO14/SCL">
<contactref element="JP5" pad="4"/>
<contactref element="U1" pad="9"/>
<contactref element="R13" pad="1"/>
<contactref element="U6" pad="1"/>
<contactref element="U7" pad="4"/>
<contactref element="U5" pad="6"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="ADC">
<contactref element="U1" pad="6"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="GPIO0">
<contactref element="U1" pad="15"/>
<contactref element="JP3" pad="4"/>
<contactref element="R15" pad="1"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="GPIO5">
<contactref element="U1" pad="24"/>
<contactref element="JP3" pad="3"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="GPIO4">
<contactref element="U1" pad="16"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="SD_!WP!">
<contactref element="U1" pad="19"/>
<contactref element="U3" pad="3"/>
<contactref element="TP1" pad="P$1"/>
</signal>
<signal name="SD_!HD!">
<contactref element="U1" pad="18"/>
<contactref element="U3" pad="7"/>
<contactref element="TP4" pad="P$1"/>
</signal>
<signal name="SD_SI">
<contactref element="U1" pad="23"/>
<contactref element="U3" pad="5"/>
<contactref element="TP2" pad="P$1"/>
</signal>
<signal name="SD_SO">
<contactref element="U1" pad="22"/>
<contactref element="U3" pad="2"/>
<contactref element="TP5" pad="P$1"/>
</signal>
<signal name="SD_CLK">
<contactref element="U3" pad="6"/>
<contactref element="R5" pad="1"/>
<contactref element="TP3" pad="P$1"/>
</signal>
<signal name="SD_CS0">
<contactref element="U1" pad="20"/>
<contactref element="U3" pad="1"/>
<contactref element="TP6" pad="P$1"/>
</signal>
<signal name="GPIO16">
<contactref element="U1" pad="8"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="GPIO15">
<contactref element="U1" pad="13"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="GPIO13">
<contactref element="U1" pad="12"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="GPIO12">
<contactref element="U1" pad="10"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="GPIO2/SDA">
<contactref element="U1" pad="14"/>
<contactref element="R11" pad="1"/>
<contactref element="JP5" pad="3"/>
<contactref element="U6" pad="6"/>
<contactref element="U7" pad="6"/>
<contactref element="U5" pad="5"/>
<contactref element="U8" pad="7"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="C7" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="U4" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="C17" pad="1"/>
<contactref element="U9" pad="1"/>
<contactref element="U9" pad="3"/>
<contactref element="R19" pad="2"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="VUSB">
<contactref element="JP1" pad="VBUS1"/>
<contactref element="U2" pad="4"/>
<contactref element="D3" pad="A"/>
<contactref element="R7" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="D1" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="U2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U2" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="U2" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="21"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R11" pad="2"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R13" pad="2"/>
<contactref element="SJ2" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="R8" pad="1"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="ANT">
<contactref element="R10" pad="1"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="TRACE_ANT">
<contactref element="R9" pad="1"/>
<contactref element="E1" pad="ANT"/>
</signal>
<signal name="N$4">
<contactref element="R16" pad="1"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="D5" pad="C"/>
<contactref element="SJ3" pad="2"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U4" pad="3"/>
</signal>
<signal name="VDD">
<contactref element="U9" pad="5"/>
<contactref element="R12" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="U10" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R12" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="U10" pad="6"/>
</signal>
<signal name="N$27">
<contactref element="R14" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="U10" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="R18" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="R19" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="U8" pad="2"/>
<contactref element="C14" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
