<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="2.5" y1="15" x2="0" y2="15" width="0" layer="20"/>
<wire x1="0" y1="15" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="55" x2="0" y2="39.5" width="0" layer="20"/>
<wire x1="2.5" y1="39.5" x2="2.5" y2="15" width="0" layer="20"/>
<wire x1="0" y1="0" x2="39" y2="0" width="0" layer="20"/>
<wire x1="2.5" y1="39.5" x2="0" y2="39.5" width="0" layer="20"/>
<wire x1="39" y1="55" x2="39" y2="39.5" width="0" layer="20"/>
<wire x1="39" y1="15" x2="36.5" y2="15" width="0" layer="20"/>
<wire x1="39" y1="39.5" x2="36.5" y2="39.5" width="0" layer="20"/>
<wire x1="39" y1="15" x2="39" y2="0" width="0" layer="20"/>
<wire x1="36.5" y1="39.5" x2="36.5" y2="15" width="0" layer="20"/>
<wire x1="39" y1="55" x2="0" y2="55" width="0" layer="20"/>
<hole x="35.687" y="52.324" drill="2.8"/>
<hole x="2.54" y="52.324" drill="2.8"/>
<hole x="36.195" y="1.905" drill="2"/>
<hole x="36.195" y="4.445" drill="2"/>
<hole x="36.195" y="6.985" drill="2"/>
<hole x="36.195" y="9.525" drill="2"/>
<hole x="36.195" y="12.065" drill="2"/>
<text>MLP4DSM</text>
<text>DX4e/DX5e</text>
<hole x="2.54" y="3.3782" drill="3.2"/>
<hole x="24.13" y="3.3782" drill="3.2"/>
<hole x="9.525" y="21.717" drill="2.8"/>
<text>SIG</text>
<text>+6V</text>
<text>BAT</text>
<text>GND</text>
<text>ANT</text>
<hole x="9.525" y="52.705" drill="2.8"/>
<hole x="28.448" y="52.705" drill="2.8"/>
<text>JR-DSMX v3.2</text>
<text>v3 Changes:
Added power LED
Converted to drills
Changed parts to use easier to solder annular rings.</text>
<text>v3.1 Changes:
Added SMD 1206 resistors in line with the through-hole variants.
Added bypass for R2</text>
<text>Bypass R2</text>
<text>LED1</text>
<text>R2</text>
<text>D1</text>
<text>R1</text>
<text>C2</text>
<text>C1</text>
<text>R3</text>
<text>JP1</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>S</text>
<text>S</text>
<text>S</text>
<text>-</text>
<text>I</text>
<text>I</text>
<text>B</text>
<text>B</text>
<text>B</text>
<text>S</text>
<text>v3.2 Changes:
Smashed part names into text fields (easier panelization)
Switched to vector font
Restricting ground pour under Vout tab from vreg</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05_LONGPADS">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
</packages>
</library>
<library name="00_PERSONAL">
<packages>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="E5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 6 mm</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="headers(2mm)">
<packages>
<package name="1X3">
</package>
<package name="2X6">
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220L1">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SOT-223">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="1N4001">
<attribute name="VALUE"/>
</element>
<element name="R2" library="00_PERSONAL" package="0207/7" value="1k">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X05_LONGPADS" value="JR Module"/>
<element name="R1" library="00_PERSONAL" package="0207/7" value="4.7k">
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="E5-6" value="10uF">
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="E5-6" value="1uF">
<attribute name="VALUE"/>
</element>
<element name="DX4E" library="headers(2mm)" package="2X6" value="2X6"/>
<element name="MLP4DSM" library="headers(2mm)" package="1X3" value="1X3"/>
<element name="R3" library="00_PERSONAL" package="0207/7" value="68">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="v-reg" package="TO220L1" value="LD1117V33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="R4" library="SparkFun-Passives" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="1206" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
<element name="VREG1" library="dp_devices" package="SOT-223" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="DATA">
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="1"/>
<contactref element="MLP4DSM" pad="3"/>
<contactref element="DX4E" pad="11"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="C"/>
<contactref element="R2" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="SIGNAL">
<contactref element="JP1" pad="5"/>
<contactref element="R2" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="+6V">
<contactref element="JP1" pad="4"/>
</signal>
<signal name="BAT">
<contactref element="JP1" pad="3"/>
<contactref element="C1" pad="+"/>
<contactref element="IC1" pad="3"/>
<contactref element="VREG1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="C2" pad="-"/>
<contactref element="C1" pad="-"/>
<contactref element="MLP4DSM" pad="2"/>
<contactref element="DX4E" pad="1"/>
<contactref element="LED1" pad="K"/>
<contactref element="IC1" pad="1"/>
<contactref element="VREG1" pad="1"/>
</signal>
<signal name="ANT">
<contactref element="JP1" pad="1"/>
</signal>
<signal name="3.3">
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="+"/>
<contactref element="MLP4DSM" pad="1"/>
<contactref element="DX4E" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="VREG1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="A"/>
<contactref element="R6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
