<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<text>GND</text>
<text>+3V</text>
<text>Lenka</text>
<text>Lenka</text>
<circle x="17" y="18.75" radius="16.68831875" width="0.01" layer="20"/>
<hole x="2" y="18.75" drill="1.4"/>
<hole x="32" y="18.75" drill="1.4"/>
<hole x="17" y="3.75" drill="1.4"/>
<hole x="28.25" y="8.75" drill="1.4"/>
<hole x="5.75" y="8.75" drill="1.4"/>
<hole x="10.5" y="5" drill="1.4"/>
<hole x="23.25" y="5" drill="1.4"/>
<hole x="3" y="13.25" drill="1.4"/>
<hole x="31" y="13.25" drill="1.4"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
<package name="0603-CAP">
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="SparkFunNew">
<packages>
<package name="BATTCOM_20MM_PTH_SMT">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun" package="0603-RES" value="47R"/>
<element name="R2" library="SparkFun" package="0603-RES" value="47R"/>
<element name="R3" library="SparkFun" package="0603-RES" value="47R"/>
<element name="R4" library="SparkFun" package="0603-RES" value="47R"/>
<element name="R5" library="SparkFun" package="0603-RES" value="47R"/>
<element name="LED1" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED9" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED10" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED11" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED12" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED13" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED14" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED15" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED16" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED17" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED18" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED19" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED20" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="AtTiny85">
<attribute name="PROD_ID" value="IC-09092"/>
</element>
<element name="C4" library="SparkFun" package="0603-CAP" value="0.1uf"/>
<element name="RESET" library="SparkFun" package="TACTILE-SWITCH-1101NE" value="">
<attribute name="VALUE"/>
</element>
<element name="BAT1" library="SparkFunNew" package="BATTCOM_20MM_PTH_SMT" value="LIR2032"/>
<element name="U$7" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0"/>
<element name="U$1" library="SparkFun" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
</elements>
<signals>
<signal name="N$6">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED20" pad="C"/>
<contactref element="LED16" pad="C"/>
<contactref element="LED12" pad="C"/>
<contactref element="LED8" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="1"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED6" pad="A"/>
<contactref element="LED7" pad="A"/>
<contactref element="LED8" pad="A"/>
<contactref element="LED19" pad="C"/>
<contactref element="LED15" pad="C"/>
<contactref element="LED11" pad="C"/>
<contactref element="LED4" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="1"/>
<contactref element="LED9" pad="A"/>
<contactref element="LED10" pad="A"/>
<contactref element="LED11" pad="A"/>
<contactref element="LED12" pad="A"/>
<contactref element="LED18" pad="C"/>
<contactref element="LED14" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED7" pad="C"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="1"/>
<contactref element="LED13" pad="A"/>
<contactref element="LED14" pad="A"/>
<contactref element="LED15" pad="A"/>
<contactref element="LED16" pad="A"/>
<contactref element="LED17" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED10" pad="C"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="1"/>
<contactref element="LED17" pad="A"/>
<contactref element="LED18" pad="A"/>
<contactref element="LED19" pad="A"/>
<contactref element="LED20" pad="A"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED9" pad="C"/>
<contactref element="LED13" pad="C"/>
</signal>
<signal name="USBP">
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="USBM">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="RES">
<contactref element="U1" pad="1"/>
<contactref element="RESET" pad="P$2"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="PIN1">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="C4" pad="2"/>
<contactref element="RESET" pad="P$1"/>
<contactref element="BAT1" pad="P$1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="C4" pad="1"/>
<contactref element="BAT1" pad="P$2"/>
<contactref element="U$1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
