<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>+12</text>
<text>B</text>
<text>G</text>
<text>R</text>
<text>0x263A</text>
<text>bike blinkenthing
haldean.org/bike</text>
<wire x1="5.08" y1="19.05" x2="5.08" y2="72.39" width="0.4064" layer="20"/>
<wire x1="5.08" y1="72.39" x2="6.35" y2="73.66" width="0.4064" layer="20"/>
<wire x1="6.35" y1="73.66" x2="17.78" y2="73.66" width="0.4064" layer="20"/>
<wire x1="17.78" y1="73.66" x2="20.32" y2="76.2" width="0.4064" layer="20"/>
<wire x1="20.32" y1="76.2" x2="53.34" y2="76.2" width="0.4064" layer="20"/>
<wire x1="53.34" y1="76.2" x2="55.88" y2="73.66" width="0.4064" layer="20"/>
<wire x1="55.88" y1="73.66" x2="58.42" y2="73.66" width="0.4064" layer="20"/>
<wire x1="58.42" y1="73.66" x2="58.42" y2="36.83" width="0.4064" layer="20"/>
<wire x1="58.42" y1="36.83" x2="50.8" y2="29.21" width="0.4064" layer="20"/>
<wire x1="50.8" y1="29.21" x2="50.8" y2="20.32" width="0.4064" layer="20"/>
<wire x1="50.8" y1="20.32" x2="46.99" y2="16.51" width="0.4064" layer="20"/>
<wire x1="46.99" y1="16.51" x2="7.62" y2="16.51" width="0.4064" layer="20"/>
<wire x1="7.62" y1="16.51" x2="5.08" y2="19.05" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUEMILANOVE_SHIELD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="COMPUTER-PERIPHERAL-POWER-RA">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RED" library="transistor" package="TO220" value="TIP31A"/>
<element name="GREEN" library="transistor" package="TO220" value="TIP31A"/>
<element name="BLUE" library="transistor" package="TO220" value="TIP31A"/>
<element name="SHIELD" library="SparkFun-Boards" package="DUEMILANOVE_SHIELD" value="ARDUINO_SHIELDLABEL"/>
<element name="J1" library="SparkFun-Connectors" package="COMPUTER-PERIPHERAL-POWER-RA" value="COMPUTER-PERIPHERAL-POWERRA"/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="100"/>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="100"/>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.3EZ" value="100"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="GREEN" pad="1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="BLUE" pad="1"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="BLUE" pad="3"/>
<contactref element="GREEN" pad="3"/>
<contactref element="RED" pad="3"/>
<contactref element="SHIELD" pad="GND@2"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="GND"/>
<contactref element="BLUE" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="NC"/>
<contactref element="GREEN" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="12V"/>
<contactref element="RED" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="SHIELD" pad="VIN"/>
<contactref element="J1" pad="5V"/>
</signal>
<signal name="N$9">
<contactref element="SHIELD" pad="D5"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="SHIELD" pad="D6"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="SHIELD" pad="D3"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="R1" pad="P$2"/>
<contactref element="RED" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
