<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="32.385" y1="48.26" x2="0" y2="48.26" width="0.1524" layer="20"/>
<wire x1="0" y1="0" x2="32.385" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="48.26" x2="0" y2="0" width="0.1524" layer="20"/>
<wire x1="33.02" y1="48.26" x2="33.02" y2="0" width="0.1524" layer="20"/>
<wire x1="33.02" y1="0" x2="32.385" y2="0" width="0.1524" layer="20"/>
<wire x1="32.385" y1="48.26" x2="33.02" y2="48.26" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-S-SILK-FEMALE">
<description>&lt;h3&gt;USB Type 'A' Female Connector - SMT Silk Outline&lt;/h3&gt;
Shield pins may be grounded.
&lt;br&gt; tDocu shows plug end. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=” https://www.sparkfun.com/datasheets/Prototyping/Connectors/USBFemaleTypeA.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="USB-A-S-SILK-FEMALE" value="USB_A_SMT_FEMALE">
<attribute name="PROD_ID" value="CONN-09520"/>
<attribute name="SF_ID" value="PRT-09011"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="USB-A-S-SILK-FEMALE" value="USB_A_SMT_FEMALE">
<attribute name="PROD_ID" value="CONN-09520"/>
<attribute name="SF_ID" value="PRT-09011"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="WHITE">
<attribute name="PROD_ID" value="DIO-09004"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="WHITE">
<attribute name="PROD_ID" value="DIO-09004"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED-0603" value="WHITE">
<attribute name="PROD_ID" value="DIO-09004"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-0603" value="WHITE">
<attribute name="PROD_ID" value="DIO-09004"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-0603" value="WHITE">
<attribute name="PROD_ID" value="DIO-09004"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="PROD_ID" value="RES-07856"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X03" value="455-1750-1-ND">
<attribute name="PROD_ID" value="XXX-00000"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J2" pad="GND"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="D+"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J2" pad="D-"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="VBUS"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="GND"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="D+"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="D-"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="VBUS"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$10">
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$11">
<contactref element="R3" pad="2"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$12">
<contactref element="R4" pad="2"/>
<contactref element="D4" pad="C"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="2"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="GROUND">
<contactref element="R1" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="LED0">
<contactref element="D1" pad="A"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="LED1">
<contactref element="D2" pad="A"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="LED2">
<contactref element="D3" pad="A"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="LED3">
<contactref element="D4" pad="A"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="LED4">
<contactref element="D5" pad="A"/>
<contactref element="J5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
