<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="15.24" y1="29.21" x2="41.58" y2="29.21" width="0" layer="20"/>
<wire x1="41.58" y1="29.21" x2="41.58" y2="54.6" width="0" layer="20"/>
<wire x1="41.58" y1="54.6" x2="15.24" y2="54.6" width="0" layer="20"/>
<wire x1="15.24" y1="54.6" x2="15.24" y2="29.21" width="0" layer="20"/>
<text>u\banjemin</text>
</plain>
<libraries>
<library name="switches">
<packages>
<package name="3PDT.LUGS">
<description>&lt;b&gt; Latching Footswitch, Solder Lugs&lt;/b&gt;
&lt;br&gt;&lt;a href="http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt/"&gt;http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt/&lt;/a&gt;
&lt;p&gt;
&lt;b&gt;Momentary Footswitch, Solder Lugs&lt;/b&gt;
&lt;br&gt;&lt;a href="http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt-momentary/"&gt;http://smallbear-electronics.mybigcommerce.com/cic-blue-3pdt-momentary/&lt;/a&gt;</description>
</package>
<package name="3PDT.WIRE">
<description>Wire to switch</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SW_1" library="switches" package="3PDT.LUGS" value=""/>
<element name="SW_2" library="switches" package="3PDT.WIRE" value=""/>
</elements>
<signals>
<signal name="N$3">
<contactref element="SW_1" pad="A2"/>
<contactref element="SW_2" pad="A2"/>
</signal>
<signal name="N$6">
<contactref element="SW_1" pad="C2"/>
<contactref element="SW_2" pad="C2"/>
</signal>
<signal name="N$9">
<contactref element="SW_1" pad="B2"/>
<contactref element="SW_2" pad="B2"/>
</signal>
<signal name="N$1">
<contactref element="SW_1" pad="A1"/>
<contactref element="SW_2" pad="A1"/>
</signal>
<signal name="N$2">
<contactref element="SW_1" pad="A3"/>
<contactref element="SW_2" pad="A3"/>
</signal>
<signal name="N$8">
<contactref element="SW_1" pad="B3"/>
<contactref element="SW_2" pad="B3"/>
</signal>
<signal name="N$4">
<contactref element="SW_2" pad="C1"/>
<contactref element="SW_1" pad="C1"/>
</signal>
<signal name="N$7">
<contactref element="SW_1" pad="C3"/>
<contactref element="SW_2" pad="C3"/>
</signal>
<signal name="N$5">
<contactref element="SW_1" pad="B1"/>
<contactref element="SW_2" pad="B1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
