<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="11.5" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2" y1="0" x2="44" y2="0" width="0" layer="20"/>
<wire x1="44" y1="0" x2="46" y2="2" width="0" layer="20" curve="90"/>
<wire x1="46" y1="2" x2="46" y2="11.5" width="0" layer="20"/>
<wire x1="46" y1="36.5" x2="46" y2="44" width="0" layer="20"/>
<wire x1="46" y1="44" x2="44" y2="46" width="0" layer="20" curve="90"/>
<wire x1="31.21" y1="36.83" x2="38.64" y2="36.83" width="0" layer="20"/>
<wire x1="38.64" y1="36.83" x2="40.64" y2="38.83" width="0" layer="20" curve="90"/>
<wire x1="40.64" y1="38.83" x2="40.64" y2="44" width="0" layer="20"/>
<wire x1="40.64" y1="44" x2="42.64" y2="46" width="0" layer="20" curve="-90"/>
<wire x1="42.64" y1="46" x2="44" y2="46" width="0" layer="20"/>
<wire x1="2" y1="46" x2="27.21" y2="46" width="0" layer="20"/>
<wire x1="27.21" y1="46" x2="29.21" y2="44" width="0" layer="20" curve="-90"/>
<wire x1="29.21" y1="44" x2="29.21" y2="38.83" width="0" layer="20"/>
<wire x1="29.21" y1="38.83" x2="31.21" y2="36.83" width="0" layer="20" curve="90"/>
<wire x1="2" y1="46" x2="0" y2="44" width="0" layer="20" curve="90"/>
<wire x1="0" y1="44" x2="0" y2="36.5" width="0" layer="20"/>
<hole x="13.84" y="36.13" drill="4"/>
<wire x1="0" y1="11.5" x2="-5" y2="11.5" width="0" layer="20"/>
<wire x1="-5" y1="11.5" x2="-7" y2="13.5" width="0" layer="20" curve="-90"/>
<wire x1="-7" y1="13.5" x2="-7" y2="34.5" width="0" layer="20"/>
<wire x1="-7" y1="34.5" x2="-5" y2="36.5" width="0" layer="20" curve="-90"/>
<wire x1="-5" y1="36.5" x2="0" y2="36.5" width="0" layer="20"/>
<wire x1="46" y1="36.5" x2="51" y2="36.5" width="0" layer="20"/>
<wire x1="51" y1="36.5" x2="53" y2="34.5" width="0" layer="20" curve="-90"/>
<wire x1="53" y1="34.5" x2="53" y2="13.5" width="0" layer="20"/>
<wire x1="53" y1="13.5" x2="51" y2="11.5" width="0" layer="20" curve="-90"/>
<wire x1="51" y1="11.5" x2="46" y2="11.5" width="0" layer="20"/>
<hole x="-3.5" y="32.5" drill="3"/>
<hole x="-3.5" y="15" drill="3"/>
<hole x="49.5" y="32.5" drill="3"/>
<hole x="49.5" y="15" drill="3"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RLB0912">
</package>
</packages>
</library>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO-08">
<description>&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt; Plastic Small Outline Package&lt;p&gt;

Source: http://focus.ti.com/lit/ds/symlink/sn65als176.pdf</description>
</package>
</packages>
</library>
<library name="Kontakr-custom">
<packages>
<package name="MICROPIRANI_905">
</package>
</packages>
</library>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LTI-SASF54GT">
<description>&lt;b&gt;SMA vertical PCB thrue hole jack&lt;/b&gt;&lt;p&gt;
Source: Lighthorse Technologies, inc. SASF54GT.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="10uF">
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="10uF">
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="L1" library="SparkFun-Passives" package="RLB0912" value=""/>
<element name="L2" library="SparkFun-Passives" package="RLB0912" value=""/>
<element name="SN65HVD96" library="texas" package="SO-08" value="SN65176D">
<attribute name="OC_FARNELL" value="9589970"/>
<attribute name="MPN" value="SN65176BD"/>
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="OC_NEWARK" value="08F5891"/>
</element>
<element name="U$1" library="Kontakr-custom" package="MICROPIRANI_905" value="MICROPIRANI905"/>
<element name="X1" library="con-coax" package="LTI-SASF54GT" value="LTI-SASF54GT">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="SN65HVD96" pad="5"/>
<contactref element="U$1" pad="P$9"/>
<contactref element="U$1" pad="P$10"/>
<contactref element="U$1" pad="P$15"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="SN65HVD96" pad="8"/>
<contactref element="L2" pad="2"/>
<contactref element="U$1" pad="P$17"/>
<contactref element="U$1" pad="P$18"/>
</signal>
<signal name="N$2">
<contactref element="C3" pad="2"/>
<contactref element="L2" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="C4" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="C3" pad="1"/>
<contactref element="SN65HVD96" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="C4" pad="1"/>
<contactref element="SN65HVD96" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="SN65HVD96" pad="1"/>
<contactref element="U$1" pad="P$20"/>
</signal>
<signal name="N$8">
<contactref element="SN65HVD96" pad="4"/>
<contactref element="U$1" pad="P$21"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$16"/>
<contactref element="SN65HVD96" pad="2"/>
<contactref element="SN65HVD96" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
