<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<hole x="9.525" y="13.335" drill="3.302"/>
<hole x="50.8" y="13.335" drill="3.302"/>
<wire x1="10.795" y1="2.54" x2="10.795" y2="24.13" width="0" layer="20" curve="-180"/>
<wire x1="61.8744" y1="15.6718" x2="61.8744" y2="10.9474" width="0" layer="20"/>
<text>LED 1</text>
<text>LED 2</text>
<text>LED 3</text>
<text>LED 4</text>
<text>LED 5</text>
<text>BLK</text>
<text>RED</text>
<text>IN</text>
<text>OUT</text>
<text>ADDRESS DIRECTION</text>
<text>ADDRESS DIRECTION</text>
<text>PARALLAX ELEV-8</text>
<text>V3 RUNNING LIGHTS</text>
<wire x1="10.795" y1="24.13" x2="54.5846" y2="24.13" width="0" layer="20"/>
<wire x1="10.795" y1="2.54" x2="54.5084" y2="2.54" width="0" layer="20"/>
<text>RED</text>
<text>BLK</text>
<wire x1="58.293" y1="20.574" x2="60.833" y2="16.256" width="0" layer="20"/>
<wire x1="60.706" y1="10.2362" x2="58.166" y2="5.9182" width="0" layer="20"/>
<wire x1="54.5846" y1="24.13" x2="58.42" y2="21.8186" width="0" layer="20"/>
<wire x1="58.42" y1="21.8186" x2="58.928" y2="20.955" width="0" layer="20"/>
<wire x1="58.928" y1="20.955" x2="58.293" y2="20.574" width="0" layer="20"/>
<wire x1="61.8744" y1="15.6718" x2="61.341" y2="16.5862" width="0" layer="20"/>
<wire x1="61.341" y1="16.5862" x2="60.833" y2="16.256" width="0" layer="20"/>
<wire x1="61.8744" y1="10.9474" x2="61.2648" y2="9.906" width="0" layer="20"/>
<wire x1="61.2648" y1="9.906" x2="60.706" y2="10.2362" width="0" layer="20"/>
<wire x1="54.5084" y1="2.54" x2="58.2676" y2="4.6228" width="0" layer="20"/>
<wire x1="58.2676" y1="4.6228" x2="58.7502" y2="5.5626" width="0" layer="20"/>
<wire x1="58.7502" y1="5.5626" x2="58.166" y2="5.9182" width="0" layer="20"/>
<text>Close on 1, 2, &amp; 3</text>
<text>Close on 2, 3, &amp; 4</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="WS2812B">
<description>&lt;b&gt;Intelligent control LED with integrated light source&lt;/b&gt;&lt;p&gt;
WS2812B&lt;br&gt;
source: http://www.world-semi.com/uploads/soft/130904/1_1500205981.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-LED" package="WS2812B" value="">
<attribute name="PROD_ID" value="DIO-12503"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK" value="JUMPER-PAD-2-NC_BY_PASTE"/>
<element name="SJ2" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK" value="JUMPER-PAD-2-NC_BY_PASTE"/>
<element name="U$1" library="SparkFun-PowerIC" package="SOT223" value="V_REG_MIC2920"/>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="PROD_ID" value="CAP-08402"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="D1" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="VSS">
<contactref element="D2" pad="3"/>
<contactref element="D1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="D3" pad="3"/>
<contactref element="C3" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="4"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="2"/>
<contactref element="D3" pad="4"/>
</signal>
<signal name="OUT3">
<contactref element="D3" pad="2"/>
</signal>
<signal name="OUT4">
</signal>
<signal name="N$1">
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="JP2" pad="3"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="2"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="SJ2" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
</signals>
</board>
</drawing>
</eagle>
